CLOVIS UNIFIED SCHOOL DISTRICT BID 2978 CLOVIS WEST HIGH SCHOOL WEST GYM FLOOR RECONSTRUCTION

Addendum No. 1 February 22, 2024

Notice to Bidders:
This addendum forms a part of the Bid /Contract Documents for the above referenced project and shall be incorporated integrally. Bidders are required to acknowledge receipt of this addendum on the sheet included with the bid package. Failure to acknowledge receipt of this addendum may subject the bidder to disqualification. Each proposer shall make necessary adjustments and submit their proposal with full knowledge of all modifications, clarifications, and supplemental data included therein. Where provisions of the following supplemental data differ from those of the original Bid / Contract Documents, this Addendum shall govern.

You are hereby notified of the following changes, clarifications or modifications to the original Bid /Contract Documents:

Clarification – The Engineer of Record has agreed to consider the use of the attached flooring systems. Product Substitutions shall be submitted to the Engineer of Record and the District after award of contract.

If you have any questions, please feel free to contact my office at 559-327-9477.

Lacey Wolf Buyer II
LaceyWolf@CUSD.com

PowerLoc™ FLOATING SYSTEM

PowerLoc is a hybrid of our ever popular ScissorLoc and PowerSleeper systems. The combination of these systems delivers a dimensionally stable floor with excellent ventilation capabilities. Our optional PowerVent™ system adds a feature to detect moisture and start drying the system with mechanical airflow. PowerLoc’s uniform performance makes it a good selection for new and retrofit sports floor applications.

www.AACERflooring.com • 877.582.1181

Jan2024
PowerLoc

PowerLoc is a hybrid of our ever popular ScissorLoc and PowerSleeper systems. The floor is a good selection for new and retrofit sports floor applications.

1

2

3

4

1.Infinity MFMA Maple	3.Pre-Engineered Plywood 2.1/2" x 5-1/2" (12mm x 140mm)       Sleeper
Dimensional Pine	4.ECO Resilient Pad

WALL BASE

Green Status and LEED Contributors

Resilience

Slab Depression

Optional PowerLoc Systems

Optional Protection System

• FSC® Certified Maple - MR

• FSC® Certified Subfloor Components - MR

• Environmental Quality - EQ • Regional Materials - MR

1/2" (12mm) ECO Pad *Other pad options available.

• 25/32" (20mm) flooring –2 5/8" (67mm)

Anchored PowerSleeper™ Anchored PowerSleeper™ SE Anchored PowerLoc Anchored PowerLoc LP

PowerVent™ Airflow System

1.

2. 3.

4. 5. 6.

7.

2 5/8"(67mm)

3" x 4" (76mm x 101mm) Vent Cove Base

1-1/2" (38mm) Min. Expansion Space

1/2" x 5-1/2" (12mm x 140mm) Pine Subfloor

1/2" (12mm) ECO Resilient Pad Engineered Plywood Sleeper
25/32" (20mm) MFMA Maple Flooring

Vapor Retarder

Subfloor Construction

System Type

Testing Laboratory Partners

Engineered Sleeper and Subfloor

Floating

THRESHOLD

2 5/8"(67mm)

1. 1/4" (6mm) Aluminum Threshold

2. 1-1/2" (38mm) Min. Expansion Space

3. 1/2" x 5-1/2" (12mm x 140mm) Pine Sub loor

4. Engineered Plywood Sleeper with Solid Blocking Attached

5. 25/32" (20mm) MFMA Maple Flooring

6. 1/2" (12mm) ECO Resilient Pad

7. Vapor Retarder

EQUIPMENT

1. 2.

3.

4.

Floor Plate

1-1/2" (38mm) Min. Expansion Space at all Inserts & Electrical Penetrations

Concrete Floor Penetration

Solid Blocking at Insert

It is the policy of Infinity Wood Floors to continuously improve its line of products. Therefore, Infinity Wood Floors reserves the right to change, modify or discontinue systems, specifications and accessories of all products at any time without notice or obligation to purchaser.

	
Description: POWERLOC
	
Resilience: 1/2" (12mm) ECO pads
	
Drawn By: RR
	Date: 1/1/23
	
Revisions
	
ID
	Description
	By
	Date

				

Warranty and Disclaimer

Aacer Sport Flooring, an Infinity Wood Floors Company, Crandon,Wisconsin, hereby warrants the materials it has supplied to be free from manufacturing defects for a period of one (1) year.THIS WARRANTY IS IN LIEU OF AND EXCLUDES ALL OTHER WARRANTIES EXPRESSED OR IMPLIED INCLUDING ANY IMPLIED WARRANTIES OF MERCHANTABILITY OR FITNESS FOR A PARTICULAR PURPOSE.

This warranty is limited to the materials manufactured and supplied by Infinity/Aacer Flooring.THIS WARRANTY EXCLUDES ANY CONSEQUENTIALOR INCIDENTAL DAMAGES and in the event of breach, Infinity/Aacer Flooring’s sole liability and your exclusive remedies will be limited to repair or replacement of materials and components supplied by Infinity/Aacer Flooring and proven to be defective by the manufacturing process.

This warranty does not cover damage (in whole or in part) caused by fire, winds, floods, chemicals, other abuse, failure of owners, contractors, or suppliers to adhere to specifications, neglect,or precautions to provide adequate ventilation at times of high humidity, excessive dryness, as well as excessive moisture from humidity, spillage, migration through the substrate, wall, or any other source. This warranty also excludes any damage to materials due to ordinary wear and tear,faulty construction of the building, separation of concrete substrate, settlement of walls or of water-based materials used on the floor.

During the warranty period, the floor shall not be recoated without the approval of the flooring contractor.

The jobsite documentation forms by the flooring contractor shall become a part of the warranty and both the owner and flooring contractor shall retain record of said forms as a permanent reference for any abrogation.

Flooring contractor warrants the installation of the floor systems to be free from defects in materials and workmanship for a period of one (1) year.

TriPower™ Pad ACCESSORY

The next generation in a sports performance pad, Aacer’s TriPower™ Pads provide certified performance systems with increased load handling. The TriPower™ Pad’s
unique, wide stance gives greater response, consistency and lower vibration than other pad designs.

www.AACERflooring.com • 877.582.1181

Jan2024
b.Vibration attenuation

TriPower™ Pad offers superior shock absorption and vibration dampening. The unique blend of EPDM ensures stability and longevity required by high performance floors.

1

2
3

1.Structural Webs - Cross-Linked	2.Stage II Heavy-Duty Load a.Greater load carrying ability           Distribution
3.3-point Surface Contact Shock c.Increased uniformity and	Pads - Athletic Resilience
consistent response
	
Composition

Hardness

ASTM Durometer

Triangular Footprint

ASTM D412 Tensile PSI

ASTM D412 Elongation

Loading

Performance Information

U.S. Patent #
	
EPDM Rubber / Recyclable
		
			Shore A
		
			Black, 1/2" (12mm), 50D Red, 3/4" (19mm), 70D Black, 3/4" (19mm), 60D Blue, 3/4" (19mm), 50D
3 Point Primary Surface Contact
1 Point Secondary Load Contact
		
			1810

648
		
			Excellent

Aacer systems meet and exceed all 3rd party industry testing standards.
• ASTM 2137 low temperature brittleness ∙ 3 min @ -40 - pass
• ASTM D395 compression set
∙ 22 hours @ 70c set % -20

#5,988,915

It is the policy of Infinity Wood Floors to continuously improve its line of products. Therefore, Infinity Wood Floors reserves the right to change, modify or discontinue systems, specifications and accessories of all products at any time without notice or obligation to purchaser.

DETAIL DRAWINGS

AACER PAD OPTION

TriPower™ Black 1/2" (12mm) 50D

ECO
1/4" (6mm), 1/2" (12mm), 3/4" (19mm)

S

Tri

Power™ Red 3/4" (19mm)
70D

AacerCush 3/8" (10mm)

TriPower™ Black           TriPower™ Blue 3/4" (19mm)                      3/4" (19mm) 60D                                   50D

Open Cell Foam	Performance Foam
1/2" (12mm),	1/4" (6mm), 1/2" (12mm), 3/4" (19mm)                          3/4" (19mm)

TriPower™ Pad

Alliance Panel

Wall Base Detail

Threshold Detail (Optional Accessory)

Equipment Detail (Optional Accessory)

PERMAFLEX™ SPECIALTY HARDWOOD SYSTEM

connorsports.com

(Optional)
Anchor Clip

PERMAFLEX™ SPECIALTY HARDWOOD SYSTEM

This unique subfloor design encapsulates Rezill™ pads between an upper flex sleeper and a lower base sleeper to extend the system’s resilient life and
accommodate heavy non-athletic loads through use of manufactured 16-gauge steel-encased sleeper subfloor supports. A truss support option allows for profile height adjustment ideal for retrofit installations.

Wall Base Detail	Threshold Detail ( Optional Accessory )	Equipment Detail ( Optional Accessory )

3” x 4” (76 mm x 102 mm) Vented Rubber Base	25/32” x 2-1/4” (20 mm x 57 mm) Laytite Maple

1-1/2” (38 mm) Expansion Space

15/32” (12 mm) APA Sheathing

Aluminum Threshold

1-1/2” (38 mm) Expansion Space

PermaFlex Channel	Floor Plate	Plywood Subfloor Rezill Pad

Upper “Flex” Sleeper	PermaFlex Channel	Equipment Sleeve

Rezill Pad

PermaFlex Channel

Lower “Perma” Base Sleeper

Vapor Barrier Rezill Pad

3” (76 mm)

Concrete Slab

Manufacturing:	Recycled Contribution:

Includes components with recycled content

Testing Laboratory:

United States Sports Surfacing Laboratory

Certified Testing:

ISS Scientific Body Membership

Green Status:

Managed Forests, Certification Available

Customer Service: 800.283.9522 | info@connorsports.com | connorsports.com/products

Where Champions Play™

a company of ©2022 Connor® is a registered trademark of Connor Sports. TLT028 Rev. 4