ADDENDUM NO. 3 4/27/2022

PROJECT:

ENGINEER:

Pavement Maintenance at Various Sites

Blair, Church & Flynn Attention:	Jenn Felix
Tanairy Barrera

OWNER:

BID NO: BCF PROJECT NO.

Clovis Unified School District

2890 221-0288

It will be the responsibility of the General Contractor to submit the information contained in this addendum to all its subcontractors and suppliers. Acknowledge receipt of this Addendum in the space provided on the Bid Form. Failure to do so may subject Bidder to disqualification. The following additions, deletions, and revisions to the Drawings and Project Manual are hereby made and do become a part of these Contract Documents.

TABLE OF CONTENTS

CHANGES TO BIDDING AND CONTRACT REQUIREMENTS AD3-BR1: Project Duration
CHANGES TO ALL DRAWINGS

AD3-1: Asphalt Pavement Structural Sections

ATTACHMENTS

EXHIBIT A – ASPHALT PAVEMENT SECTION DETAIL

Blair, Church & Flynn Consulting Engineers 451 Clovis Avenue, Suite 200
Clovis, CA 93612

(559) 326-1400 FAX (559) 326-1500

Page 1 of 2

ADDENDUM NO. 3 4/27/2022

CHANGES TO BIDDING AND CONTRACT REQUIREMENTS AD3-BR1: Project Duration

1.	The project duration has been revised from 40 calendar days to 60 calendar days.

CHANGES TO ALL DRAWINGS AD3-1: Asphalt Pavement Structural Sections

1.	 Revise the asphalt pavement structural section detail as shown in the attachment EXHIBIT A – ASPHALT PAVEMENT SECTION DETAIL. Assume the following pavement structural sections for the following sites:
·	Buchanan High School: 3” AC over 10.5” Class 2 AB over 12” compacted subgrade

·	Clovis High School Playcourts: 2” AC over 4” Class 2 AB over 12” compacted subgrade ·	Clovis High Access Road: 3” AC over 10.5” Class 2 AB over 12” compacted subgrade
·	Clovis West High School: 3” AC over 6” Class 2 AB over 12” compacted subgrade

·	Community Day School Parking Lot: 3” AC over 4” Class 2 AB over 12” compacted subgrade ·	Community Day Playcourt: 2” AC over 4” Class 2 AB over 12” compacted subgrade
·	Professional Development Center: 3” AC over 4” Class 2 AB over 12” compacted subgrade ·	CART: 3” AC over 4” Class 2 AB over 12” compacted subgrade
·	Jefferson Elementary: 2” AC over 6” Class 2 AB over 12” compacted subgrade

·	Mickey Cox Elementary: 2” AC over 6” Class 2 AB over 12” compacted subgrade ·	Pinedale Elementary: 3” AC over 4” Class 2 AB over 12” compacted subgrade

Blair, Church & Flynn Consulting Engineers 451 Clovis Avenue, Suite 200
Clovis, CA 93612

(559) 326-1400 FAX (559) 326-1500

Page 2 of 2

7

ASPHALTIC CONCRETE, TYPE B WITH 1/2" MAX. AGGREGATE. SEE ADDENDUM 3 FOR THICKNESS.

AGGREGATE BASE, CLASS 2. SEE ADDENDUM 3 FOR THICKNESS.

SOIL STERILANT

12" COMPACTED SOIL
	
		CLOVIS UNIFIED SCHOOL DISTRICT
	
		2022 PAVEMENT MAINTENANCE ADDENDUM 03
EXHIBIT A - ASPHALT PAVEMENT SECTION DETAIL
	DATE:4/27/22 ISSUED BY: JF