ADDENDUM NO. 1

PROJECT:

PROJECT LOCATION:

BID DATE:

DSA APP. NO.:

FILE. NO.:

Date: May 24, 2021

BUD RANK ELEMENTARY SCHOOL Lockdown System
CLOVIS UNIFIED SCHOOL DISTRICT

3650 Power Avenue Clovis, CA 93619

June 07, 2021, 11:00 am

02-119185

10-27

John H. Smith Project Architect

This Addendum forms a part of the Contract Documents. It modifies the original Project Manual and Drawings, as well as any Addendum previously issued, as noted below. Bidders are required to acknowledge receipt of this Addendum in the space provided in the proposal form.	Failure to acknowledge receipt of each addendum may subject bidder to disqualification.

GENERAL

Item No. 1-01

Item No. 1-02

BID WALK SIGN IN SHEET See attached.

CLOVIS U.S.D. NEEDS/WANTS OF SOFTWARE SYSTEM(S)

Needs Automation

1. An app on every employee’s phone, with options of emergency type

(disgruntled parent, active shooter on campus, injured student)

2. Ability to assign permissions to every app – give us the flexibility to not allow every employee to initiate lockdown (Windows groups?)
3. Automate the calling of 911.
4. Automate the notification of essential District staff (both on-site and off-site) 5. Automate lockdown announcement (if lockdown is initiated)
6. Automate lockdown siren (if lockdown is initiated)
7. Automate the locking of doors (if lockdown is initiated)
8. Automate the disabling of access control (if lockdown is initiated)
9. Automate the takeover of every employees’ computer (if lockdown is initiated)

7790 N. PALM || FRESNO, CA 93711 || T 559.448.8400	SIM-PBK.COM

Page 1 of 3

10. Ability to provide classroom status and two-way communication. 11. Ability to use for drills.

Wants
1. Ability to notify parents/community (not automated) 2. Ability to look at roster based on daily attendance.

Item No. 1-03

Item No. 1-04

Item No. 1-05

Item No. 1-06

BID RFI’s
RFI’s to be emailed to Luis Olvera at SIM-PBK – lolvera@sim-pbk.com.
RFI’s and clarification to be submitted to SIM-PBK prior to May 27, 2021 – 5:00 pm.

SITE PROJECT WORK HOURS
Monday thru Friday days. District will have limited staff availability on Friday June 7, 2021 thru July 30, 2021.

UPCCA CALENDAR YEAR 2021
Registration is required on this project. Application information with website is referenced in original bid documents.

PUBLIC WORKS
This is a PUBLIC WORKS project which requires, but not limited to, the following:
Bid Bond or Cashier’s Check (due at time of sealed bid submittal) Prevailing Wage as mandated by State of California.
Valid & Active State of California Contractors License Megan’s Law Fingerprint Requirements
Project Payment & Performance Bonds (after award) Insurance Limits as noted in original bid documents. Current and Valid Workers Compensation Insurance
Contractor Registration with Department of Industrial Relations (DIR) District DIR project registration with State of California
Contractor upload of project Certified Payroll with DIR

DRAWINGS

Item No. 1-07

Item No. 1-08

Item No. 1-09

Item No. 1-10

SHEET A1.1 ADMINISTRATION FLOOR PLAN Revised door schedule. See attached.

SHEET A2.1 MULTI-PURPOSE FLOOR PLAN Revised door schedule. See attached.

SHEET A3.1 CLASSROOM FLOOR PLAN Revised door schedule. See attached.

SHEET A4.1 CLASSROOM FLOOR PLAN Revised door schedule. See attached.

Page 2 of 3

Item No. 1-11

Item No. 1-12

Item No. 1-13

SHEET A5.1 CLASSROOM FLOOR PLAN Revised door schedule. See attached.

SHEET A6.1 CLASSROOM FLOOR PLAN Revised door schedule. See attached.

SHEET A7.1 CLASSROOM FLOOR PLAN Revised door schedule. See attached.

SPECIFICATIONS

Item No. 1-14	 REPLACE SECTION 08 71 00 HARDWARE See attached for revised hardware.

END OF ADDENDUM

7790 N. PALM || FRESNO, CA 93711 || T 559.448.8400	SIM-PBK.COM

Page 3 of 3

ITEM NO. 1-01

A1.1
15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

L	L

K	K

J		J 1        N

5A 1 A

I

1

WALL S

8	DOOR SCHEDULE X
D1.1	DOOR	FRAME	WALL	CEILING

I

W. x H.

DOOR No.
DOOR TYPE
DOOR SIZE
EXISTING CONST.
EXISTING CONST.
EXISTING FINISH
EXISTING FINISH
REMARKS
HARDWARE
(SEE SPECS)
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING WALL CONST.
BUILDING 1 : ADMINISTRATION

H

1     P COUNTER

6	6 1	D1.1                                                                                                                                                                                                             D1.1

P     1 COUNTER

1

1	SI      (E) 3'-0" x 7'-0"

2	SI      (E) 3'-0" x 7'-0"

3	SI      (E) 3'-0" x 7'-0"

SF	FF	SF	FF

HM	P	HM	FF

SF	FF	SF	FF

WC	WIN      WIN

WC	STU	TK

WC	WIN	WIN

STU      GYP      01	2	H

STU      GYP      02	2

STU      GYP      03	2

3	1	4	SI      (E) 3'-0" x 7'-0"	HM	SGP	HM	SGP	WC	STU	TK	STU      GYP      01	2

G	8

D1.1	1

4	A
A	A

2	1

8

D1.1

A

A	5	1

5	SI      (E) 3'-0" x 7'-0"

5A      SI      (E) 3'-0" x 7'-0"

6
D1.1	ABBREVIATIONS

SF	FF	SF

HM	SGP	HM

FF	WC	WIN	WIN

SGP	WC	STU	TK

STU	TB	01	2	G

STU      GYP      05	2

FF      FACTORY FINISH	WC      WOOD CONSTRUCTION FT      FACTORY                                                      SI	SINGLE DOOR

F	 P	1	HM     HOLLOW METAL DESK                                                                                                                                                               PT      PAINT

DL      DOUBLE DOOR	F

FRP     FIBER RESISTANT PANEL

GYP     GYP. BOARD FINISH

PH      PANIC HARDWARE

STU     STUCCO FINISH
TB.     T-BAR CEILING SYSTEM

SF      STOREFRONT	TK      TACKBOARD FINISH

P	1
DESK	S      1

E	WALL

SGP     SEMI-GLOSS PAINT	WIN     WINDOW SYSTEM

KEYNOTES	E

N	NOTIFIER	S .
P	PANIC BUTTON	A

LOW VOLTAGE PATHWAY

STROBE LIGHT. SEE DETAIL 10/D1.1

CARD READER / ACCESS DEVICE

FLOOR PLAN D	BUILDING 1
DSA # 02-106638

N	KEYNOTES X

1. DEMO FINISHES TO ACCESS WORK. REPAIR ALL FINISHES BACK TO ORIGINAL FINISH/CONDITION.	D 2. SEE SPECIFICATIONS FOR MORE INFORMATION.

KEY PLAN

C

EXTERIOR DOOR # 1	EXTERIOR DOOR # 2	EXTERIOR DOOR # 3	EXTERIOR DOOR # 4	EXTERIOR DOOR #5	L

C 15885

9-30-21 RENEWAL DATE

B		B PROJECT NAME
BUD RANK ELEMENTARY SCHOOL 3650 Powers Ave, Clovis Ca. 93619

No. DATE .	-
.	.

.	.

DESCRIPTION -
.

.

No. DATE .	.
.	.

.	.

DESCRIPTION	REVISIONS .
.

.

N

A

INTERIOR DOOR # 1	INTERIOR DOOR # 2	INTERIOR DOOR # 3	INTERIOR DOOR # 4	INTERIOR DOOR #5

SHEET NAME
BUILDING 1 - ADMINISTRATION/LIBRARY FLOOR PLAN BUILDING 1
.
JOHN SMITH     PROJECT ARCHITECT	S21005	PROJECT NUMBER	SHEET NUMBER       A LUIS OLVERA	DRAWN BY                   N.T.S.                              SCALE
.
CHECKED BY		DATE MAY 26, 2021

15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

ITEM NO. 1-07

A2.1
.
WC
WC

1

TY

DOOR

N
		
	1

		

15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

L	L

EXISTING CONST.
EXISTING CONST.
EXISTING FINISH
EXISTING FINISH
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING WALL CONST.
K	DOOR SCHEDULE X	K DOOR               FRAME                      WALL                    CEILING

8	1

6
D1.1	9

6

D1.1

10 1

8

PE
D1.1

DOOR No.
DOOR SIZE
REMARKS
HARDWARE
(SEE SPECS)
J	A	A	A	W. x H.	J

BUILDING 1 : ADMINISTRATION

I

A

11 1

8

D1.1

6	DL     (E) 3'-0" x 7'-0"

7	DL     (E) 3'-0" x 7'-0"

8	DL     (E) 3'-0" x 7'-0"

9	DL     (E) 3'-0" x 7'-0"

SF	FF	SF	FF

SF	FF	SF	FF

SF	FF	SF	FF

SF	FF	SF	FF

WC	STU	TK

WC      STU	TK

WC      STU	TK

WC      STU	TK

STU	TB	04	2

STU	TB	04	2

STU	TB	04	2	I

STU	TB	04	2

10	SI      (E) 3'-0" x 7'-0"	HM	PT	HM	PT	WC      STU      GYP      STU	TB	05	2

6	1	7	11

H	D1.1		12 A

DL     (E) 3'-0" x 7'-0"

DL     (E) 3'-0" x 7'-0"

HM	PT	HM	PT	WC

HM	PT	HM	PT	WC

GYP
STU	TK      STU	TB	06

STU      GYP	STU     OPEN 07

2

2	H

13      DL     (E) 3'-0" x 7'-0"	HM	PT	HM	PT	WC      STU      GYP	STU	TB	06	2

6	1	6 D1.1

14	SI      (E) 3'-0" x 7'-0"

15	SI      (E) 3'-0" x 7'-0"

SF	FF	SF	FF

SF	FF	SF	FF

STU	GYP
WIN	WIN      WIN     STU

STU	GYP
WIN	WIN      WIN     STU

TB	01	2

TB	01	2

G	A	16	SI      (E) 3'-0" x 7'-0"	HM	PT	HM	PT	WC      STU      GYP	STU	TB	05	2	G

ABBREVIATIONS

16 1

8
D1.1	FF      FACTORY FINISH

FT      FACTORY

WC      WOOD CONSTRUCTION

SI	SINGLE DOOR

F	A	HM     HOLLOW METAL PT      PAINT

DL      DOUBLE DOOR	F

FRP     FIBER RESISTANT PANEL

GYP     GYP. BOARD FINISH

PH      PANIC HARDWARE

STU     STUCCO FINISH
TB.     T-BAR CEILING SYSTEM

SF      STOREFRONT                                                TK      TACKBOARD FINISH SGP     SEMI-GLOSS PAINT                                    WIN     WINDOW SYSTEM

E	LEGEND	E

N	NOTIFIER .

P	PUSH BUTTON

S	STROBE LIGHT. SEE DETAIL 10/D1.1

A	CARD READER / ACCESS DEVICE

D

8	1	15 A D1.1

6 D1.1
C

8 12	1	D1.1

A

8	1	13 D1.1

A

1	14 A

LOW VOLTAGE PATHWAY

KEYNOTES X

1. DEMO FINISHES TO ACCESS WORK. REPAIR ALL FINISHES BACK TO ORIGINAL FINISH/CONDITION.	D 2. SES SPECIFICATIONS FOR MORE INFORMATION.

KEY PLAN

L

C 15885

9-30-21 RENEWAL DATE

B		B PROJECT NAME
BUD RANK ELEMENTARY SCHOOL 3650 Powers Ave, Clovis Ca. 93619

No. DATE .	-
.	.

.	.

DESCRIPTION -
.

.

No. DATE .	.
.	.

.	.

DESCRIPTION	REVISIONS .
.

.

A	N

BUILDING 2 DSA # 02-106638

SHEET NAME
BUILDING 2 - MULTI-PURPOSE FLOOR PLAN BUILDING 2
.
JOHN SMITH     PROJECT ARCHITECT	S21005	PROJECT NUMBER	SHEET NUMBER       A LUIS OLVERA	DRAWN BY                   N.T.S.                              SCALE
CHECKED BY		DATE MAY 26, 2021

15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

ITEM NO. 1-08

A3.1
.

	N

	1

15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

L	L

K	K

J	J

DOOR SCHEDULE X

A	DOOR	FRAME	WALL	CEILING

EXISTING EXT. FINISH
EXISTING EXT. FINISH
EXISTING WALL CONST.
18A

EXISTING CONST.
EXISTING CONST.
EXISTING FINISH
EXISTING FINISH
EXISTING INT. FINISH
EXISTING INT. FINISH
I	A	I

6

D1.1	1

17	18 1

A

6 D1.1

W. x H.

DOOR No.
DOOR TYPE
DOOR SIZE
REMARKS
HARDWARE
(SEE SP     S)
BUILDING 1 : ADMINISTRATION

H	17	DL     (E) 3'-0" x 7'-0"

18      DL     (E) 3'-0" x 7'-0"

SF	FF	SF	FF	WC

SF	FF	SF	FF	WC

WIN	GYP STU     TK        STU          TB

WIN	GYP STU     TK        STU          TB

04	2	H

04	2

18A      SI      (E) 3'-0" x 7'-0"	HM	PT	HM	PT	WC	STU      GYP      GYP     GYP      05	2

G	G

ABBREVIATIONS S	WALL S      1

FF      FACTORY FINISH	WC      WOOD CONSTRUCTION FT      FACTORY                                                      SI	SINGLE DOOR

F	HM     HOLLOW METAL PT      PAINT

DL      DOUBLE DOOR	F

FRP     FIBER RESISTANT PANEL

GYP     GYP. BOARD FINISH

PH      PANIC HARDWARE

STU     STUCCO FINISH
TB.     T-BAR CEILING SYSTEM

SF      STOREFRONT                                                TK      TACKBOARD FINISH SGP     SEMI-GLOSS PAINT                                    WIN     WINDOW SYSTEM

E	LEGEND	E

BUILDING 3 DSA # 02-106638

N	NOTIFIER

P	PUSH BUTTON

LOW VOLTAGE PATHWAY

S	STROBE LIGHT. SEE DETAIL 10/D1.1

A	CARD READER / ACCESS DEVICE

KEYNOTES X

D	1. DEMO FINISHES TO ACCESS WORK. REPAIR ALL FINISHES BACK TO ORIGINAL FINISH/CONDITION.	D 2. SEE SPECIFICATIONS FOR MORE INFORMATION.

KEY PLAN

C

SEE BUILDING 5 PICTURES ARE SIMILAR.	L
C 15885

9-30-21 RENEWAL DATE

B		B PROJECT NAME
BUD RANK ELEMENTARY SCHOOL 3650 Powers Ave, Clovis Ca. 93619

No. DATE .	-
.	.

.	.

DESCRIPTION -
.

.

No. DATE .	.
.	.

.	.

DESCRIPTION	REVISIONS .
.

.

N

A

SHEET NAME
BUILDING 3 - CLASSROOMS FLOOR PLAN BUILDING 3
.
JOHN SMITH     PROJECT ARCHITECT	S21005	PROJECT NUMBER	SHEET NUMBER       A LUIS OLVERA	DRAWN BY                   N.T.S.                              SCALE
CHECKED BY		DATE MAY 26, 2021

15	14	13	12	11	10	9	8	7	6	5	4	3	 2	1 ITEM NO. 1-09

A4.1
.

	N
		
		1

15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

L	L

K	K

J	J

WALL	DOOR SCHEDULE S
A
1	20A

I	A

X

DOOR	FRAME	WALL	CEILING

I

6

D1.1	1

19	20 1

6

D1.1

DOOR No.
DOOR TYPE
DOOR SIZE
EXISTING CONST.
EXISTING CONST.
EXISTING FINISH
EXISTING FINISH
REMARKS
HARDWARE
(SEE SPECS)
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING WALL CONST.
A
W. x H.

BUILDING 1 : ADMINISTRATION

H	19      DL     (E) 3'-0" x 7'-0"

20      DL     (E) 3'-0" x 7'-0"

SF	FF	SF	FF

SF	FF	SF	FF

WIN	GYP

WC	 STU      TK	STU	TB WIN                               GYP

WC	STU      TK	STU	TB

04	2	H

04	2

20A     SI      (E) 3'-0" x 7'-0"	HM	PT	HM	PT	WC	STU      GYP      GYP     GYP      05	2

G	G

ABBREVIATIONS

FF      FACTORY FINISH	WC      WOOD CONSTRUCTION FT      FACTORY                                                      SI	SINGLE DOOR
F	HM     HOLLOW METAL	DL      DOUBLE DOOR	F PT      PAINT                                                            FRP     FIBER RESISTANT PANEL

GYP     GYP. BOARD FINISH

PH      PANIC HARDWARE

STU     STUCCO FINISH
TB.     T-BAR CEILING SYSTEM

SF      STOREFRONT                                                TK      TACKBOARD FINISH SGP     SEMI-GLOSS PAINT                                    WIN     WINDOW SYSTEM

E	LEGEND	E

BUILDING 4 DSA # 02-106638

N	NOTIFIER	S .                                                                 A
P	PUSH BUTTON

LOW VOLTAGE PATHWAY

STROBE LIGHT. SEE DETAIL 10/D1.1

CARD READER / ACCESS DEVICE

KEYNOTES X

D	1. DEMO FINISHES TO ACCESS WORK. REPAIR ALL FINISHES BACK TO ORIGINAL FINISH/CONDITION.	D 2. SEE SPECIFICATIONS FOR MORE INFORMATION.

KEY PLAN

C

L SEE BUILDING 5 PICTURES ARE SIMILAR.	C 15885
9-30-21 RENEWAL DATE

B		B PROJECT NAME
BUD RANK ELEMENTARY SCHOOL 3650 Powers Ave, Clovis Ca. 93619

No. DATE .	-
.	.

.	.

DESCRIPTION -
.

.

No. DATE .	.
.	.

.	.

DESCRIPTION	REVISIONS .
.

.

A	N

SHEET NAME
BUILDING 4 - CLASSROOMS FLOOR PLAN BUILDING 4
.
JOHN SMITH     PROJECT ARCHITECT	S21005	PROJECT NUMBER	SHEET NUMBER       A LUIS OLVERA	DRAWN BY                   N.T.S.                              SCALE
CHECKED BY		DATE MAY 26, 2021

15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

ITEM NO. 1-10

A5.1
.

	N

	1

	

A

15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

L	L

K	K

WALL S

1

J	J

8

D1.1	1

I

23

A

22A 1

DOOR SCHEDULE X

DOOR	FRAME	WALL	CEILING 8
D1.1

I

6

D1.1	1

21	22 1

DOOR No.
DOOR TYPE
DOOR SIZE
EXISTING CONST.
EXISTING CONST.
EXISTING FINISH
EXISTING FINISH
REMARKS
HARDWARE
(SEE SPECS)
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING WALL CONST.
6
A	D1.1	W. x H.

8

D1.1	1

24	BUILDING 1 : ADMINISTRATION

H	21	DL     (E) 3'-0" x 7'-0"

22      DL     (E) 3'-0" x 7'-0"

SF	FF	SF	FF

SF	FF	SF	FF

WIN	GYP

WC	 STU      TK	STU	TB WIN                               GYP

WC	STU      TK	STU	TB

04	2	H

04	2

22A     SI      (E) 3'-0" x 7'-0"	HM	PT	HM	PT	WC	STU      GYP      GYP     GYP      05	2

23      SI      (E) 3'-0" x 7'-0"

24      SI      (E) 3'-0" x 7'-0"

G

HM	PT	HM	PT	WC

HM	PT	HM	PT	WC

GYP STU	FRP
GYP

STU	FRP

STU      GYP      02	2

STU      GYP      02	2

G

ABBREVIATIONS

FF      FACTORY FINISH	WC      WOOD CONSTRUCTION FT      FACTORY                                                      SI	SINGLE DOOR
F	HM     HOLLOW METAL	DL      DOUBLE DOOR	F PT      PAINT                                                            FRP     FIBER RESISTANT PANEL

BUILDING 5 DSA # 02-106638

E

GYP     GYP. BOARD FINISH PH      PANIC HARDWARE

SF      STOREFRONT

SGP     SEMI-GLOSS PAINT

LEGEND

STU     STUCCO FINISH
TB.     T-BAR CEILING SYSTEM

TK      TACKBOARD FINISH WIN     WINDOW SYSTEM

E

N	NOTIFIER

P	PUSH BUTTON

LOW VOLTAGE PATHWAY

S	STROBE LIGHT. SEE DETAIL 10/D1.1

A	CARD READER / ACCESS DEVICE

KEYNOTES X

D	1. DEMO FINISHES TO ACCESS WORK. REPAIR ALL FINISHES BACK TO ORIGINAL FINISH/CONDITION.	D 2. SEE SPECIFICATIONS FOR MORE INFORMATION.

KEY PLAN

C

L

C 15885

9-30-21 RENEWAL DATE

B		B PROJECT NAME
BUD RANK ELEMENTARY SCHOOL 3650 Powers Ave, Clovis Ca. 93619

No. DATE .	-
.	.

.	.

DESCRIPTION -
.

.

No. DATE .	.
.	.

.	.

DESCRIPTION	REVISIONS .
.

.

INTERIOR DOOR #22 A	DOOR 21 SIMILAR

EXTERIOR DOOR #22
DOOR 21 SIMILAR	N

SHEET NAME
BUILDING 5 - CLASSROOMS FLOOR PLAN BUILDING 5
.
JOHN SMITH     PROJECT ARCHITECT	S21005	PROJECT NUMBER	SHEET NUMBER       A LUIS OLVERA	DRAWN BY                   N.T.S.                              SCALE
CHECKED BY		DATE MAY 26, 2021

15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

ITEM NO. 1-11

A6.1
.

1
			
	N

8A 1

OR No.

OR TYPE
	DOOR SIZE

EXISTING CONST.

	

OO

OO

DO

DO

15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

L	L

K	K

27 1

A

J

8 D1.1

A

28 1

8

D1.1	WALL S      1

J

DOOR SCHEDULE X

DOOR	FRAME	WALL	CEILING

EXISTING CONST.
EXISTING FINISH
EXISTING FINISH
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING WALL CONST.
I	2	I

REMARKS
HARDWARE
(SEE SPECS)
A

A

H	25 1

A

8

D1.1

26 1

W. x H.

BUILDING 1 : ADMINISTRATION

8	25      SI      (E) 3'-0" x 7'-0"	SF	FF	SF	FF D1.1

26      SI      (E) 3'-0" x 7'-0"	SF	FF	SF	FF

27	SI	(E) 3'-0" x 7'-0"	SF	FF	SF	FF

28      SI	(E) 3'-0" x 7'-0"	SF	FF	SF	FF

WIN WC	STU
WIN WC	STU
WIN WC	STU

WIN WC	STU

GYP TK	STU	TB

GYP TK	STU	TB
GYP TK	STU	TB
GYP TK	STU	TB

01	2	H

01	2

01	2

01	2

28A     SI      (E) 3'-0" x 7'-0"	HM	PT	HM	PT	WC	STU      GYP      GYP     GYP      05	2

G	G

ABBREVIATIONS

FF      FACTORY FINISH	WC      WOOD CONSTRUCTION FT      FACTORY                                                      SI	SINGLE DOOR

F	BUILDING 6 DSA # 02-106638

HM     HOLLOW METAL

PT      PAINT

GYP     GYP. BOARD FINISH

PH      PANIC HARDWARE

DL      DOUBLE DOOR	F FRP     FIBER RESISTANT PANEL

STU     STUCCO FINISH
TB.     T-BAR CEILING SYSTEM

SF      STOREFRONT                                                TK      TACKBOARD FINISH SGP     SEMI-GLOSS PAINT                                    WIN     WINDOW SYSTEM

E	LEGEND	E

N	NOTIFIER	S
.
P	PUSH BUTTON	A

LOW VOLTAGE PATHWAY

STROBE LIGHT. SEE DETAIL 10/D1.1

CARD READER / ACCESS DEVICE

KEYNOTES X

D
EXTERIOR DOOR #25 DOOR 26, 27, 28 SIMILAR

EXTERIOR DOOR #25 DOOR 26, 27, 28 SIMILAR

1. DEMO FINISHES TO ACCESS WORK. REPAIR ALL FINISHES BACK TO ORIGINAL FINISH/CONDITION.	D 2. SEE SPECIFICATIONS FOR MORE INFORMATION.

KEY PLAN

C

L

C 15885

9-30-21 RENEWAL DATE

B		B PROJECT NAME
BUD RANK ELEMENTARY SCHOOL 3650 Powers Ave, Clovis Ca. 93619

No. DATE .	-
.	.

.	.

DESCRIPTION -
.

.

No. DATE .	.
.	.

.	.

DESCRIPTION	REVISIONS .
.

.

A	     INTERIOR DOOR #25 DOOR 26, 27, 28 SIMILAR

INTERIOR DOOR #25	N DOOR 26, 27, 28 SIMILAR

SHEET NAME
BUILDING 6 - CLASSROOMS FLOOR PLAN BUILDING 6
.
JOHN SMITH     PROJECT ARCHITECT	S21005	PROJECT NUMBER	SHEET NUMBER       A LUIS OLVERA	DRAWN BY                   N.T.S.                              SCALE
CHECKED BY		DATE MAY 26, 2021

15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

ITEM NO. 1-12

N
N

1

15	14	13	12	11	10	9	8	7	6	5	4	3	2	1

CC1 CC2
L		L 30 32
8

D1.1	A

K	K

DOOR SCHEDULE X

DOOR No.
DOOR TYPE
DOOR SIZE
EXISTING CONST.
EXISTING CONST.
EXISTING FINISH
EXISTING FINISH
REMARKS
HARDWARE
(SEE SPECS)
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING WALL CONST.
J	DOOR	FRAME	WALL	CEILING	J

A I

38 37 36 35 34 33 1

A

8	31 29 1 D1.1                                                                                  CC2 CC1

8

D1.1

W. x H.

BUILDING 1 : ADMINISTRATION	I

29      SI      (E) 3'-0" x 7'-0"	HM	PT	HM	PT	WC	STU      GYP      GYP     GYP      09	2

H

G

P32 P31 P30 P29 P28 P27

FLOOR PLAN
PORTABLE P27, P28, P29 P30, P31, P32

DSA # 02-113647 DSA # 02-114230 DSA # 02-116698

FLOOR PLAN PORTABLE CC1 & CC2
DSA # 02-112901 DSA # 02-110110

30      SI      (E) 3'-0" x 7'-0"

31	SI      (E) 3'-0" x 7'-0"

32      SI      (E) 3'-0" x 7'-0"

33      SI      (E) 3'-0" x 7'-0"

34      SI      (E) 3'-0" x 7'-0"

35      SI      (E) 3'-0" x 7'-0"

36      SI      (E) 3'-0" x 7'-0"

37	SI      (E) 3'-0" x 7'-0"

38      SI      (E) 3'-0" x 7'-0"

HM	PT	HM	PT

HM	PT	HM	PT

HM	PT	HM	PT

HM	PT	HM	PT

HM	PT	HM	PT

HM	PT	HM	PT

HM	PT	HM	PT

HM	PT	HM	PT

HM	PT	HM	PT

WC	STU      GYP

WC	STU      GYP

WC	STU      GYP

WC	STU      GYP

WC	STU      GYP

WC	STU      GYP

WC	STU      GYP

WC	STU      GYP

WC	STU      GYP

GYP     GYP      09	2

GYP     GYP      09	2

GYP     GYP      09	2	H

GYP     GYP      05	2

GYP     GYP      05	2

GYP     GYP      08	2

GYP     GYP      05	2

GYP     GYP      05	2	G

GYP     GYP      05	2

ABBREVIATIONS

FF      FACTORY FINISH	WC      WOOD CONSTRUCTION FT      FACTORY                                                      SI	SINGLE DOOR

F	HM     HOLLOW METAL PT      PAINT

DL      DOUBLE DOOR	F

FRP     FIBER RESISTANT PANEL

GYP     GYP. BOARD FINISH

PH      PANIC HARDWARE

STU     STUCCO FINISH
TB.     T-BAR CEILING SYSTEM

SF      STOREFRONT                                                TK      TACKBOARD FINISH SGP     SEMI-GLOSS PAINT                                    WIN     WINDOW SYSTEM

E	LEGEND	E

N	NOTIFIER	S
.
P	PUSH BUTTON	A

LOW VOLTAGE PATHWAY

STROBE LIGHT. SEE DETAIL 10/D1.1

CARD READER / ACCESS DEVICE

KEYNOTES X

D	1. DEMO FINISHES TO ACCESS WORK. REPAIR ALL FINISHES BACK TO ORIGINAL FINISH/CONDITION.	D 2. SEE SPECIFICATIONS FOR MORE INFORMATION.

C

L

C 15885

9-30-21 RENEWAL DATE

B		B PROJECT NAME
BUD RANK ELEMENTARY SCHOOL 3650 Powers Ave, Clovis Ca. 93619

No. DATE .	-
.	.

.	.

DESCRIPTION -
.

.

No. DATE .	.
.	.

.	.

DESCRIPTION	REVISIONS .
.

.

SHEET NAME PORTABLES - CLASSROOMS FLOOR PLAN

A

15	14	13	12	11	10	9	8	7	6

JOHN SMITH     PROJECT ARCHITECT

.
LUIS OLVERA	DRAWN BY .                                  CHECKED BY
5	4	3

S21005

N.T.S.

MAY 26, 2021

2

PROJECT NUMBER

SCALE

DATE

SHEET NUMBER       A

A7.1

1

ITEM NO. 1-13

SIM-PBK                           ITEM NO. 1-14           S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

SECTION 08 71 00

DOOR HARDWARE

PART 1 - GENERAL

1.1	RELATED DOCUMENTS

A.	Drawings and general provisions of Contract, including General and Supplementary Conditions of Division 01 Specification Sections, apply to this Section.

1.2	SUMMARY

A.	This Section includes items known commercially as door or finish hardware that are required for swing, sliding, and folding doors, except special types of unique hardware specified in the same sections as the doors and door frames on which they are installed.

B.	Related Sections: The following sections are noted as containing requirements that relate to this Section, but may not be limited to this listing.
1.	Division 08: Section - Hollow Metal Doors and Frames. 2.	Division 08: Section - Flush Wood Doors.
3.	Division 08: Section - Aluminum-Framed Storefronts.
4.	Division 28: Section - Access Control and Fire/Life-Safety Systems

1.3	REFERENCES

A.	2019 California Building Code, CCR Title 24, Part 2

B.	BHMA - Builders’ Hardware Manufacturers Association

C.	DHI - Door and Hardware Institute

D.	NFPA - National Fire Protection Association.
1.	NFPA 80 - Fire Doors and Other Opening Protectives 2.	NFPA 105 - Smoke and Draft Control Door Assemblies

E.	UL - Underwriters Laboratories.
1.	UL 10C - Fire Tests of Door Assemblies 2.	UL 305 - Panic Hardware

F.	WHI - Warnock Hersey Incorporated

G.	SDI - Steel Door Institute

1.4	SUBMITTALS & SUBSTITUTIONS

A.	General: Submit in accordance with Conditions of the Contract and Division 01 Specification sections.

B.	Submit product data (catalog cuts) including manufacturers' technical product information for each item of door hardware, installation instructions, maintenance of operating parts and finish, and other information necessary to show compliance with requirements.

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 1

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

C.	Submit electronic PDF copies of schedule organized vertically into “Hardware Sets” with index of doors and headings, indicating complete designations of every item required for each door or opening. Include following information:
1.	Include a Cover Sheet with:
a.	Job Name, location, telephone number.
b.	Architects name, location and telephone number.
c.	Contractors name, location, telephone number and job number. d.	Suppliers name, location, telephone number and job number. e.	Hardware consultant's name, location and telephone number.
2.	Job Index information included:
a.	Numerical door number index including; door number, hardware heading number and page number.
b.	Complete keying information (referred to DHI hand-book "Keying Systems and Nomenclature"). Provision should be made in the schedule to provide keying information when available; if it is not available at the time the preliminary schedule is submitted.
c.	Manufacturers' names and abbreviations for all materials.
d.	Explanation of abbreviations, symbols, and codes used in the schedule. e.	Mounting locations for hardware.
f.	Clarification statements or questions.
g.	Catalog cuts and manufacturer’s technical data and instructions. 3.	Vertical schedule format sample:

Heading Number 1 (Hardware group or set number - HW Group #1)

(a) 1 Single - Door #101 - Corridor 101 to Exterior
	(b) 90
	(c) RH

(d) 3'-0" x 7'-0" x 1-3/4" - Wood Door x Hollow Metal Frame - 20 Minute

(e) 1.
	(f) 3 ea
	(g) Hinges - (h) 5BB1 4.5 x 4.5 NRP (i) 1/2 TMS
	(j) 630
	(k) IVE
	
2.
	1 ea
	Lockset - ND80P6D x RHO x RH x 10-025 x JTMS
	626
	SCH
	
3.
	1 ea
	Closer - 4040XP x EDA x TBSRT
	689
	LCN

(a)	Single or pair of doors with opening number and location. (b)	Degree of opening.
(c)	Hand of door(s).
(d)	Door/frame dimensions and material; Label requirements, if any. (e)	Hardware item line # (Optional).
(f)	Quantity.
(g)	Product description. (h)	Product part number.
(i)	Fastenings and other pertinent information.
(j)	Hardware finish codes per ANSI/BHMA A156.18. (k)	Manufacturer abbreviation.

D.	Make substitution requests in accordance with Division 01. Substitution requests must be made prior to bid date. Include product data and indicate benefit to the project. Furnish samples of any proposed substitution.

E.	Wiring Diagrams: Provide product data and wiring and riser diagrams for all electrical products listed in the Hardware Schedule portion of this section.

F.	Keying Schedule: Submit separate detailed schedule indicating clearly how the Owner's final instructions on keying of locks has been fulfilled.

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 2

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

G.	Templates for doors, frames, and other work specified to be factory prepared for the installation of door hardware. Check shop drawings of other work to confirm that adequate provisions are made for locating and installing door hardware to comply with indicated requirements.

H.	Furnish as-built/as-installed schedule with close-out documents, including keying schedule and transcript, wiring/riser diagrams, manufacturers’ installation and adjustment and maintenance information.

I.	Fire Door Assembly Testing: Submit a written record of each fire door assembly to the Owner to be made available to the Authority Having Jurisdiction (AHJ) for future building inspections.

J.	LEED Certification Points: Submit information and certifications necessary to achieve maximum points for LEED certification; coordinate and cooperate with Owner and Architect in providing information necessary for required LEED rating.

1.5	QUALITY ASSURANCE

A.	Obtain each type of hardware (latch and lock sets, hinges, closers, exit devices, etc.) from a single manufacturer.

B.	Supplier Qualifications: A recognized architectural door hardware supplier, with warehousing facilities in the project's vicinity, that has a record of successful in-service performance for supplying door hardware similar in quantity, type, and quality to that indicated for this project and that employs an experienced architectural hardware consultant (AHC) who is available to Owner, Architect, and Contractor, at reasonable times during the course of the Work, for consultation.
1.	Responsible for detailing, scheduling and ordering of finish hardware.
2.	Meet with Owner to finalize keying requirements and to obtain final instructions in writing. 3.	Stock parts for products supplied and are capable of repairing and replacing hardware
items found defective within warranty periods.

C.	Hardware Installer: Company specializing in the installation of commercial door hardware with five years documented experience.

D.	Fire-Rated Openings: Provide door hardware for fire-rated openings that complies with NFPA 80 and requirements of authorities having jurisdiction. Provide only items of door hardware that are listed and tested by UL or Warnock Hersey for given type/size opening and degree of label. Provide proper latching hardware, door closers, approved-bearing hinges and seals whether listed in the Hardware Schedule or not.
1.	Where emergency exit devices are required on fire-rated doors, (with supplementary marking on doors' UL labels indicating "Fire Door to be Equipped with Fire Exit Hardware") provide UL label on exit devices indicating "Fire Exit Hardware".

E.	Exit Doors: Operable from inside with single motion without the use of a key or special knowledge or effort.

F.	Product packaging to be labelled in compliance with CA Prop 65, Safe Drinking Water and Toxic Enforcement Act of 1986.

1.6	DELIVERY, STORAGE AND HANDLING

A.	Coordinate delivery of packaged hardware items to the appropriate locations (shop or field) for installation.

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 3

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

B.	Hardware items shall be individually packaged in manufacturers’ original containers, complete with proper fasteners. Clearly mark packages on outside to indicate contents and locations in hardware schedule and in work.

C.	Provide locked storage area for hardware, protect from moisture, sunlight, paint, chemicals, etc.

D.	Contractor to inventory door hardware jointly with representatives of hardware supplier and hardware installer until each all are satisfied that count is correct.

1.7	WARRANTY

A.	Provide warranties of respective manufacturers’ regular terms of sale from day of final acceptance as follows:
1.        Locksets: Ten (10) years. 2.        Closers: Thirty (30) years.
3.	Exit devices: Three (3) years. 4.	Electronic: One (1) year.
5.	All other hardware: Two (2) years.

1.8	MAINTENANCE

A.	Maintenance Tools and Instructions:	Furnish a complete set of specialized tools and maintenance instructions as needed for Owner's continued adjustment, maintenance, and removal and replacement of door hardware.

1.9	PRE-INSTALLATION CONFERENCE

A.	Convene a pre-installation conference at least one week prior to beginning work of this section.

B.	Attendance: Architect, Construction Manager, Contractor, Security Contractor, Hardware Supplier, Installer, Key Owner’s Personnel, and Project Inspector.

C.	Agenda:	Review hardware schedule, products, installation procedures and coordination required with related work. Review Owner's keying standards.

PART 2 - PRODUCTS

2.1	MANUFACTURERS

Item	Manufacturer	Acceptable Substitutes

Hinges
Locks, Latches & Cylinders Exit Devices
Closers
Push, Pulls & Protection Plates Door Stops
Overhead Stops Thresholds Seals & Bottoms

Ives Schlage Von Duprin LCN Ives Ives
Glynn-Johnson Zero Zero

Hager, Stanley, McKinney None – District Standard None – District Standard None – District Standard Trimco, BBW, DCI Trimco, BBW, DCI
Or Approved Equal Pemko, National Guard Pemko, National Guard

2.2	MATERIALS

A.	Hinges:

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 4

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

1.	Provide hinges conforming to ANSI/BHMA A156.1.
2.	Hinges shall be sized in accordance with the following: a.	Height:
1)	Doors up to 42" wide: 4-1/2 inches. 2)	Doors 43" to 48" wide: 5 inches.
b.	Width: Sufficient to clear frame and trim when door swings 180 degrees.
c.	Number of Hinges: Provide 3 hinges per leaf to 7'-5" in height. Add one for each additional 2 feet in height.
3.	Exterior out-swinging hinges shall be non-ferrous material and shall have stainless steel hinge pins. All doors to have non-rising pins.
4.	Furnish non-removable pins (NRP) at all exterior out-swing doors and interior key lock doors with reverse bevels.
5.	Provide hinges with electrified options as scheduled in the hardware sets. Provide with sufficient number and wire gage to accommodate electric function of specified hardware. Locate electric hinge at second hinge from bottom or nearest to electrified locking component.

B.	Continuous Hinges:
1.	Provide aluminum geared continuous hinges fabricated from 6063-T6 aluminum conforming to ANSI/BHMA A156.26, Grade 1.
2.	Provide split nylon bearings at each hinge knuckle for quiet, smooth, self-lubricating operation.
3.	Provide continuous hinges capable of supporting door weights up to 450 pounds, and successfully tested for 1,500,000 cycles.
4.	Provide continuous hinges 1” shorter in length than nominal height of door, unless otherwise noted, with symmetrical hole pattern.
5.	Provide continuous hinges with electrified option, as scheduled, with sufficient number and wire gage to accommodate electric function of specified hardware.
6.	Install continuous hinges with fasteners supplied by manufacturer.

C.	Heavy Duty Cylindrical Locks and Latches: Schlage "ND" Series as scheduled with "Rhodes" lever design.
1.	Provide cylindrical locks conforming to ANSI/BHMA A156.2 Series 4000, Grade 1, and UL Listed for 3 hour fire doors.
2.	Provide cylindrical locksets exceeding the ANSI/BHMA A156.2 Grade 1 performance standards for strength, security, and durability in the categories below:
a.	Abusive locked lever torque – minimum 3,100 inch-pounds without gaining access. b.	Offset lever pull – minimum 1,600 foot pounds without gaining access.
c.	Vertical lever impact – minimum 100 impacts without gaining access.
d.	Cycle Test – tested to minimum 16 million cycles with no visible lever sag; without the use of performance aids such as set screws or spacers.
3.	Cylinders: Refer to “KEYING” article, herein.
4.	Provide locks with standard 2-3/4” backset, unless noted otherwise, with 1/2” latch throw. Provide proper latch throw for UL listing at pairs.
5.        Provide locksets with separate solid steel anti-rotation thru-bolts, and no exposed screws. 6.        Provide independently operating levers with two external return spring cassettes mounted
under roses to prevent lever sag.
7.	Provide standard ASA strikes unless extended lip strikes are necessary to protect trim. 8.	Lever Trim: Solid cast levers without plastic inserts and wrought roses on both sides.
9.	Provide levers with vandal resistant technology as scheduled for use at abusive applications.

D.	Exit devices: Von Duprin as scheduled.
1.	Provide exit devices tested to ANSI/BHMA A156.3 Grade 1 and UL listed for Panic Exit or Fire Exit Hardware.

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 5

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

2.	Provide certificate by independent testing laboratory that device has completed over 1,000,000 cycles and can still meet ANSI/BHMA A156.3 standards.
3.	Provide touchpad type exit devices, fabricated of brass, bronze, stainless steel, or aluminum, plated to standard architectural finishes to match balance of door hardware.
4.	Provide exit devices cut to door width and height. Touchpad must extend a minimum of one half of door width. No plastic inserts are allowed in touchpads.
5.	Mount mechanism case flush on face of doors, or provide spacers to fill gaps behind devices. Where glass trim or molding projects off face of door, provide glass bead kits.
6.	Provide flush end caps for exit devices.
7.	Exit devices shall comply with CBC Section 11B-404.2.7 and shall be mounted between 34" and 44" above the finished floor surface.
8.	Provide exit devices UL certified to meet 5 lbs. maximum unlatching force requirements according to the CBC Section 11B-309.4.
9.	Cylinders: Refer to “KEYING” article, herein.
10.	Provide cylinder or hex-key dogging as specified at non fire-rated openings.
11.	Provide cylinder dogging indicators (CDSI) for visible indication of dogging status as specified.
12.	Removable Mullions: Provide type that can be removed by use of a keyed cylinder, which is self-locking when re-installed.
13.	Provide factory drilled weep holes for exit devices used in full exterior application, highly corrosive areas, and where noted in hardware sets.
14.	Provide exit devices with deadlatching feature for security and for future addition of alarm kits and/or other electrified requirements.
15.	Provide exit devices with optional trim designs to match other lever and pull designs used on the project.
16.	Provide exit devices with manufacturer’s approved strikes.

E.	Closers: LCN as scheduled.
1.	Provide door closers conforming to ANSI/BHMA A156.4 Grade 1 requirements by BHMA certified independent testing laboratory. ISO 9000 certify closers. Stamp units with date of manufacture code.
2.	Provide door closers with fully hydraulic, full rack and pinion action with high strength cast iron cylinder, and full complement bearings at shaft.
3.	Provide certificate by independent testing laboratory that door closers have completed over 10,000,000 cycles and can still meet ANSI/BHMA A156.4 standards.
4.	Cylinder Body: 1-1/2” diameter with 3/4” diameter double heat-treated pinion journal.
5.	Hydraulic Fluid: Fireproof, passing requirements of UL10C, and requiring no seasonal closer adjustment for temperatures ranging from 120° F to -30° F.
6.	Spring Power: Continuously adjustable over full range of closer sizes, and providing reduced opening force as required by accessibility codes and standards.
7.	Hydraulic Regulation: By tamper-proof, non-critical valves, with separate adjustment for latch speed, general speed, and backcheck.
8.	Provide closers with solid forged steel main arms and factory assembled heavy-duty forged forearms for parallel arm closers.
9.	Pressure Relief Valve (PRV) Technology: Not permitted.
10.	Provide door closers powder coated to match balance of door hardware. Powder coating finish shall be certified to exceed 100 hours salt spray testing as described in ANSI/BHMA A156.4 and ASTM B117.
11.	Provide special rust inhibitor (SRI) in highly corrosive areas, and where noted in hardware sets.
12.	Provide special templates, drop plates, mounting brackets, or adapters for arms as required for details, overhead stops, and other door hardware items interfering with closer mounting.

F.	Door Stops:

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 6

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

1.	Unless otherwise noted in hardware sets, provide floor type with appropriate fasteners. Where floor type cannot be used, provide wall type. If neither can be used, provide overhead type.
2.	Do not install floor stops more than four (4) inches from the face of the wall or partition (CBC Section 11B-307).
3.	Provide backing plate at wall framing behind wall type.
4.	Overhead stops shall be made of stainless steel and non-plastic mechanisms and finished metal end caps. Field-changeable hold-open, friction and stop-only functions. Stop-only function shall be provided at fire-rated openings.

G.	Protection Plates:
1.	Provide kick, mop, and/or armor plates minimum of 0.050” thick, with four beveled edges. Furnish with sheet metal or wood screws, finished to match plates.
2.	Kick plates shall be sized 10" high and 2" less door width (LDW) at single doors and 10” high and 1” LDW at pairs or doors.
3.	Provide mop and armor plates with sizes as scheduled in hardware sets.

H.	Thresholds: As scheduled and per details.
1.	Thresholds shall not exceed 1/2" in height, with a beveled surface of 1:2 maximum slope. Thresholds shall comply with CBC Section 11B-404.2.5.
2.	Set thresholds in a full bed of butyl-rubber or polyisobutylene mastic sealant complying with requirements in Division 07 “Thermal and Moisture Protection”.
3.	Use 1/4” fasteners, red-head flat-head sleeve anchors (SS/FHSL).

I.	Seals: Provide silicone gasket at all rated and exterior doors.
1.	Smoke & Draft Control Doors: Provide UL10C Classified complies with NFPA 80 & NFPA 252 for use on “S” labeled Positive Pressure door assemblies.

2.3	KEYING

A.	Furnish a Proprietary Schlage masterkey system as directed by the owner or architect. Key system to be designated and combinated by the Schlage Master Key Department even if pinned by the Authorized Key Center, Authorized Security Center or a local authorized commercial dealer.

B.	A detailed keying schedule is to be prepared by the owner and/or architect in consultation with a representative of Allegion or an Authorized Key Center or Authorized Security Center. Each keyed cylinder on every keyed lock is to be listed separately showing the door #, key group (in BHMA terminology), cylinder type, finish and location on the door.

C.	Furnish all cylinders in the Schlage conventional style except the exit device and removable mullion cylinders which will be supplied in Schlage Full Size Interchangeable Core (FSIC). Pack change keys independently (PKI).

D.	Furnish construction keying for doors requiring locking during construction.

E.	Furnish all keys with visual key control. 1.	Stamp key “Do Not Duplicate”.
2.	Stamp (BHMA) key symbol on key.
3.	Stamp unique owner identifier from the key bow.

F.	Furnish all cylinders with visual key control.
1.	Stamp (BHMA) key symbol on side of cylinder (CKC).

G.	Furnish mechanical keys as follows:

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 7

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

1.	Furnish 2 cut change keys for each different change key code. 2.	Furnish 1 uncut key blank for each change key code.
3.	Furnish 6 cut masterkeys for each different masterkey set. 4.	Furnish 3 uncut key blanks for each masterkey set.
5.	Furnish 2 cut control keys cut to the top masterkey for permanent I/C cylinders. 6.	Furnish 1 cut control key cut to each SKD combination.

2.4	FINISHES

A.	Generally to be satin chrome US26D (626 on bronze and 652 on steel) unless otherwise noted.

B.	Furnish push plates, pull plates and kick or armor plates in satin stainless steel US32D (630) unless otherwise noted.

C.	Door closers shall be powder-coated to match other hardware, unless otherwise noted.

D.	Aluminum items to be finished anodized aluminum except thresholds which can be furnished as standard mill finish.

2.5	FASTENERS

A.	Screws for strikes, face plates and similar items shall be flat head, countersunk type, provide machine screws for metal and standard wood screws for wood.

B.	Screws for butt hinges shall be flathead, countersunk, full-thread type.

C.	Fastening of closer bases or closer shoes to doors shall be by means of sex bolts and spray painted to match closer finish.

D.	Provide expansion anchors for attaching hardware items to concrete or masonry.

E.	All exposed fasteners shall have a phillips head.

F.	Finish of exposed screws to match surface finish of hardware or other adjacent work.

G.	All Exit Devices and Lock Protectors shall be fastened to the door by the means of sex bolts or through bolts.

PART 3 - EXECUTION

3.1	INSPECTION

A.	Verify that doors and frames are square and plumb and ready to receive work and dimensions are as instructed by the manufacturer.

B.	Beginning of installation means acceptance of existing conditions.

3.2	INSTALLATION

A.	Install hardware in accordance with manufacturer's instructions and requirements of DHI.

B.	Use the templates provided by hardware item manufacturer.

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 8

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

C.	Mounting heights for hardware shall be as recommended by DHI. Operating hardware shall be located between 34" and 44" above finish floor to comply with CBC Section 11B-404.2.7.

D.	Door Closers:
1.	Place door closers inside building, stairs, rooms, etc. Closers shall be installed to permit doors to swing 180 degrees or maximum allowable by conditions.
2.	Maximum effort to operate closers shall not exceed 5 lbs., such pull or push effort being applied at right angles to hinged doors.
3.	When fire doors are required, the maximum effort to operate the closer may be increased but shall not exceed 15 lbs. when specifically approved by fire marshal.
4.	All closers shall be adjusted to operate with the minimum amount of opening force and still close and latch the door. These forces do not apply to the force required to retract latch bolts or disengage other devices that hold the door in a closed position.
5.	Compensating devices or automatic door operators may be utilized to meet the above standards.
6.	Per CBC Section 11B-404.2.8.1, doors shall take minimum of 5 seconds to move from an open position of 90 degrees to 12 degrees to the latch jamb.

E.	Set units level, plumb and true to line and location. Adjust and reinforce the attachment substrate as necessary for proper installation and operation.

F.	Drill and countersink units that are not factory-prepared for anchorage fasteners.	Space fasteners and anchors in accordance with industry standards.

G.	Set thresholds for exterior doors in full bed of butyl-rubber sealant.

H.	If hand of door is changed during construction, make necessary changes in hardware at no additional cost.

I.	Electronic Hardware:
1.	Hardware Installer shall coordinate with security contractor to route cable to connect electrified locks, panic hardware and fire exit hardware to power transfers or electric hinges at the time these items are installed so as to avoid disassembly and reinstallation of hardware.
2.	Hardware Installer shall also be present with the security contractor when the power is turned on for the testing of the electronic hardware applications. Installer shall make adjustments to solenoids, latches, vertical rods and closers to insure proper and secure operation.
3.	All wiring for electro-mechanical hardware mounted on the door shall be connected through the power transfer and terminated in the interface junction box specified for in the Electrical Section.
4.	Conductors shall be minimum 18 gage stranded, multicolored. A minimum 12 in. loop of conductors shall be coiled in the interface junction box.	Each conductor shall be permanently marked with its function.
5.	If a power supply is specified in the hardware sets, all conductors shall be terminated in the power supply. Make all connections required for proper operation between the power supply and the electro-mechanical hardware. Provide the proper size conductors as specified in the manufacturer’s technical documentation.

3.3	ADJUST AND CLEAN

A.	Adjust and check each operating item of hardware and each door, to ensure proper operation or function of every unit. Replace units which cannot be adjusted to operate freely and smoothly as intended for the application made.

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 9

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

B.	Clean adjacent surface soiled by hardware installation.

C.	Final Adjustment: Wherever hardware installation is made more than one month prior to acceptance or occupancy, return to that work area and make final check and adjustment of all hardware items in such space or area. Clean operating items as necessary to restore proper function and finish of hardware and doors. Adjust door control devices to compensate for final operation of heating and ventilating equipment.

D.	Instruct Owner's Personnel in proper adjustment and maintenance of hardware finishes, during the final adjustment of hardware.

E.	Continued Maintenance Service: Approximately six months after the completion of the project, the Contractor accompanied by the Architectural Hardware Consultant, shall return to the project and re-adjust every item of hardware to restore proper functions of doors and hardware. Consult with and instruct Owner's personnel in recommended additions to the maintenance procedures. Replace hardware items which have deteriorated or failed due to faulty design, materials or installation of hardware units. Prepare a written report of current and predictable problems (of substantial nature) in the performance of the hardware.

3.4	HARDWARE LOCATIONS

A.	Conform to CCR, Title 24, Part 2; and ADAAG; and the drawings for access-compliant positioning requirements for the disabled.

3.5	FIELD QUALITY CONTROL

A.	Contractor is responsible for providing the services of an Architectural Hardware Consultant (AHC) or a proprietary product technician to inspect installation and certify that hardware and its installation have been furnished and installed in accordance with manufacturers’ instructions and as specified herein.

3.6	HARDWARE SCHEDULE

A.	The items listed in the following schedule shall conform to the requirements of the foregoing specifications.

B.	While the hardware schedule is intended to cover all doors, and other movable parts of the building, and establish type and standard of quality, the contractor is responsible for examining the Plans and Specifications and furnishing proper hardware for all openings whether listed or not. If there are any omissions in hardware groups in regard to regular doors they shall be called to the attention of the Architect prior to bid opening for instruction; otherwise, list will be considered Complete. No extras will be allowed for omissions.

C.	The Door Schedule on the Drawings indicates which hardware set is used with each door.

MANUFACTURERS ABBREVIATIONS

IVE	=	Ives
SCE	=	Schlage Electronics SCH	=	Schlage Lock
VON	=	Von Duprin

Hinges
Electronic Door Components Locks, Latches & Cylinders Exit Devices & Electric Strikes

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 10

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

HW GROUP NO. 01

For use on Door #(s):

1	4	5	14	15	25 26	27	28

QTY	DESCRIPTION

1	EA	ELECTRIC HINGE
1	EA	QEL CONVERSION KIT 1	EA	RX SWITCH KIT
1	EA	LD COVER PLATE
1	EA	MULTITECH READER 1	EA	DOOR CONTACT

CATALOG NUMBER

5BB1HW 4.5 X 4.5 TW8 958003
050251-00 050589
MT15 12 VDC 7766
RE-USE BALANCE OF EXISTING HARDWARE

FINISH	MFR

630	IVE 626	VON 626	VON 626	VON BLK	SCE 628	SCE

HW GROUP NO. 02

For use on Door #(s):

2	23	24

QTY	DESCRIPTION

1	EA	STOREROOM LOCK 1	EA	ELECTRIC STRIKE
1	EA	MULTITECH READER 1	EA	DOOR CONTACT
1	EA	REQUEST TO EXIT SENSOR POWER SUPPLY

CATALOG NUMBER

ND80P6D RHO
6400 FSE 12/24 VAC/VDC MT15 12 VDC
7766
SCANII 12/24 VDC
BY WORK OF DIVISION 28
RE-USE BALANCE OF EXISTING HARDWARE

FINISH	MFR

626	SCH 630	VON BLK	SCE 628	SCE WHT	SCE

HW GROUP NO. 03

For use on Door #(s): 3

QTY	DESCRIPTION

1	EA	ELEC CONT. HINGE
1	EA	QEL CONVERSION KIT 1	EA	RX SWITCH KIT
1	EA	LD COVER PLATE
1	EA	MULTITECH READER 1	EA	DOOR CONTACT

CATALOG NUMBER

112XY TWP 958003 050251-00 050589
MT15 12 VDC 7766
RE-USE BALANCE OF EXISTING HARDWARE

FINISH	MFR

628	IVE 626	VON 626	VON 626	VON BLK	SCE 628	SCE

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 11

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

HW GROUP NO. 04

For use on Door #(s):
6	7	8	9	17	18 19	20	21	22

QTY	DESCRIPTION

2	EA	ELECTRIC HINGE
1	EA	QEL CONVERSION KIT 2	EA	RX SWITCH KIT
2	EA	LD COVER PLATE 1	EA	EXIT DEVICE TRIM 1	EA	RIM CYLINDER
1	EA	MULTITECH READER 2	EA	DOOR CONTACT

CATALOG NUMBER

5BB1HW 4.5 X 4.5 TW8 958003
050251-00 050589 990-NL
20-057
MT15 12 VDC 7766

FINISH	MFR

630	IVE 626	VON 626	VON 626	VON 626	VON 626	SCH BLK	SCE 628	SCE

RE-USE BALANCE OF EXISTING HARDWARE

HW GROUP NO. 05

For use on Door #(s):

10	16	33 38	5A                         18A

34	36	37 20A                      22A                      28A

QTY	DESCRIPTION

1	EA	STOREROOM LOCK 1	EA	ELECTRIC STRIKE
1	EA	MULTITECH READER 1	EA	DOOR CONTACT
1	EA	REQUEST TO EXIT SENSOR POWER SUPPLY

CATALOG NUMBER

ND80P6D RHO
6400 FSE 12/24 VAC/VDC MT15 12 VDC
7766
SCANII 12/24 VDC
BY WORK OF DIVISION 28
RE-USE BALANCE OF EXISTING HARDWARE

FINISH	MFR

626	SCH 630	VON BLK	SCE 628	SCE WHT	SCE

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 12

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

HW GROUP NO. 06

For use on Door #(s): 11                         13

QTY	DESCRIPTION

2	EA	ELECTRIC HINGE
1	EA	QEL CONVERSION KIT 2	EA	RX SWITCH KIT
2	EA	LD COVER PLATE
1	EA	MULTITECH READER 2	EA	DOOR CONTACT

CATALOG NUMBER

5BB1HW 4.5 X 4.5 TW8 958003
050251-00 050589
MT15 12 VDC 7766

FINISH	MFR

630	IVE 626	VON 626	VON 626	VON BLK	SCE 628	SCE

RE-USE BALANCE OF EXISTING HARDWARE

HW GROUP NO. 07

For use on Door #(s): 12

QTY	DESCRIPTION

1	EA	ELECTRIC HINGE
1	EA	EU STOREROOM LOCK 1	EA	MULTITECH READER
2          EA         DOOR CONTACT POWER SUPPLY

CATALOG NUMBER

5BB1HW 4.5 X 4.5 TW8 ND80P6DEU RHO RX 12V/24V DC MT15 12 VDC
7766
BY WORK OF DIVISION 28
RE-USE BALANCE OF EXISTING HARDWARE

FINISH	MFR

630	IVE 626	SCH BLK	SCE 628	SCE

HW GROUP NO. 08

For use on Door #(s): 35

QTY	DESCRIPTION

1	EA	STOREROOM LOCK 1	EA	ELECTRIC STRIKE
1	EA	MULTITECH READER 1	EA	DOOR CONTACT
1	EA	REQUEST TO EXIT SENSOR POWER SUPPLY

CATALOG NUMBER

L9080P6 06L
6400 FSE 12/24 VAC/VDC MT15 12 VDC
7766
SCANII 12/24 VDC
BY WORK OF DIVISION 28
RE-USE BALANCE OF EXISTING HARDWARE

FINISH	MFR

626	SCH 630	VON BLK	SCE 628	SCE WHT	SCE

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 13

SIM-PBK                                                                                                S21005 BUD RANK ELEMENTARY SCHOOL LOCKDOWN SYSTEM

HW GROUP NO. 09

For use on Door #(s):

29	30	31	32

QTY	DESCRIPTION

1	EA	ELECTRIC HINGE
1	EA	ELEC PANIC HARDWARE 1	EA	RIM CYLINDER
1	EA	MULTITECH READER 1	EA	DOOR CONTACT

CATALOG NUMBER

5BB1HW 4.5 X 4.5 TW8
RX-QELX-PA-AX-99-NL 24 VDC 20-057
MT15 12 VDC 7766
RE-USE BALANCE OF EXISTING HARDWARE

FINISH	MFR

630	IVE 626	VON 626	SCH BLK	SCE 628	SCE

HW GROUP NO. MISC

QTY	DESCRIPTION

13	EA	POWER SUPPLY
100	EA	SMART CREDENTIAL

CATALOG NUMBER

PS902 900-2RS 120/240 VAC 2520 SPV MIFARE DESFIRE EV2

FINISH	MFR

VON WHT	SCE

SHARE POWER SUPPLIES BETWEEN THE FOLLOWING DOORS: -	DOORS 1 & 5
-	DOORS 3 & 4
-	DOORS 14 & 15 -	DOORS 25 & 26 -	DOORS 27 & 28 -	DOORS 29 & 30 -	DOORS 31 & 32 -	DOORS 6 & 7
-	DOORS 8 & 9
-	DOORS 11 & 13 -	DOORS 17 & 18 -	DOORS 19 & 20 -	DOORS 21 & 22

END OF SECTION

Prepared by Allegion, PLC

OPT0211887

DOOR HARDWARE 08 71 00 - 14