ADDENDUM NO. 1	DATE: 03/20/23

PROJECT:

McKinley/ Fowler Elementary School- Increment2- Electrical Rebid Fresno, CA
CUSD Bid No.: 2932

OWNER:

Clovis Unified School District 1450 E. Herndon Ave.
Clovis, CA 93611

ARCHITECT:

DARDEN ARCHITECTS, INC.

Attention: Andrew Corral/ Mike Fennacy 6790 N. West Avenue
Fresno, California 93711 T.	(559) 448-8051
F.	(559) 446-1765

DARDEN PROJECT NO. 2116 DSA File Nos. 10-48
DSA APPL. NO. 02-120543

It will be the responsibility of the General Contractor to submit the information contained in this addendum to all its subcontractors and suppliers. Acknowledge receipt of this Addendum in the space provided on the Bid Form. Failure to do so may subject B disqualification.

The following additions, deletions, and revisions to the SHEETS and Project Manual are hereby made and do become a part of these Contract Documents.

William Brandle

PROJECT: McKinley/ Fowler Elementary School- Increment 2- Electrical Rebid

ADDENDUM NO.1...............................................................................................................DATE: 03/20/23 PAGE 2

INDEX OF ADDENDATRANSMITTED HEREWITH

PROJECT MANUAL:

BIDDING AND CONTRACTREQUIREMENTS:

CHANGES TOINTRODUCTORYINFORMATION....................................................AD1-CII01 Thru CII02

CHANGES TO CONDITIONS OF THE CONTRACT................................................................. AD1-CCC01

SPECIFICATIONS:

CHANGES TO SPECIFICATIONS..............................................................................................AD1-SP01

ATTACHMENTS:

DOCUMENTS OR SPECIFICATIONS:

01 11 13 SUMMARY OF WORK.........................................................................................(Pages 1 thru 91)

PROJECT: McKinley/ Fowler Elementary School- Increment 2- Electrical Rebid

ADDENDUM NO.1...............................................................................................................DATE: 03/20/23 PAGE 3

PROJECT MANUAL:

BIDDING AND CONTRACT REQUIREMENTS:

CHANGES TOINTRODUCTORYINFORMATION: AD1-CII01	Refer to NOTICE TO CONTRACTORS:
1. Remove and replace the NOTICE TO CONTRACTORS with the attached NOTICE TO CONTRACTORS as indicated with an AD-1 in the upper right-hand corner.

AD1-CII02	Refer to NOTICE TO CONTRACTORS:

1. Insert the following dates included in the attached Revisions to NOTICE TO CONTRACTORS as indicated with an AD-1 in the upper right-hand corner.

CHANGES TO CONDITIONS OF THE CONTRACT: AD1-CCC01	Refer to General Conditions:
1. Refer to the Insurance rating requirement change described in the attached letter from the district as indicated with an AD-1 in the upper right-hand corner.
END OF ADDENDUM NO. 1

NOTICE TO CONTRACTORS

Notice is hereby given that CLOVIS UNIFIED SCHOOL DISTRICT, (hereinafter referred to as "Owner") will receive sealed bids prior to the date and time stated for the Bid Opening for construction of:

BID 2932– REBID FOWLER MCKINLEY ELEMENTARY SCHOOL - PHASE 2 ELECTRICAL

as per drawings and specifications which may be obtained from architect: DARDEN ARCHITECTS
MIKE FENNACY or ANDREW CORRAL 6790 N. WEST AVENUE FRESNO, CALIFORNIA 93711 (559) 448-8051

Upon receipt of the contract documents provide the following information: 1.      Organization/Contact Person for each Prime Contractor
2.	Mailing address and P.O. Box Number for each Prime Contractor 3.	Phone Number for each Prime Contractor
4.	FAX Number for each Prime Contractor

The project will be bid as multiple prime contracts according to the list below:

Bid Package #
	Bid Package Description
	Contractor License Requirement (, = or)
	
CES-15
	BUILDING ELECTRICAL
	C-10

Mandatory Pre-Bid Meeting
To be eligible to bid this project, ALL bid packages must attend pre-bid meeting job walk.

March 28, 2023 at 10:00AM at corner of N. Fowler Ave & E. Weldon Avenue, Fresno County (map location provided in bid documents)

Time of completion for this project shall 544 calendar days (per construction manager’s work schedule) from the start of the project as established within the Owner’s Notice to Proceed. All procurement, coordination, milestones, durations, activities, and sequences for the bid packages shall be performed as shown in the Construction Management Bid Schedule and Section 01320 of the specification and as modified by a monthly schedule update, if any.

Bids will be sealed and filed at the following address: Bids will NOT be accepted at the bid opening location.
Clovis Unified School District PURCHASING
1450 Herndon Avenue Clovis, California 93611
before 11:00 AM on APRIL 5, 2023

Bids will be opened in public at the following address: Bids will NOT be accepted at the bid opening location.
Clovis Unified School District CONSTRUCTION SERVICES OFFICE 1470 Herndon Avenue Clovis, California 93611

The DVBE Declaration of Good Faith Efforts to use Disabled Veteran Business Enterprises must be signed, filed, and included in sealed bid package, before 11:00 AM on APRIL 5, 2023, at which time the bids (including the DVBE Declaration of Good Faith Efforts to Use Disabled Veteran Business Enterprises) will be opened in public.

Bids must be accompanied by a bidder's bond, cashier's check, or certified check for at least ten per cent (10%) of the amount of the base bid and made payable to the Owner, issued by an Admitted Surety (an

insurance organization authorized by the Insurance Commissioner to transact business of insurance in the State of California during this calendar year), which shall be given as a guarantee that the bidder will enter into a contract if awarded the work and will be declared forfeited, paid to, or retained by the Owner as liquidated damages if the bidder refuses or neglects to enter into the contract provided by the Owner after being requested to do so.

The Contractor shall be required to satisfy the conditions set forth in the contract and Education Code section 45125.2 regarding fingerprinting requirements and student safety prior to permitting any contact with students. Upon award of the contract and before beginning work, the Contractor shall be required to provide a verification of compliance with the student safety provisions of the contract and Education Code section 45125.2.

Upon award of the bid, require signature on the enclosed declaration to ensure compliance with the general Conditions and the Education Code.

The successful bidder will be required to furnish a Payment (Labor and Material) Bond in the amount of one hundred per cent (100%) of the contract price, and a Faithful Performance Bond in the amount of one hundred per cent (100%) of the contract price, said bonds to be secured from an Admitted Surety (an insurance organization authorized by the Insurance Commissioner to transact business of insurance in the State of California during this calendar year), and satisfactory to the Owner. The bidder will be required to give satisfactory proof to the Owner of the maintenance of Public Liability and Property Damage Insurance in an amount with a combined single limit of not less than $2,000,000 per occurrence.

The successful bidder will be allowed to substitute securities or establish an escrow in lieu of retainage, pursuant to Public Contract Code Section 22300, and as described in the General Conditions.

The Owner will not consider or accept any bids from contractors who are not licensed to do business in the State of California, in accordance with the California Public Contract Code, providing for the licensing of contractors. In accordance with Section 3300 of said Code, the Contractor shall have a license classification as described in the MULTIPLE PRIME CONTRACT SCHEDULE.

In accordance with Public Contract Code 20111.6, Notice is hereby given that the Clovis Unified School District has determined Bidders performing as both a Prime Contractor and General Contractor (A or B license), or an Electrical, Mechanical, and Plumbing Contractor utilized as a Prime Contractor or Subcontractor must be prequalified prior to bidding on this project. For purposes of this prequalification, Electrical, Mechanical, and Plumbing contractors are contractors holding either a C-4, C-7, C-10, C-16, C-20, C-34, C-36, C-38, C-42, C-43, and C-46 California State Contractors license. Prequalification Applications may be obtained from Clovis USD Purchasing Web Site: https://www.cusd.com/Pre-Qualification.aspx Questionnaire and Financial Statement shall be submitted directly to Clovis Unified School District prior to 11:00 am MARCH 27, 2023. BIDDER MUST PREQUALIFIY UNDER CALENDAR YEAR 2023 APPLICATION PROCESS. ONLINE SUBMITTAL ONLY.

Pursuant to Labor Code sections 1725.5 and 1771.1, all contractors and subcontractors that wish to bid on, be listed in a bid proposal, or enter into a contract to perform public work must be registered with the Department of Industrial Relations. No bid will be accepted, nor any contract entered into without proof of the contractor’s and subcontractors’ current registration with the Department of Industrial Relations to perform public work. If awarded a Contract, the Bidder, and its subcontractors, of any tier, shall maintain active registration with the Department of Industrial Relations for the duration of the Project.

This Project is subject to compliance monitoring and enforcement by the Department of Industrial Relations. In bidding on this project, it shall be the Bidder’s sole responsibility to evaluate and include the cost of complying with all labor compliance requirements under this contract and applicable law in its bid.

The lowest bid shall be determined as follows: The lowest total of the prime bid on the base contract and the bids on all additive items and all deductive items. (Public Contract Code section 20103.8, subd. (b)). The District reserves the right to add or deduct any of the additive or deductive items from the project or contract after the lowest responsible and responsive bidder is determined.

The Director of the Department of Industrial Relations of the State of California, in the manner provided by law, has ascertained the general prevailing rate per diem wages and rate for legal holidays and overtime work

as set forth in the Agreement. The Contractor must pay for any labor therein described or classified in an amount not less than rates specified. Copies of the required rates are on file at the Owner's business office and are available to any interested party on request.

The Owner reserves the right to waive any irregularity and to reject any or all bids.

Unless otherwise required by law, no bidder may withdraw its bid for a period of sixty (60) days after date set for the opening thereof.

Dated:

Advertise:

March 17, 2023

March 20, 2023 March 27, 2023

Clovis Unified School District

By: MICHAEL JOHNSTON
ASSISTANT SUPERINTENDENT OF BUSINESS SERVICES

END OF SECTION

March 17, 2023

CLOVIS UNIFIED SCHOOL DISTRICT

BID 2932 - REBID Fowler McKinley Elementary School – Phase 2 Electrical

ADDENDUM NO. 1

This addendum forms a part of the bid/contract documents. It modifies the original project plans, specifications and instructions. Bidders are required to acknowledge receipt of this addendum on the sheet included with the bid package. Failure to acknowledge receipt of this addendum may subject the bidder to disqualification.

REVISIONS TO NOTICE TO CONTRACTORS:

Mandatory Job Walk - Date changed to Tuesday, March 28, 2023 @ 10:00 am.

Bid Opening - Date changed to Wednesday, April 5, 2023 @ 11:00 am.

DVBE Declaration of Good Faith Efforts – Must be signed, filed, and included in sealed bid package before11:00 am on April 5, 2023.

Prequalification - Bidder must prequalify under the calendar year 2023 application process prior to March 27, 2023 @ 11:00 am.

Advertisement Dates - Changed to 3/20/2023 & 3/27/2023.

If you have any questions, please feel free to contact my office at 559-327-9479.

Leeann Errotabere Director of Purchasing

1-page addendum

Rebid- AD-1

MARCH 17, 2023

CLOVIS UNIFIED SCHOOL DISTRICT
BID 2932 REBID FOWLER MCKINLEY ELEMENTARY SCHOOL - PHASE 2 ELECTRICAL

ADDENDUM NO. 1

This addendum forms a part of the bid/contract documents. It modifies the original project plans, specifications and instructions. Bidders are required to acknowledge receipt of this addendum on the sheet included with the bid package. Failure to acknowledge receipt of this addendum may subject the bidder to disqualification.

Revisions:
Due to COVID and California Wildfire impact on the insurance industry, the AM Best rating requirement on this project is now A- rated or better. Please provide and sign all needed AM Best verification paperwork outlined in bid packet with your sealed bid at time of bid submittal.

Clarification:
AM Best rating requirement of A or better has been reduced to A- or better.
Rating Report information to be obtained from A.M. Best Company –http://www.ambest.com

IF BIDDER SUBMITTED BID AND BID BOND FOR ORIGINAL BID 2923, THEY CAN SUBMIT A COPY OF THAT BID BOND WITH THIS BID SUBMITTAL. IF BIDDER DID NOT PARTICIPATE IN BID 2923, AN ORIGINAL NEWLY ISSUED B ID BOND IS REQUIRED AT TIME OF BID SUBMITTAL. EITHER BOND SUBMITTAL TYPE MUST BE INCLUDED WITH SEALED BID RESPONSE ON DESIGNATED DATE AND TIME.

RFI DEADLINE – MARCH 27, 2023 – 2:00 PM Submit RFI to Andrew Corral – Darden Architects andrewc@dardenarchitects.com

If you have any questions, please feel free to contact my office at 559-327-9479.

Leeann Errotabere Director of Purchasing

1-page addendum

Rebid- AD-1

INCREMENT NO. 1

Bid Package #
	Bid Package Description
	Contractor License Requirement (, = or)
	
CES-01
	EARTHWORK, CONCRETE, & CMU
	A, B, C-8, C-12
	
CES-02
	SITE UTILITIES PLUMBING: DOMESTIC, SANITARY, STORM, FIRE, & GAS
	A, C-36
	
CES-03
	SITE ELECTRICAL & LOW VOLTAGE
	C-10
	
CES-04
	LANDSCAPE
	C-27

INCREMENT NO. 2

Bid Package #
	Bid Package Description
	Contractor License Requirement (, = or)
	
CES-05
	BUILDING CONCRETE & REBAR
	B, C-8
	
CES-06
	STRUCTURAL STEEL
	C-51
	
CES-07
	METAL PANELS, ROOFING, & SHEET METAL
	C-39, C-43
	
CES-08
	FINISH CARPENTRY
	B, C-6
	
CES-09
	METAL FRAMING, PLASTER, AND GYPSUM BOARD
	C-9, C-35
	
CES-10
	WALL MATERIALS AND ACOUSTICAL CEILINGS
	C-2
	
CES-11
	PAINTING
	C-33
	
CES-12
	GENERAL SPECIALTIES
	B
	
CES-13
	FIRE SPRINKLERS
	C-16
	
CES-14
	BUILDING PLUMBING & HVAC
	C-36, C-20
	
CES-15
	BUILDING ELECTRICAL
	C-10
	
CES-16
	OFF-SITE IMPROVEMENTS
	A

*ALL BID PACKAGES PREVIOUSLY BID EXCEPT BID PACKAGE CES-15 BUILDING ELECTRICAL

1

Rebid- AD-1

FOWLER MCKINLEY ELEMENTARY SCHOOL

CES-01 EARTHWORK, SITE CONCRETE, & CMU – THIS BID PACKAGE PREVIOUSLY BID Section 01 57 23 Storm Water Pollution Prevention Plan
Section 03 11 01 Concrete Formwork Section 03 15 14 Drilled Anchors Section 03 20 00 Reinforcement Section 03 30 00 Cast-In-Place Concrete
Section 04 22 00 Concrete Masonry Units (CMU) Section 07 14 16 Fluid-Applied Waterproofing Section 07 92 00 Sealants
Section 08 70 00 Hardware
Section 08 70 00.01 Hardware schedule
Section 10 05 00 Miscellaneous Specialties (Stair Striping) Section 10 14 53 Road and Parking Signage
Section 10 75 00 Flagpoles Section 11 68 13 Play Equipment Section 12 93 13 Bicycle Racks
Section 31 00 00 Offsite Development Section 31 10 00 Site Clearing
Section 31 11 00 Clearing and Demolition Section 31 20 00 Earthwork
Section 31 22 22 Soil Materials
Section 31 23 33 Trench Excavation and Backfill Section 32 12 00 Pavement
Section 32 12 16 Soil Sterilization (Weed Control) Section 32 18 16 Playground Surfacing
Section 32 19 19 Ornamental Metal Section 32 31 13 Chain Link

CES-02 SITE UTILITIES PLUMBING: DOMESTIC, SANITARY, STORM, FIRE, & GAS - THIS BID PACKAGE PREVIOUSLY BID
Section 03 30 00 Cast in place Concrete (As applicable to storm, sewer, manholes, thrust blocks, etc.) Section 21 05 23 General Duty Valves for Fire Protection
Section 21 05 53 Identification for Fire Protection
Section 21 11 00 Facility Fire Suppression Water Service Piping Section 21 11 19 Fire Department Connections
Section 22 00 00 General Plumbing Provisions (Gas, Water, Fire Water, Storm, Sewer) Section 22 00 50 Plumbing (Gas, Water, Fire Water, Storm, Sewer)
Section 23 01 00 General Mechanical Provisions (As Applicable) Section 31 23 33 Trench Excavation and Backfill
Section 33 12 00 Water Utilities Section 33 30 00 Site Sewer Systems Section 33 40 00 Storm Drainage

2

Rebid- AD-1

CES-03 SITE ELECTRICAL & LOW VOLTAGE - THIS BID PACKAGE PREVIOUSLY BID Section 03 15 14 Drilled Anchors
Section 03 30 00 Cast in place Concrete (As applicable to slurry, and light pole bases, and grouting) Section 26 05 00 Common Work Results for Electrical
Section 26 05 26 Grounding
Section 26 05 53 Electrical Identification
Section 26 20 00 Low Voltage Electrical Transmission Section 27 00 00 Telecommunication Systems
Section 27 05 28 Communications Infrastructure System Section 27 10 00 Structured Cabling System

CES-04 LANDSCAPE - THIS BID PACKAGE PREVIOUSLY BID Section 03 15 14 Drilled Anchors
Section 32 84 00 Landscape Irrigation System Section 32 90 00 Landscape Construction

CES-05 BUILDING CONCRETE AND REBAR - THIS BID PACKAGE PREVIOUSLY BID Section 03 11 01 Concrete Formwork
Section 03 15 14 Drilled Anchors Section 03 20 00 Reinforcement Section 03 30 00 Cast-In-Place Concrete
Section 07 14 16 Fluid Applied Waterproofing Section 07 92 00 Sealants

CES-06 STRUCTURAL STEEL - THIS BID PACKAGE PREVIOUSLY BID Section 05 12 00 Steel and Fabrications
Section 05 30 00 Metal Deck

CES-07 SHEET METALS, MEMBRANE ROOFS, WALL AND ROOF PANEL SYSTEMS - THIS BID PACKAGE PREVIOUSLY BID
Section 07 21 00 Insulation (As applicable to roof systems) Section 07 40 00 Metal Panels
Section 07 54 19 Elastomeric Membrane Roofing Section 07 60 00 Sheet Metal
Section 07 92 00 Sealants

CES-08 FINISH CARPENTRY - THIS BID PACKAGE PREVIOUSLY BID Section 06 22 00 Millwork
Section 06 41 23 Modular Casework

CES-09 METAL FRAMING, PLASTER, AND GYPSUM BOARD - THIS BID PACKAGE PREVIOUSLY BID Section 03 15 14 Drilled Anchors
Section 07 21 00 Insulation (as applicable to all exterior wall rigid insulation) Section 09 22 16 Metal Framing
Section 09 24 00 Cement Plaster Section 09 29 00 Gypsum Board

3

Rebid- AD-1

CES-10 WALL MATERIALS AND ACOUSTICAL CEILINGS - THIS BID PACKAGE PREVIOUSLY BID Section 09 50 00 Acoustical Ceilings
Section 09 72 00 Wall Coverings
Section 10 26 00 Wall and Corner Guards

CES-11 PAINTING - THIS BID PACKAGE PREVIOUSLY BID Section 03 35 10 Polished Concrete Finishing
Section 07 92 00 Sealants
Section 09 67 23 Resinous Flooring Section 09 91 00 Painting

CES-12 GENERAL SPECIALTIES - THIS BID PACKAGE PREVIOUSLY BID Section 01 64 00 Owner Furnished Items
Section 01 74 19 Waste Management Section 03 15 14 Drilled Anchors Section 06 10 00 Rough Carpentry
Section 07 18 50 Vapor-Alkalinity Control Section 07 21 00 Insulation
Section 07 72 00 Roof Accessories Section 07 92 00 Sealants
Section 08 11 00 Metal Doors and Frames Section 08 15 13 Laminate-Faced Wood Doors Section 08 31 13 Access Doors and Frames Section 08 33 00 Coiling Doors
Section 08 41 00 Storefronts
Section 08 41 13 Folding Door System Section 08 56 59 Service Windows Section 08 70 00 Hardware
Section 08 70 00.1 Hardware Schedule Section 08 80 00 Glass
Section 09 30 00 Tile
Section 09 64 66 Resilient Wood Floor
Section 09 65 10 Resilient Base and Accessories Section 09 65 16 Resilient Sheet
Section 09 68 40 Carpet
Section 10 05 00 Miscellaneous Specialties (Building Plaque, Dimensional Letters, Cubicle Curtain System, Folding Partitions, Lock Box, Stair Stripping, Safe, Book Cart, Projection Screen)
Section 10 11 00 Visual Display Boards Section 10 14 00 Identifying Devices Section 10 21 13 Toilet Partitions Section 10 28 13 Toilet Accessories
Section 10 44 00 Fire Protection Specialties Section 10 51 13 Metal Lockers
Section 11 40 00.01 Food Service Equipment Section 11 61 43 Stage Curtains
Section 11 68 13 Play Equipment Section 14 42 00 Wheelchair Lifts

4

Rebid- AD-1

CES-13 FIRE SPRINKLERS - THIS BID PACKAGE PREVIOUSLY BID Section 03 15 14 Drilled Anchors
Section 07 92 00 Sealants
Section 21 05 17 Sleeves and Sleeve Seals for Fire-Suppression Piping Section 21 05 18 Escutcheons for Fire-Suppression Piping
Section 21 05 23 General-Duty Valves for Fire Protection Piping
Section 21 05 29 Hangers and Supports for Fire Suppression Piping and Equipment Section 21 05 48 Vibration & Seismic Controls for Fire-Suppression Piping & Equipment Section 21 05 53 Identification for Fire-Suppression Piping and Equipment
Section 21 11 00 Facility Fire-Suppression Water-Service Piping Section 21 11 19 Fire Department Connections
Section 21 13 13 Wet-Pipe Sprinkler Systems

CES-14 BUILDING PLUMBING and HVAC - THIS BID PACKAGE PREVIOUSLY BID Section 03 15 14 Drilled Anchors
Section 05 12 00 Steel and Fabrications (For downspouts/RWL’s and support attachments) Section 07 92 00 Sealants
Section 08 91 00 Louvers
Section 22 00 00 General Plumbing Provisions Section 22 00 50 Plumbing
Section 23 01 00 General Mechanical Provisions Section 23 01 00 General Mechanical Provisions Section 23 05 00 Common Work Results for HVAC
Section 23 05 13 Common Motor Requirements for HVAC Equipment Section 23 05 29 Hangers and Supports for HVAC Piping and Equipment
Section 23 05 48 Vibration and Seismic Controls for HVAC Piping and Equipment Section 23 05 53 Identification for HVAC Piping and Equipment
Section 23 05 93 Testing, Adjusting, and Balancing for HVAC Section 23 07 00 HVAC Insulation
Section 23 08 00 Commissioning of HVAC Section 23 17 10 Variable Frequency Drives Section 23 23 00 Refrigerant Piping
Section 23 31 13 Metal Ducts Section 23 31 16 Nonmetal Ducts
Section 23 33 00 Air Duct Accessories Section 23 34 23 HVAC Power Ventilators Section 23 34 33 Air Curtains
Section 23 38 13 Commercial Kitchen Hoods
Section 23 72 00 Air to Air Energy Recovery Equipment
Section 23 74 13 Package Outdoor Central Station Air Handling Units Section 23 74 33 Packaged Outdoor Heat and Cool Makeup Air Units Section 23 81 50 Variable Refrigerant Flow Air Conditioners
Section 25 50 00 Direct Digital Control and Energy Management Systems

5

Rebid- AD-1

CES-15 BUILDING ELECTRICAL Section 03 15 14 Drilled Anchors Section 07 92 00 Sealants
Section 10 05 00 Miscellaneous Specialties (Projector Support Panel) Section 26 05 00 Common Work Results for Electrical
Section 26 05 26 Grounding
Section 26 05 53 Electrical Identification
Section 26 20 00 Low Voltage Electrical Transmission Section 26 50 00 Lighting Fixtures
Section 27 00 00 Telecommunication Systems
Section 27 05 28 Communications Infrastructure System Section 27 10 00 Structured Cabling System
Section 27 20 10 Uninterruptible Power Supply Section 27 42 00 Classroom Audio-Visual Systems Section 27 53 13 Analog Synchronous Clocks
Section 27 70 00 Intercom Clock Public Address System Section 27 80 00 Video Surveillance
Section 28 31 00 Fire Alarm and Detection

CES-16 OFF SITE IMPROVEMENTS - THIS BID PACKAGE PREVIOUSLY BID
Section 32 84 00 Landscape Irrigation System (For Backflow Preventor and installation)

6

Rebid- AD-1

SUMMARY OF WORK FOR FOWLER MCKINLEY ELEMENTARY SCHOOL

PART 1 – GENERAL

As the Construction Manager (CM) for this project, David A Bush, Inc. (CM) reserves the right to publish Contractor Information Memos (CIM) prior to bid modifying the contract documents, as necessary. Please acknowledge all CIM on your proposal.

The following bidding instructions shall be adhered to by ALL BIDDERS and all bids shall include cost and time to incorporate all of the instructions noted below.

Please note this is a CM Multiple Prime project with all trades contracted to Clovis Unified School District as in a normal lump sum public works contract. All normal aspects of school construction will apply. All Prime Contracts shall be on the District’s form which is included in the Contract Documents. Failure to adhere to these contract requirements and instructions may be grounds for rejection of proposal.

1. All bidders must submit proposals on the form provided in the contract documents.
2. All prime contractors will be responsible for paying the non-refundable fees associated with the use of the Architects project CAD files. Fees, forms, and limitations can be found in the project specifications, 01 33 00.
3. In all cases where the plans and specifications are unclear or conflicting it shall be the responsibility of those submitting a bid to EITHER provide a proposal which includes the greater scope or most expensive option or choice at the time of bid OR provide a timely pre-bid RFI that addresses the question in detail.
4. All salvaged items shall be relocated per the contract documents direction and in the absence of direction to the Owners main yard.
5. Any and all miscellaneous or incidental materials or work normally provided by industry standard shall be provided by the Prime Contractor for their Bid Package.
6. Each Prime Contractor shall be responsible for the Safe performance of all of their work and adhere to all safety requirements required by the contract documents and by law.
7. Proposals will be evaluated first on their conformance to the contract documents as a complete bid. Proposals may be rejected as non-responsive if determined to be inconsistent with the bid documents requirements.
8. All Prime Contractors shall provide insurance in a form and limits as required by the contract documents. Prime Contractors shall require their Subcontractors of every tier to carry insurance in a form and limits as required by the contract documents.
9. If a tentative project construction schedule is published prior to bid, it shall become part of the contract documents.
10. If a RFI LOG and/or responses are published prior to bid it shall become part of the contract documents.
11. If a soils report is published prior to bid it shall become part of the contract documents with limitations as stated therein.
12. If a SWPPP is published prior to bid it shall become part of the project and each Prime Contractor, whose work is affected by the implementation shall be responsible for that cost.
13. Each Prime Contractor shall be responsible for locating roof jacks for their scope of work.
14. Any repairs (if required, due to damage by a Prime Contractor) to existing finishes such as plaster, sheetrock, paint, or concrete must be done between natural breaks such as corner to corner or score line to score line.

7

Rebid- AD-1

15. All Prime Contractors shall provide a contact cell phone number to the Construction Manager for contact.
16. Fire watch, if required, shall be provided by the Electrical Bid Package Prime Contractor.

1.01 SUMMARY

A.	General: Construction of BASE BID and Alternate portions of the work for this project, Clovis Unified School District, Elementary School #35, Increment 1 and 2. BASE BID and Alternate portions of the work is defined as all material, labor, equipment, and services necessary to do all work shown on the drawings and called for in the Specifications. The following specific trade requirements shall not be excluded from their proposal. Exclusion of any required scope specified shall be grounds for rejection. The scope of work for each trade shall remain as required by the Contract Documents. The specific list of scope herein shall be minimum and shall not limit the scope of that trade where required otherwise.

General Summary of the Project
The following information applies to all Bid Packages and shall be reviewed carefully for inclusion in each bid. Following are critical logistics related to the Project:

1. Hazardous Abatement is required if Hazardous Abatement Report is included in Contract Documents.
2. All work for the project will be performed during the hours of 7:00 a.m. to 3:30 p.m.
3. Submittals and material procurement shall begin immediately upon award or letter of intent from the CM.
4. Material procurement is critical and shall be diligently pursued to meet the contract schedule. 5. Prime Contractors shall review the project completely prior to bidding the work.
6. Coordination of work during the preconstruction period is equally as critical to resolving all issues prior to the start of work. Prime Contractor shall review the project, coordinate, and question any issues to allow resolution prior to the start of work.

In addition to the work noted in each package, the following will apply and become a part of the contract with each respective Prime Contractor.

Contract
All successful bidders will be required to enter into a Prime Contract Agreement with Clovis Unified School District.

Contractor Information Memos
All Addendums and Contractor Information Memo’s issued during bidding will be incorporated into the Contract Documents by reference. Submission of proposal shall acknowledge that Prime Contractor has reviewed and accepts these documents as part of the Contract Documents.

Submittals and Material Procurement
1. Submittals and material procurement shall begin immediately upon award or letter of intent from the District.
2. Material procurement is critical and shall be diligently pursued to meet the contract schedule.
3. Substitutions must be noted in each bid with all costs for the specified product included in the bid and the substitution cost noted separately.

8

Rebid- AD-1

Alternates

Additive Alternates for the work are as follows. Please provide a base bid for the project then list all alternates:
1. As shown in the plans and specifications and clarified in any Addendum.

Crew Sizes
Given the tight schedule for the project, it will be necessary to have larger than normal crew sizes to meet the schedule. This is inclusive of all trades. All Prime Contractors shall review the schedule and confirm that they can crew the project accordingly prior to submitting a bid. Include with each bid minimum and maximum crew sizes projected for the project.

Schedule
1. Prime Contractors shall review the project and schedule completely prior to bidding the work.
2. Prime Contractor will be required to provide a schedule and crew sizing showing how the work will be accomplished within the given time frame.

State Agency Requirements
1. Work under each contract shall comply with the Storm Water Pollution Prevention Plan (SWPPP) standards and as set forth in the Contract Documents.
2. All work under each contract shall comply with San Joaquin Air Pollution Control District standards. Provide dust control for own work.
3. All work shall comply with OSHA requirements.

Access Plan
If an access and site logistics plan is included in the Contract Documents, access and restriction shall be enforced as a part of the project. Please advise of any questions regarding the plan prior to bid.

Site Logistics, Work and Coordination (applies to each Prime Contractor):
1. Fingerprinting will berequired ascalledfor inthecontract documentswhen contact with students may occur.
2. Review and verify all existing conditions.
3. Power will be provided to within 100’-0” of all buildings. Each Prime will be required to provide all necessary temporary utility distribution from services provided.
4. All Prime Contractors shall attend coordination meetings and provide coordination drawings for underground and above ceiling work for work related to its Bid Package and scope for coordination of utilities, openings and other areas that require interface between trades. Coordinate alldrawings withthe drawings ofthis bidpackage. Noteconflictsandprovidepotential solutions to the CM for Architect review. Coordination and drawing approval must occur prior to excavation and/or overhead work. Prime Contractors shall attend a pre-installation meeting prior to the start of its work onsite. All Prime contractors shall be available for pre-installation meetings of other Bid Packages for coordination of related work.
5. Only company vehicles are allowed onsite. Personal vehicles will not be allowed on-site except for in identified locations shown in contract documents. Prime Contractor to make provisions for transport or tool distribution needs.
6. Lunch and breaks shall be at designated areas. No other areas will be allowed. 7. Protect all work, new and existing from damage until acceptance by owner.

9

Rebid- AD-1

8. Storage areas will be confined to the areas designated by CM. Staging areas around the building shall be coordinated with the CM.
9. Provide written request for information through the CM for layout information from related Bid Packages for all rough-in, embedded items, openings, and block-outs, etc.
10. Request and review all associated shop drawings for coordination and layout purposes prior to installation of related materials.
11. Furnish and install all trims, escutcheons, and sealant for own work abutting other materials. 12. Furnish and install protection of all roofing for own work.
13. Furnish and install all physical layout for own work.
14. There will be one wash out area as designated by the CM. Each Prime Contractor will be responsible for removal from the site of all debris and spoils generated by their scope. All spoils are to be moved to the dedicated location on site.
15. Coordinate all work with mechanical, plumbing, fire sprinkler, and electrical Bid Packages for shut down of services as needed. 48-hour notice is required prior to all shut down activities.
16. Review as-builts and underground locator survey and pothole utilities prior to starting work.
17. All Bid Packages are responsible for cleaning of the street, due to tracking out excess dirt or mud, should the preventative measures set in place in accordance with the SWPPP and Dust Control Plans fail to stop all spoils from escaping the site.
18. Secure all ladders and lifts each evening.
19. Provide caution tape and/or barriers for open area work and traffic control. 20. Protect all work, new and existing, from damage until acceptance by owner. 21. Provide water and shade for own crews.
22. Furnish access to roof for own work. Ladders are to be removed and secured at the end of each shift.
23. Provide fall protection for own work in own Bid Package unless specifically noted otherwise in each Bid Package.
24. Provide caution tape and/or barriers for open area work and traffic control. In accordance with all applicable Federal, State, Local, and District standards.
25. Provide layout and coordinate all demolition and ceiling removal required for your scope of work. 26. Coordinate extent of all demolition with related Prime Contractors prior to starting work.
27. Patch Fireproofing at all utilities for own work. 28. Protect all countertops as required by each trade.
29. Furnish and install fire stop for all required through penetrations for own work.
30. Core penetrations through walls as required for installation of own work and patch as noted on the plans.
31. Furnishand install allaccess doorsnecessarytoprovide accesstowork includedinyour respective scope of work.
32. Any deviation from the contract documents resulting in additional design will be at the cost of the Prime Contractor responsible for the additional design, as well as any associated cost for delay of schedule.
33. Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
34. Monthly payment applications will not be approved if as-builts are not up to date.
35. Adequate manpower is required by Prime Contractor to maintain the posted construction schedule.
36. Prime Contractor consents to execute District’s Prime Contractor Agreement as provided in the Contract documents, without modification.

10

Rebid- AD-1

37. Furnish daily cleanup of all debris generated by your respective scope of work. Prime Contractor must abide by the Waste Management Specification.
38. Water Hydrants are located in development around site. Prime Contractors are responsible for own water meters for construction water needs throughout the project. Methods of delivery and use of water for the work of each trade are the responsibility of the Prime contractor.
39. Coordinate all work to provide access to buildings for other trades as scheduled. Provide a breakout schedule of where and when work will be performed that has been coordinated with other activities in the schedule for other trades.
40. Furnish and install own floor protection (i.e., tarps, plastic, plywood, etc.)
41. Furnish and install covers at all holes in elevated decks created by your work in which debris may fall to the level below, per CAL OSHA regulations.
42. All construction equipment shall meet the requirements of the SJVAPCD ISR report (Air Impact Assessment – AIA) under the Construction Clean Fleet Summary. This shall include reporting requirement as defined within the Monitoring and Reporting Schedule within the ISR for this project.

General Items to be Provided by the CM 1. Toilet and hand wash facilities. 2. Temporary site fencing.

Drawings and Specifications
Drawings and general provisions of Contract, including General and Supplementary Conditions, and Division 00 Bidding and Contract Requirements, and Division 01 General Requirements, apply to the work of each Bid Package. The work under each Bid Package shall include the furnishing and installation of all material, equipment, procedures, methods, items, and labor as required to complete the work described in each Bid Package. The work shall be completed as shown on the Drawings and Specified in any and all applicable Specification Sections.

Completion of Work
The work of each Bid Package must be completed according to the construction schedule included with the Contract Documents.

Note: The term “provide” means to “furnish and install, complete and ready for the intended use.”

The work includes, but is not limited to, the items numerically listed in each Bid Package and in accordance with the applicable Drawings and Specification Section(s). Provide all work specified within each Bid Package and applicable Specification Section(s) with the exception of items listed as “work by others.”

While the ways, means, and methods will be the responsibility of the Prime Contractor, the items in the Bid Package Summary of Work are presented for construction clarifications.

General Items – All Prime Contractors
Furnish and install all work specifically required throughout the project documents to complete the work of this Prime Contractor that specifically includes, but is not limited to the following:

11

Rebid- AD-1

Specification Sections Division 01
Division 00

Refer to additional related specifications sections for work specifically included in this bid package noted below.

1.03 WORK UNDER OTHER CONTRACTS: A. General Requirements:
1. Work under separate contracts may occur throughout the duration of the project. The work being installed under separate contracts will occur adjacent to the Contract project site including offsite work.
2. Prime Contractor shall be responsible for coordinating access to and from the site throughout the duration of the project. Access points to and from the site may vary, based upon timing and duration of separate contracts.
3. Prime Contractor shall cooperate and coordinate all work under this Contract with all work under separate contracts.
4. Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
5. Prior to the installation of the Work, coordinate the work installed or to be installed by separate contracts relative to own work.
B. Separate Contracts by Owner: 1. Coordinate as awarded.
C. Separate Contracts by Others:
1. Adjacent Properties: Residential. D. Phasing:
1. Phasing is projected to be as shown on the Bid Schedule. However, the owner reserves the right to revise start times pending the review and award of bids.

1.04 BID PACKAGE'S DUTIES:
A. Except as specifically noted, provide, and pay for:
1. Labor, material, and equipment. All bid packages will be required to provide full time, qualified, knowledgeable supervision for their self-performed, and sub contracted labor. See General Conditions for Contractors specification 00 07 00, and specifics of Article 4 in this reference.
2. Tools, construction equipment and machinery
3. Other facilities and services necessary for proper execution and completion of Work. 4. Water: See Specification Section – TEMPORARY FACILITIES AND CONTROLS.
B. Pay legally required sales, consumer and use taxes. C. Give required notices.
D. Comply with codes, ordinances, rules, regulations, orders, and other legal requirements of public authorities which bear on performance of Work.
1. Prime Contractor shall certify in writing that no materials containing Asbestos are incorporated in the work, in accordance with the Asbestos Hazard Emergency Regulations Act.
E. Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.

12

Rebid- AD-1

1. Appropriate modifications to Contract Documents will adjust necessary changes.
2. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
F.	Enforce strict discipline and good order among employees. Do not employ on Work: 1. Unfit persons.
2. Persons not skilled in assigned task.
G. Provide material, equipment, and manpower to meet Construction Schedule provided in Contract Documents.
H. All Prime Contractors will be responsible for paying the non-refundable fees associated with the use of the Architects project CAD files. Fees, forms, and limitations can be found in the project specifications, 01 33 00.

1.05 BID PACKAGE USE OF PREMISES:
A. Confine operations at sites to areas permitted by: 1. Laws.
2. Ordinances. 3. Permits.
4. Contract Documents.
B. Do not unreasonably encumber site with materials or equipment. C. Do not load structure with weight that will endanger structure.
D. Assume full responsibility for protection and safekeeping of Prime Contractor's and Owner's material stored on premises and keep the site and building secure at all times.
E. Obtain and pay for use of additional storage or Work areas needed for operations. F.	Limit use of site for work and storage.

End of Section

13

Rebid- AD-1

BID PACKAGES CES-01, CES-02, CES-03, AND CES-04 PREVIOUSLY BID IN INCREMENT #1

CES-01 – EARTHWORK, SITE CONCRETE & CMU

Earthwork, Grading, Paving, Soil Treatment, Site Concrete, Rebar, Misc. Specialties (Stair Stripping), Flag Pole, CMU, Fencing, Playground Equipment, Site Furnishings.

Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections
Refer to additional related specifications sections for work specifically included in this bid package noted below.
Division 00 Division 01
Section 01 57 23 Storm Water Pollution Prevention Plan Section 03 11 01 Concrete Formwork
Section 03 15 14 Drilled Anchors Section 03 20 00 Reinforcement Section 03 30 00 Cast-In-Place Concrete
Section 04 22 00 Concrete Masonry Units (CMU) Section 07 14 16 Fluid-Applied Waterproofing Section 07 92 00 Sealants
Section 08 70 00 Hardware
Section 08 70 00.01 Hardware schedule
Section 10 05 00 Miscellaneous Specialties (Stair Striping) Section 10 14 53 Road and Parking Signage
Section 10 75 00 Flagpoles Section 11 68 13 Play Equipment Section 12 93 13 Bicycle Racks
Section 31 00 00 Offsite Development Section 31 10 00 Site Clearing
Section 31 11 00 Clearing and Demolition Section 31 20 00 Earthwork
Section 31 22 22 Soil Materials
Section 31 23 33 Trench Excavation and Backfill Section 32 12 00 Pavement
Section 32 12 16 Soil Sterilization (Weed Control) Section 32 18 16 Playground Surfacing
Section 32 19 19 Ornamental Metal Section 32 31 13 Chain Link

General Items

1. See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.

14

Rebid- AD-1

2. Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3. Provide all backfill of excavations to original sub-grade for work included in this bid package.
4. Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5. Provide daily cleanup to keep site clean and orderly.
6. Protect identified improvements to remain on civil plan sheets.
7. Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8. Prime Contractor is required to attend all coordination meetings as required by CM
9. Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10. Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11. Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12. Each bid package is responsible for dewatering as it pertains to their scope of work.
13. Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14. Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15. Monthly pay apps will not be approved if as-builts are not updated monthly.
16. Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17. Provide daily cleanup to keep site clean and orderly.
18. There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

19. All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

20. This contract is to provide temporary power for own work until such time as building temporary power is established.

15

Rebid- AD-1

Coordination with Other Trades

1. This Prime Contractor will be responsible for the initial setup of SWPPP BMP’s, as shown in the SWPPP plan drawings, including but not limited to, silt fencing, track outs and fiber rolls surrounding existing drain inlets.
2. Allow for twoadditional mobilizations for movement orrelocationof track outs as requiredduring construction.
3. Hold all turf areas down 2” at concrete walks and mow strips for turf, 1” at planters.
4. Location for trades to stockpile their spoils will be established with CM, and this CES-01 Prime Contractor.
5. Any survey requests require a minimum of 48-hour notice.
6. Coordinate dimensions with other related Prime Contractors of all equipment and housekeeping pads. Pad sizes shall be provided by other Prime Contractors and physically laid out and installed by this contract.
7. Coordinate installation of all sleeves for work passing through concrete work with respective Prime Contractors prior to excavation.
8. Electrical and site utility Prime Contractors shall furnish and install all concrete required for installation of thrust blocks, manholes, vaults, boxes, underground structures for work related to their contract. This contract shall furnish and install all other concrete shown including aprons mow strips and collars.
9. Install and coordinate block-outs at the site concrete to facilitate installation of fine grading by Earthwork Prime contractor and to protect concrete until fine grading is complete. Complete site concrete block-outs once fine grading is complete. Backfill and fine grade once block-outs have been poured.
10. Install and physically layout all embedded items (as provided by other Prime Contractors), holes, sleeves and block outs in concrete as shown in the contract documents, related shop drawings or provided written layout. Coordinate locations with related Prime Contractors prior to installation.
11. Provide layout drawings for all site concrete joints for approval prior to installation of site concrete.
12. Review as-builts prior to starting work.

Furnish and Install Items

DEMOLITION – SITE CLEARING

1.	Provide all cut, demolition, removal, and off-haul of all items noted to be removed as shown on contract documents.
2.	For site clearing and demolition follow recommendations as outlined within the soils report prepared by RMA Geoscience included in the project documents, in association with the contract documents.
3.	Investigate and remove the existing 3” steel post that stands approx. 100 feet south of Weldon, and 300 feet east of Fowler. It is believed to be an abandoned fence post.
4.	Make provisions to obtain water for own work. Dust control, excavations, backfills, compactions, etc. There are fire hydrants on two sides of the project. Make necessary arrangements with the city of Fresno to acquire a meter and pay for own water usages until such time that the site water has been installed and approved for site usage.

16

Rebid- AD-1

EARTHWORK AND GRADING

1.	Grade all earthwork to within +/-0.05’ from a planned elevation.
2.	Furnish and install all cut and fill necessary to perform work. Sand to be furnished and installed by the concrete bid package at the buildings only. All other materials shall be provided by this bid package.
3.	Clarification: This will be an “Import” project. This bid package will provide and incorporate approximately 35,000 cu yds of soil to the site. The material will be obtained from the CUSD Terry Bradly Ed Center ponding basin, located between DeWolf and Leonard Ave, at East Clinton Ave, where the soils has been previously tested for toxicity and suitability. Provide a per cubic yard Schedule of Values for these import soils, should additional soils, or a reduction of soils be required, other than the estimated 35,000 cu yds. Provide for All loading, hauling, street cleaning, dust controls, or traffic managements required will be provided under this CES-01 Earthwork and Grading bid package. Prior to starting this scope, there will be a required coordination meeting with	CES-01 contractor, CUSD, RMA, and Bush Construction to discuss plan, routing, and execution.
4.	All areas of planters, or turf are to have a minimum top layer of 1’ from existing native soil.

5.	Furnish and install all grading of the site on separate move-ins (as scheduled by the CM) to accommodate the site concrete and mow strips installation. Coordinate backfill and final fine grading activities to eliminate damage to new site concrete. Consult, and coordinate all elevations with the Landscape bid package where applicable.
6.	Furnish and install over excavations and building pads.
7.	Specific to building E, from grid lines H to N, and 9 to 12, the slab is 3’-7” higher than the overall building slab. The earthwork Prime Contractor will build this up as required, then cut the material back toallow adequatework space for thestructuralconcretebidpackage to install footings,pour

17

Rebid- AD-1

footings, build formwork, pour walls, strip, clean, and install fluid applied waterproofing. Once cured, the earthwork Prime Contractor will return to backfill and compact up against new walls and fine grade in preparation for elevated slab pour. See plan detail at end of this section for additional reference.
8.	Furnish and install temporary ag base roadway on site for construction use, including base at laydown area. After the threat of rain, towards the end of the project, the base will need to be scraped off, final gradingestablished per plans, andthebase is to be hauledoffunder this contract bid package. (See temporary access and yard plan for extent) CLARIFICATION: The depth of the ag base may vary but must be thick enough to hold up during the rains and site traffic. If repairs need to be made to maintain an adequate roadway, it will be performed under this bid package. Spray on dust control/soil stabilizer will also be a suitable alternative for the roadways but may require more frequent maintenance and product applications.
9.	Maintain and protect building pads to within tolerance, elevation, moisture, weed free and compaction until accepted/received by the concrete contractor as noted in the schedule.
10. Furnish and install all soil Sterilization as per the contract documents.
11. Furnish and install backfill of mow strips, walks, curb, curb & gutter, planter, and turf areas. 12. Furnish, install, and maintain traffic control for work included in this bid package.
13. Furnish and install engineered shoring at all locations as required.
14. For excavation, backfill and compaction efforts, follow recommendations as outlined within the soils report prepared by RMA Geoscience included in the project documents, in association with the contract documents.
15. Make provisions to obtain water for own work. Dust control, excavations, backfills, compactions, etc. There are fire hydrants on two sides of the project. Make necessary arrangements with the city of Fresno to acquire a meter and pay for own water usages until such time that the site water has been installed and approved for site usage.
16. Furnish and install all SWPPP items as outlined in the SWPPP plan and in spec section 01 50 00. CLARIFICATION: SWPPP installation is to be at and within the perimeter of the project site. All “Off Site” SWPPP to and along the west side of Fowler, and south of McKinley will be bid separately.
17. This package is responsible for setup and implementation of SWPPP plan. This package is also responsible for monitoring, documentation, reporting, teardown, and final cleanup of SWPPP items at completion of the project.

18

Rebid- AD-1

PAVING

1. Furnish and install all On Site paving base rock as identified on plans, including but not limited to under parking areas, basketball courts and drives. CLARIFICATION: All grading, paving associated with the Off-Site improvements will be furnished and installed with that bid package.
2. Furnish and install all compacted base rock as identified in contract documents. 3. Furnish and install parking bumpers and wheel stops where shown.
4. Furnish and install parking striping and/or accessible symbols as shown on contract documents. 5. Furnish and install all parking and road signage as indicated in contract documents, including
concrete at posts where indicated.

19

Rebid- AD-1

6. Furnish and install all asphalt paving and patch backs.
7. All parking areas are to be scheduled for two separate mobilizations, as the first 1 ½” lift will be placed, and the areas utilized for parking and staging during construction. At a later scheduled time in the project, this package will clean, prep, install tack, remobilize, and place the final finish section of the parking lots and entrance access points.
8. Furnish and install all slurry seal.
9. Furnish and install all play court striping as indicated in the contract documents.
10. Furnish and install pressure treated/redwood 2x4 header form at asphalt edge where unsupported unless noted otherwise.
11. Make provisions to obtain water for own work. Dust control, excavations, backfills, compactions, etc. There are fire hydrants on two sides of the project. Make necessary arrangements with the city of Fresno to acquire a meter and pay for own water usages until such time that the site water has been installed and approved for site usage.

SITE CONCRETE

1. Furnish and install all site concrete, including but not limited to, flatwork, curbs, curb and gutter, planter curbs, planter walls, gutters, valley gutters, mow strips, seat walls, all CMU footings (Site & Maintenance Yard), and amphitheater walls. Clarification of scope limits of work boundaries. See attached sketch at the end of this section.
2. Furnish and install all reinforcing as required for all site concrete per contract documents. Including but not limited to CMU footings, seat walls, fire lane, etc.
3. Furnish and install rebar caps per OSHA for all rebar associated with this contract’s scope of work, installed by the reinforcement contractor. Furnish and install concrete stake caps associated with this contract’s scope of work. Maintaining of Caps is the responsibility of this Prime Contractor. Safety walks at end of day required to ensure caps are in place, and any missing caps replaced.
4. Furnish any and all excavation necessary for work included in thiscontract.
5. Furnish and install all mow strips in site and around buildings, including at chain link, and ornamental fencing.
6. Furnish and install all sealants at all site concrete. This includes all sealant where site concrete abuts all buildings and structural concrete or CMU.
7. Furnish and install amphitheater steps, with reinforcing and stair nosing. (N1/SD/A302 & P11/SD/A302)
8. Install bollards (a.k.a. drinking fountain rails - furnished by others) in concrete footing. (J7/X/A531)
9. Furnish and install all parking and walkway accessible concrete ramps per contract documents. 10. Furnish and install all truncated domes.
11. Furnish and install all play access and play access perimeter curbs (B/SD/X107, C/SD/X107)
12. Install steel anchor plates, steel keeper plates and welded straps at thickened concrete walk at cane bolt locations. (N13/SD/A402) – Steel anchor plates, keeper plates and welded straps to be provided by fencing contractor F.O.B.
13. Install Flagpole in concrete base with reinforcing – see detail (A1/SD/A301)
14. Furnish and Install Concrete Monument Sign with reinforcing, V groove, chamfer, etc. Refer to details.
15. Furnish and install footings and sleeves/inserts for volleyball, tetherball, and basketball posts. 16. Furnish and install footings and sleeves/inserts for bicycle racks and any hand railing. Rails and
racks to be supplied by others. Note: Bike racks provided by this bid package, Bike Lockers are owner furnished, owner installed.
17. Furnish and install fibrous expansion joint, and sealant where required. 18. Install three sets of handrails at amphitheater.
19. Furnish and install concrete for all site housekeeping pads. Including but not limited to,

20

Rebid- AD-1

transformer, and electrical pads. Coordinate dimensions and layout with Prime Contractors.
20. Furnish and install concrete for all irrigation equipment/devices. Including, but not limited to, backflow pad, and booster pump pad. Coordinate dimensions and layout with site plumber and site landscape Prime Contractors.
21. Physically layout and install all block outs, openings, backing, etc. from written layout provided by other Prime Contractors for installation of their work.
22. This contract is to provide temporary power for own work until such time as building temporary power is established.
23. Make provisions to obtain water for own work. Dust control, excavations, backfills, compactions, etc. There are fire hydrants on two sides of the project. Make necessary arrangements with the city of Fresno to acquire a meter and pay for own water usages until such time that the site water has been installed and approved for site usage.
24. Install steel angles, and vent grating at portables, as supplied by Struct Steel bid package. See P/a101
25. CLARIFICATION: The perimeter sidewalks, including all drive access approaches are to be furnished and installed by the “Off-Site” bid package as highlighted site sketch below. Sidewalks will pour to the CMU, and chain link fence mow strip poured within this CES-01 bid package.
26. Furnish and install removable bollards for vehicular access per plans.

21

Rebid- AD-1

22

Rebid- AD-1

FENCING

1. Furnish and install all chain link fences, gates, and hardware, including those embedded or attached to CMU. Include new padlocks as noted in site drawings.
2. Furnish and install all backstop fencing including any horizontal backboards.
3. Furnish and install all ornamental iron fence, gates, and hardware, including those embedded or attached to CMU.
4. Provide Steel Anchor Plate, Steel Welded Straps and Steel Keeper plate F.O.B. jobsite (N13/SD/A402) for placement with site concrete.
5. Make provisions to obtain water for own work. Dust control, excavations, backfills, compactions, etc. There are fire hydrants on two sides of the project. Make necessary arrangements with the city of Fresno to acquire a meter and pay for own water usages until such time that the site water has been installed and approved for site usage.

CONCRETE MASONRY UNIT (CMU)

1. Provide and install all CMU block walls as identified in contract documents.

2. Furnish and install all rebar associated and shown to be installed in CMU, with exception of the rebar which is to be installed with the CMU footings.
3. Provide and install all smooth dowels, or other reinforcement and expansion components associated with CMU installation.
4. Coordinate and confirm reinforcement layout in footings with concrete contractor.

5. Make provisions to obtain water for own work. Dust control, excavations, backfills, compactions, etc. There are fire hydrants on two sides of the project. Make necessary arrangements with the city of Fresno to acquire a meter and pay for own water usages until such time that the site water has been installed and approved for site usage.

PLAY EQUIPMENT AND SITE FURNISHINGS

1. Bike lockers are Owner Furnished, Owner Installed.

2. Provide and install all playfield and court equipment as shown in contract documents. Including, but not limited to; basketball backboards (single & double), volleyball posts, volleyball nets, tether balls and tetherball posts, dugout benches etc. Furnish all sleeves as required for proper installation of equipment.
3. Provide and install EPDM wearing surface and SBR Rubber over concrete at play structure basins. 4. Provide and install loose engineered wood fiber at play structure basins.
5. Furnish and install bicycle racks per contract documents (six total). 6. Furnish and install flagpole per detail A1/SD/A301.
7. Make provisions to obtain water for own work. Dust control, excavations, backfills, compactions, etc. There are fire hydrants on two sides of the project. Make necessary arrangements with the city of Fresno to acquire a meter and pay for own water usages until such time that the site water has been installed and approved for site usage.
8. Furnish and install all drainage fabric, felt, and drainage matrix material, to storm drain pipe stub, that will be coordinated and provided by the site utilities contractor.

23

Rebid- AD-1

FOB Items

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.

1. Install all items embedded in concrete provided FOB Jobsite by other Prime Contractors from written layout provided by those Prime Contractors.
2. Install all bolt templates provided by other trades. 3. Install angle iron embeds at rolling gates.

End of Bid Package

24

Rebid- AD-1

BID PACKAGES CES-01, CES-02, CES-03, AND CES-04 PREVIOUSLY BID IN INCREMENT #1

CES-02 SITE UTILITIES PLUMBING: DOMESTIC, SANITARY, STORM, FIRE, & GAS
Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections Division 00
Division 01
Section 03 30 00 Cast in place Concrete (As applicable to storm, sewer, manholes, thrust blocks, etc.) Section 21 05 23 General Duty Valves for Fire Protection
Section 21 05 53 Identification for Fire Protection
Section 21 11 00 Facility Fire Suppression Water Service Piping Section 21 11 19 Fire Department Connections
Section 22 00 00 General Plumbing Provisions (Gas, Water, Fire Water, Storm, Sewer) Section 22 00 50 Plumbing (Gas, Water, Fire Water, Storm, Sewer)
Section 23 01 00 General Mechanical Provisions (As Applicable) Section 31 23 33 Trench Excavation and Backfill
Section 33 12 00 Water Utilities Section 33 30 00 Site Sewer Systems Section 33 40 00 Storm Drainage

Refer to additional related specifications sections for work specifically included in this bid package noted below.

General Items
1. See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2. Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3. Provide all backfill of excavations to original sub-grade for work included in this bid package.
4. Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5. Provide daily cleanup to keep site clean and orderly.
6. Protect identified improvements to remain on civil plan sheets.
7. Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8. Prime Contractor is required to attend all coordination meetings as required by CM.
9. Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.

25

Rebid- AD-1

10. Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11. Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12. Each bid package is responsible for dewatering as it pertains to their scope of work.
13. Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14. Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15. Monthly pay apps will not be approved if as-builts are not updated monthly.
16. Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17. Provide daily cleanup to keep site clean and orderly.
18. There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.
19. All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.
20. This contract is to provide temporary power for own work until such time as building temporary power is established.

Coordination with Other Trades
1. Provide coordination drawings for underground work related to this bid package. Coordinate all drawings(Plumbing, Electrical, site, Off Site, andLandscape)with the drawings ofthis bidpackage. Noteconflictsandprovide potential solutions tothe architect for review. Coordinationmust occur prior to excavation and/or installation of the work. Attend all coordination meetings required to coordinate all underground.
2. Coordinate routing of underground utilities miss foundations.
3. Coordinate alignment of all utilities between plumbing and civil drawings prior to excavation. 4. All underground utilities (Gas/DCW/Fire) are to be a minimum of 3’ below finish grade.

Furnish and Install Items
1. Furnish and install all site utilities and fixtures complete. Water, Fire, Sewer, Storm.
2. Make provisions to obtain water for own work. Dust control, excavations, backfills, compactions, etc. There are fire hydrants on two sides of the project. Make necessary arrangements with the city of Fresno to acquire a meter and pay for own water usages until such time that the site water has been installed and approved for site usage.

26

Rebid- AD-1

3. Provide all backfill of excavations to original subgrade for work included in this bid package. 4. Stockpile extra spoils from excavations in location to be determined by CM.
5. Furnish and install all attachment of all equipment related to this scope of work. 6. Furnish and install all excavation for own work.
7. Furnish and install all concrete required for installation of thrust blocks, manholes, vaults, boxes, underground structures, mow strips and collars for work related to this bid package.
8. Furnish and install asphalt patch back related to own work as required. 9. Adjust all utility boxes to finish grade.
10. Clean and disinfect all site piping required for this project to subsequent point of connection. 11. Furnish and install all piping required to accommodate new work.
12. Furnish, install, and maintain traffic control for work included in this package.
13. Furnish and install all site fire water, sewer systems, storm systems, domestic water & gas.
14. Furnish and install all dry wells, drainage, water and drinking fountains. Clarification: see G/SD/X102 for dry well at ball fields.
15. Furnish and install all site trench drains and piping (If shown)
16. Furnishandinstall allsite Fire, allfire line piping, andstubinto buildingper plansto above finished floor with a capped flanged fitting, as the POC for the fire sprinkler contractor. Furnish and install all site check valves, Christy vaults, PIV’s, FDC’s, Hydrants, Backflow Preventors, and Bollards per plans at fire equipment per plans. CLARIFICATION: See note # 6 on site plans, and J7/SD/A302
17. Furnish and install all site domestic water complete from POC at back flow preventors, check valves, SOV’s, etc. to within 5’ of buildings.
18. F&I complete storm to within 5’.
19. F&I complete gas to within 5’ of where pressure regulators are shown for each building.

FOB Items
1. None

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.
1.	Not Applicable.

End of Bid package

27

Rebid- AD-1

BID PACKAGES CES-01, CES-02, CES-03, AND CES-04 PREVIOUSLY BID IN INCREMENT #1

CES-03  SITE ELECTRICAL & LOW VOLTAGE
Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections
Refer to additional related specifications sections for work specifically included in this bid package noted below.

Division 00 Division 01
Section 03 15 14 Drilled Anchors

Section 03 30 00 Cast in place Concrete (As applicable to slurry, and light pole bases, and grouting) Section 26 05 00 Common Work Results for Electrical
Section 26 05 26 Grounding

Section 26 05 53 Electrical Identification

Section 26 20 00 Low Voltage Electrical Transmission Section 27 00 00 Telecommunication Systems
Section 27 05 28 Communications Infrastructure System Section 27 10 00 Structured Cabling System

General Items
1. See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2. Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3. Provide all backfill of excavations to original sub-grade for work included in this bid package.
4. Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5. Provide daily cleanup to keep site clean and orderly.
6. Protect identified improvements to remain on civil plan sheets.
7. Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8. Prime Contractor is required to attend all coordination meetings as required by CM.
9. Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10. Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.

28

Rebid- AD-1

11. Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12. Each bid package is responsible for dewatering as it pertains to their scope of work.
13. Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14. Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15. Monthly pay apps will not be approved if as-builts are not updated monthly.
16. Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17. Provide daily cleanup to keep site clean and orderly.
18. There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.
19. All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.
20. This contract is to provide temporary power for own work until such time as building temporary power is established.

Coordination with Other Trades
1.	Provide coordination drawings for underground work for work related to this bid package. Coordination must occur prior to excavation and/or installation of the work. Attend all coordination meetings required to coordinate all underground.
2.	Coordinate all work to provide access to buildings for other trades as scheduled. Provide an underground utility schedule of where and when piping operations will be performed.
3.	Coordinate location of UG utilities to be out of angle of repose of foundations.
4.	Poured in place housekeeping and equipment pads to be supplied by concrete team. Precast housekeeping and equipment pads to be supplied and installed by this package
5.	Review as-builts and pothole existing utilities prior to starting work.
6.	Verify continuity of electrical and low voltage conduits for work in this contract.
7.	Provide shop drawings for equipment layout in electrical rooms & yards to confirm that dimensions are adequate prior to rough in and pouring of footings and curbs.
8.	Coordinate all underground utilities to miss foundation.
9.	Provide Safe off of all electrical equipment as required for trade work.
10.	Provide an underground utility schedule of where and when piping operations will be Installed.

Furnish and Install Items

CLARIFICATION:
Several pieces of equipment were added in the electrical drawing revisions that were included in (Increment #1 Addendum # 3), and are not to be furnished or installed within this bid package. The conduit, Christy’s/ underground pathways for these items are to be included in this bid package. Mini Substation, PV disconnect, Transformer, IDF, and back stop PA will all be provided and installed with the

29

Rebid- AD-1

Inc 2 electrical bid package, with the exception of the Owner Supplied Switchgear, that will be installed under this CES-03 package, and previously addressed.

1.	Furnishand install all site utilities conduit and infrastructure complete for allPower, Data, Fire Alarm, Security, Irrigation line voltage (pumps/time clocks), and EMS. See SD/M101 for EMS site conduit clarification. All conduits are to be brought to within 10’ of the buildings. All stopping points are to be flagged, swing tied if possible, and recorded on the As-Builts for Increment 2 continuation. Conduits are to stop within 5’ of pumps and time clocks if specific layout cannot be determined during the time of installation., and 5’ for fire sprinkler components where alarm is required. CLARIFICATION:This includes power conduit for “Coach control switches”, as described in the Landscape plans. Building electrical contractor will provide and install the housing, wiring, receptacle.
2.	Site lighting conduit is to stop approximately 5’ from the flagpole, all light pole bases, and first light of radiused (T-2’s) at the concrete monument wall. Clarifications: 1. The in-ground T-2 lighting was removed from the site at the flag pole area. Disregard reference. 2. (Increment #1 Addendum 3) added lights at the CMU service yard. Install conduits to the footing alignment where each light is shown. Inc 2 electrician will coordinate and install the continuation conduit up in CMU.
3.	Make provisions to obtain water for own work. Dust control, excavations, backfills, compactions, etc. There are fire hydrants on two sides of the project. Make necessary arrangements with the city of Fresno to acquire a meter and pay for own water usages until such time that the site water has been installed and approved for site usage.
4.	Furnish and install physical layouts for all deepened foundations at utilities prior to excavation.
5.	All excavation spoils to be deposited at one location on site as determined by CM.
6.	Furnish and install all sleeves for work passing through masonry and concrete work. Coordinate with respective bid packages.
7.	Provide all backfill of excavations to original subgrade for work included in this bid package. 8.	Furnish and install fire stopping and fire caulking of own penetrations for own work.
9.	Furnish and install pull strings/rope in all empty or future conduits.
10.	Furnish and install all concrete required for installation of vaults, boxes, underground structures for work related to this bid package.
11.	Furnish and install all site conduit required for Owner furnished equipment hook up as required.
12.	Furnish and install all rough-in for all equipment of other bid packages as required by the related specification sections and drawings. Connect and or stub as described.
13.	Furnish and install all conduit and sleeves for future low voltage and telecommunications wiring. Install fire stopping as required.
14.	Furnish and install all attachment of all equipment related to this scope of work. 15.	Furnish and install all supports and bracing required for electrical work.
16.	Furnish and install all identification and lettering called for in the contract documents related to the work of this bid package.
17.	Adjust all electrical and low voltage boxes in new landscape and concrete areas as needed. 18.	Furnish and install all physical layout for your own work.
19.	Furnishand install all site conduits, including vaults and boxes for allelectrical andlow voltage systems.
20.	Provide all power/Breaker testing for own work.
21.	Chase and prove all electrical site pathways as required to complete work.

30

Rebid- AD-1

22.	Furnish and install electrical equipment, conduit, pre cast pads required for the utility provider (Rule 16 and similar for site power connections). Switchgear will be Owner Furnished, Contractor Installed.
23.	Furnish and install all site rough-in conduit for all equipment of other trade as required by the related specification sections and drawings. Connect and or stub as described.
24.	Furnish and install all site lighting conduits including vaults / boxes. Bring all conduits to withing 5’ of light pole locations and buildings. Cap and flag each end, (swing tie if possible) for subsequent connection by the building electrical contractor. Coordinate the location of the conduit at the building end to the point of entry established by the building electrician.
25.	Furnish and install disconnects and associated supports as applicable to increment 1.
26.	Furnish and install sealant system as required to provide watertight condition at devices mounted on masonry units.
27.	Furnish and install PG&E, ATT, and Comcast conduit for onsite as shown on the drawings. 28.	Furnish and install all colored concrete cap over all required duct banks.
29.	Furnish and install conduits for all landscape equipment such as controllers, pumps, etc. as required by the landscape drawings.
30.	Furnish and install all backfill of excavations to original subgrade for work included in this contract.
31.	Provide Dust Control for own work.
32.	This contract will adhere to guidelines for all work per the requirements of the Dust Control Plan and SWPPP Plan.
33.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this Project.
34.	Electrical Prime Contractor responsible for any and all patch back and finishing for any trenching made in roadways, for work performed under this bid package.
35.	All excavation spoils to be deposited at one location on site as determined by CM.
36.	Furnish and install all sleeves for work passing through masonry and concrete work. Coordinate with respective bid packages.
37.	Provide all backfill of excavations to original subgrade for work included in this bid package. 38.	Furnish and install drilling of holes for work performed in this bid package.
39.	Furnish and install pull strings/rope in all empty or future conduits.
40.	Furnish and install all concrete required for installation of vaults, boxes, underground structures for work related to this bid package.
41.	Furnish and install all conduit and sleeves for future low voltage and telecommunications wiring. Install fire stopping as required.
42.	Furnish and install all attachment of all equipment related to this scope of work.
43.	Furnish and install all identification and lettering called for in the contract documents related to the work of this bid package.
44.	Furnish and install all physical layout for your own work. Same as 18
45.	This contract shall be responsible for holes at metal deck for installation of hanger wires for own work.

For Rule 16, and associated PG&E work.

1. This contract will provide all PG&E electrical requirements as outlined for connection to/for PG&E Rule 16 work in conjunction with the project drawings. This Prime Contractor will run all conduits,

31

Rebid- AD-1

proof, and mandrel all conduits for the new PG&E feeders from the POC shown in the attached marked up site plan for reference, then to the transformer, then to the Switchgear.
2. Coordinate all meetings with PG&E, obtain permits, and provide all services required to facilitate and install the main power distribution on to the site.
3. Furnish and install all work relating to PG&E rule drawings, off-site plans of existing conduit pathway, to connect to new conduit and vault on site, and leading to the switchgear.
4. Furnish and install all excavations, and patch back to road crossing. CLARIFICATION: Millard street is not currently paved, nor have the sidewalks been installed on either side. The curbs and gutters are already installed. If damaged during installation, these repairs would also be included in this package responsibility.

FOB Items

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.
End of Bid package

32

Rebid- AD-1

BID PACKAGES CES-01, CES-02, CES-03, AND CES-04 PREVIOUSLY BID IN INCREMENT #1

CES-04 LANDSCAPE
Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections Division 00
Division 01
Section 03 15 14 Drilled Anchors

Section 32 84 00 Landscape Irrigation System Section 32 90 00 Landscape Construction

Refer to additional related specifications sections for work specifically included in this bid package noted below.

General Items
1.	See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2.	Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3.	Provide all backfill of excavations to original sub-grade for work included in this bid package.
4.	Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5.	Provide daily cleanup to keep site clean and orderly.
6.	Protect identified improvements to remain on civil plan sheets.
7.	Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8.	Prime Contractor is required to attend all coordination meetings as required by CM.
9.	Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10.	Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11.	Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12.	Each bid package is responsible for dewatering as it pertains to their scope of work.
13.	Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.

33

Rebid- AD-1

14.	Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15.	Monthly pay apps will not be approved if as-builts are not updated monthly.
16.	Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17.	Provide daily cleanup to keep site clean and orderly.
18.	There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.
19.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.
20.	This contract is to provide temporary power for own work until such time as building temporary power is established.

Coordination with Other Trades
1. Coordinate sleeve installations with site concrete.
2. Coordinate pump location, house pad, layout, and elevation with electrical, plumbing, and concrete packages.
3. Coordinate all valve boxes, quick connects, with concrete, planters, and elevations.

Furnish and Install Items
1. Furnish and install all irrigation and landscaping complete. Connect to existing power, wiring and controls where required at existing landscape areas.
2. Make provisions to obtain water for own work. Dust control, excavations, backfills, compactions, etc. There are fire hydrants on two sides of the project. Make necessary arrangements with the city of Fresno to acquire a meter and pay for own water usages until such time that the site water has been installed and approved for site usage.
3. Provide and install new irrigation, controls, wiring, pumps, premanufactured concrete pads, etc. for own work. Main power supply and connection to pumps or equipment (Line voltage), will be supplied by the electrical Prime Contractor.
4. Furnish and install all thrust blocks for own work. 5. Furnish and install grading and top soil.
6. Provide water test of turf and planter areas prior to planting to confirm proper drainage and coverage.
7. Furnish and install all irrigation sleeves. 8. Furnish and install backfill all planters.
9. Furnish and install all fine grading of planter areas prior to planting.
10. Furnish and install all irrigation pipe system from POC at main backflow preventor, installed by the site plumbing Prime Contractor per spec.
11. Furnishandinstall irrigationpump(s), controls,secondary backflow preventerif applicable, valves, etc. associated with the irrigation system, complete ready for electrical connection where applicable.
12. Furnish and install all new irrigation and drip irrigation complete.

34

Rebid- AD-1

13. Furnish and install all new planter dressings, bark, mulches, and all landscape materials. CLARIFICATION: This Landscape package will be responsible to supply and install all materials as noted within the landscape plans, including screened infield top soil materials, DG, sod, Stolens, Mulches, etc. unless specifically noted otherwise.
14. Furnish and install all baseball bases and pitching blocks per plans.

15. Furnish and provide weed control and clean up of grasses/weeds for the project site, and associated off site locations for the duration of the project, until such time that the district takes possession and acceptance of the new facility.
16. This Landscape contractor is responsible for all the final elevations of Turf, infields, including pitchers mounds, DG, planters, tree wells, and mulches. Coordinate subgrades with Earthwork Contractor, as they will be responsible for the subgrades.
17. Furnish and install all coaches boxes/switches as shown in the Landscape plans, including valves, conduit, control wiring and connections. Coordinate locations with the Site electrical contractor for AC power conduit. Building electrical contractor to install wiring, housing for controller, and receptacle.

FOB Items
1. Provide remote controllers and extra materials to the district through close out procedures with CM Construction Management process.

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.

End of Bid package

35

Rebid- AD-1

THIS BID PACKAGE PREVIOUSLY BID IN INCREMENT #2

CES-05 BUILDING CONCRETE AND REBAR

Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Division 00 Division 01
Section 03 11 01 Concrete Formwork Section 03 15 14 Drilled Anchors Section 03 20 00 Reinforcement Section 03 30 00 Cast-In-Place Concrete
Section 07 14 16 Fluid Applied Waterproofing Section 07 92 00 Sealants
Appendix “B” Interior Color Schedule Plus Drawings Appendix “C” Exterior Color Schedule
Geotechnical Engineering Report

General Items

1.	See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2.	Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3.	Provide all backfill of excavations to original sub-grade for work included in this bid package.
4.	Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5.	Provide daily cleanup to keep site clean and orderly.
6.	Protect identified improvements to remain on civil plan sheets.
7.	Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8.	Prime Contractor is required to attend all coordination meetings as required by CM
9.	Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10.	Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11.	Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.

36

Rebid- AD-1

12.	Each bid package is responsible for dewatering as it pertains to their scope of work.
13.	Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14.	Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15.	Monthly pay apps will not be approved if as-builts are not updated monthly.
16.	Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17.	There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

18.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

19.	This contract is to provide temporary power for own work until such time as building temporary power is established.
20.	SUBMITTALS: Provide Rebar reinforcement shop drawings for all footings, curbs, and building columns for buildings E and A will be the first order of business, and due within 30 days of NTP. Bar needs to be pulled for initial tagging at the earliest lab availability following approved review, to expedite production. Following in order will be buildings B, C, D, and K, no later than one week each, after the initial 30 day start for buildings E and A. All subsequent building reinforcement steel drawings are due for submittal no later than 30 days of their scheduled start, noted above.
21.	Furnish clean up daily and off-haul of all debris generated by this contract to disposal bins provided under CES-12. Prime Contractor must abide by the Waste Management specification.

Coordination with Other Trades

1.	Location for trades to stockpile their spoils will be established with David A. Bush, and the CES-01 Bid Package contractor.
2.	Any survey requests require a minimum of 48-hour notice.
3.	Coordinate dimensions with other related contractors of all equipment and housekeeping pads. Pad sizes shall be provided by other contractors and physically laid out and installed by this contract.
4.	Coordinate installation of all sleeves for work passing through concrete work with respective contractors prior to excavation.
5.	Install and physically layout all embedded items (as provided by other contractors), holes, sleeves and block outs in concrete as shown in the contract documents, related shop drawings or provided written layout. Coordinate locations with related contractors prior to installation.
6.	Provide layout drawings for all slab concrete joints for approval prior to installation of site concrete.
7.	Review as-builts prior to starting work.
8.	This bid package will received all building pads at +/-0.05’and will be responsible for all cut and fill necessary to complete the work of this bid package.
9.	Maintain building slab subgrade moisture content per soils report once building pad is received from the earthwork bid package.
10.	Coordinate all work to provide access to buildings for other trades as scheduled.

37

Rebid- AD-1

11.	Coordinate the location of depressions, block outs, slopes and drains prior to pour. 12.	Coordinate concrete curbs relative to framing and door jambs prior to pour.
13.	Review as-builts and underground locator survey and pothole utilities prior to starting work. 14.	Work must be coordinated to accommodate staff and other trade access.
15.	Once all steel embed templates and bolts have been formed and set in place by this bid package, the contractor will schedule with the surveyor to survey the templates for accuracy. Modification and fine tuning to be done under the building concrete bid package, prior to pouring footings. Once footings have been poured, and this bid package has stripped forms and templates, the concrete contractor will set a minimum of one leveling nut to the planned elevation at each column or tube frame.
16.	Clean all footings, furnish dewatering and protection of all embed bolts until turned over to structural steel for erection.
17.	Set a minimum of one leveling nut, to the planned finish elevation, at each steel column location, interior and exterior.
18.	For reference, the following note is in CES-01, Increment 1 for the earthwork contractor, and the coordination with this CES-05 Structural building Concrete package. Specific to building E, from grid lines H to N, and 9 to 12, the slab is 3’-7” higher than the overall building slab. The earthwork contractor will build this up as required, then cut the material back to allow adequate work space for the structural concrete Bid Package to build footings. The structural concrete contractor will pour footings, build formwork, pour walls, strip, clean, and install fluid applied waterproofing. Once cured, the earthwork contractor will return to backfill and compact up against new walls, and fine grade in preparation for elevated slab pour. See plan detail below for additional reference.

38

Rebid- AD-1

39

Rebid- AD-1

Furnish and Install Items

1. Furnish and install all building concrete. Buildings A, B, C, D, E, K, and Portable building P with associated access, vents, 2-inch rat slab, stem walls and piers. Furnish and install ADA ramps, stairs, and stem walls associated with Building E. Flatwork surrounding these areas to be provided with the site concrete package CES-01, in Increment 1.
2. Furnish and install all curbs as identified for typical restrooms and kitchen areas, in addition to those shown on the plans. See details N7 and J7 on X/A101.
3. Furnish and install all rebar complete. including ties to existing slab, footings, or stem walls where applicable.
4. Furnish and install all surface saw cutting and sealer per the contract documents.
5. Furnish and install all expansion joints and sealant complete required by the contract documents in concrete.
6. Furnish and install all fluid applied waterproofing at formed walls for elevated slab. Bldg. E
7. Furnish and install all sand, gravel, crushed rock, etc. as detailed at building concrete. All other fill material shall be furnished and installed by the earthwork bid package.
8. Furnish and install any and all excavations and backfill of excavations at all foundations, to the required grade. Excavations to includelayout and digging of allbuilding and CMU footings, spread footings, grade beams, etc.
9. Physically layout and install all blockouts, openings, etc.… in concrete from written layout provided by other bid packages for installation of their work.
10. Protect all slab blockouts for other trades working in the area.
11. Furnish and install all building anchor bolts. Coordinate layout with respective primes.
12. Furnish installation of all steel column templates, including bolts, as provided by Steel Contractor. Once installed, schedule a request for survey to have the bolt layouts confirmed with the steel shop drawings layout. Fine tune and adjust as necessary prior to pour.
13. Furnish & install all floor prep for floors out of tolerance poured by this contract, except at LVT. 14. Furnish & install all concrete equipment and housekeeping pads within the buildings.
15. All minordepressions for tile(if applicable) and slopes to drain shall beperformed by this Concrete Bid package.
16. Furnish and install all patch and infill at slab as required for all work.
17. Furnish and install redwood nailers in concrete curbs the attachment of finishes as detailed. 18. Furnish and install all drilling of holes for work performed in this contract.
19. Furnish & install all building concrete sealant. Exterior walk sealant to be provided and installed by CES-01, Inc 1 package.
20. Furnish and install all grouting under handrails and at sleeves within the buildings.
21. Furnish and install steel channels for knee wall supports, as provided by the steel bid package, and coordinate layout and quantities with the framing bid package.
22. Provide for architect and engineer’s review, saw cutting and expansion joint plan, prior to pouring any interior building concrete.
23. At all exposed concrete floors, pay special attention to obtain a uniform finish, and flatness per specifications. Areasfoundto beoutof tolerancemaybe requiredtoberemoved intheir entirety/ or from joint to joint, at the owner/Architect’s discretion.
24. Provide and install rebar and concrete at the stairs and landings to the second floor of Building E. 25. Furnish and install rebar caps per OSHA for all rebar associated with this contract’s scope of
work, installed by the reinforcement contractor. Furnish and install concrete stake caps associated with this contract’s scope of work. Maintaining of Caps is the responsibility of this Prime Contractor. Safety walks at end of day required to ensure caps are in place, and any

40

Rebid- AD-1

missing caps replaced.

FOB Items

1. None.

Installation of FOB Items

Note. Unload, inventory, store and notify of deficiencies for all items delivered to the jobsite FOB, to be installed by this bid package.

1. Physically layout and install all items embedded in concrete within the building and structural footings. (i.e. plates, angles, non-bolted tube steel, rails, sleeves, pipe rail, handrails, stair nosing, etc.…) as provided FOB jobsite by other bid packages from written layout provided by those bid packages. Install and grout all items installed in sleeves.
2. Install and remove when complete all bolt templates provided by other bid packages except for sill plate bolts.
3.	Furnish and install templates from layout provided by the framing and steel bid package.

41

Rebid- AD-1

THIS BID PACKAGE PREVIOUSLY BID IN INCREMENT #2

CES-06  STRUCTURAL STEEL
Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections
Refer to additional related specifications sections for work specifically included in this bid package noted below.

Division 00 Division 01
Section 05 12 00 Steel and Fabrications Section 05 30 00 Metal Deck
Appendix “B” Interior Color Schedule Plus Drawings Appendix “C” Exterior Color Schedule
Geotechnical Engineering Report

General Items
1. See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2. Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3. Provide all backfill of excavations to original sub-grade for work included in this bid package.
4. Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5. Provide daily cleanup to keep site clean and orderly.
6. Protect identified improvements to remain on civil plan sheets.
7. Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8. Prime Contractor is required to attend all coordination meetings as required by CM.
9. Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10. Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11. Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12. Each bid package is responsible for dewatering as it pertains to their scope of work.

42

Rebid- AD-1

13. Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14. Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15. Monthly pay apps will not be approved if as-builts are not updated monthly.
16. Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17. There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

18. All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

19. This contract is to provide temporary power for own work until such time as building temporary power is established.
20. SUBMITTALS: Provide erection, bolt templates and shop drawings for all structural steel columns. Buildings are all to be submitted separately, site FOB items can be as one. Anchor bolt drawings, along with actual templates with the anchor bolts installed, for buildings E and A will be the first order of business, and due within 30 days of NTP. Following in order will be buildings B, C, D, and K, no later than one week each, after the initial 30 day start for buildings E and A. All subsequent building steel drawings are due for submittal no later than 30 days of their scheduled start.
21. Furnish clean up daily and off-haul of all debris generated by this contract to disposal bins provided under CES-12. Prime Contractor must abide by the Waste Management specification.

Coordination with Other Trades
1.	Provide coordination drawings for work related to this bid package. Coordinate all drawings with the drawings of other bid packages. Note conflicts and provide potential solutions to CM for review. Coordination must occur prior to installation of work. A representative from your company must be in attendance at all coordination meetings.
2.	Field measure all guardrails and handrails.
3.	Provide erection and shop drawings for all handrails, stair rails and guard rails.
4.	All steel shall be detailed, ordered, fabricated, and erected per the project schedule.
5.        All miscellaneous iron shallbe detailed, ordered,fabricated, anderected per the project schedule. 6.        Provide erection, bolt templates and shop drawings for all structural steel columns. Buildings are all to be submitted separately, site FOB items can be as one. Anchor bolt drawings, along with actual templates with the anchor bolts installed, for buildings E and A will be the first order of business, and due within 30 days of NTP. Following in order will be buildings B, C, D, and K, no
later than one week each, after the initial 30 day start for buildings E and A. All subsequent building steel drawings are due for submittal no later than 30 days of their scheduled start.
7.	Provide shop drawings for all steel fabrications. 8.	Coordinate structural steel embeds.
9.	Coordinate steel gate sizes with plans and CMU contractor for embed components/frame. Install frame in conjunction with the CMU installation process.
10.        Request and Receive layout (prior to detailing and fabrication) from other Prime Contractors for all items which require holes, openings, reinforcing and bracing related to this Prime Contractor’s

43

Rebid- AD-1

scope of work, including but not limited to, bolt holes for attachments, roof openings, HVAC supports, reinforcing steel, etc. Allow 10 days for return of dimensions. Provide coordination drawings for dimension mark ups by other Prime Contractors.
11.	Provide a written crane access plan, laydown areas, and movement schedule for coordination with other Prime Contractors.
12.	Coordinate vent frames and grating with plans for Portables, and see P/A101 for additional information.

Furnish and Install Items
1.	Furnish and install all steel and fabrications, metal deck, and railing systems complete per plans and specifications.
2.	Furnish and install all structural steel, miscellaneous iron, metal decking and closures at buildings and canopies, tube steel, channel, and outriggers.
3.	Furnish and install all steel stairs, and associated support and anchorage. See Building E, specifically E/A901.
4.	Physicallylayoutand installall block outs,openings, reinforcing, bracingand holesinsteel &metal deck from written layout provided by other Prime Contractors.
5.	Furnish and install deck supports, steel beams, angles, “C” channel reinforcing at all deck penetrations and openings shown on the architectural, mechanical, electrical, plumbing, structural drawings & coordination drawings.
6.	Furnish and install all deck support plates required on parallel to deck spanning beams.
7.	Furnish and install all metal deck closures, profile closures, closures strips, penetration closures, and neoprene closures at metal deck, exterior canopies, and head of walls. Framing Prime Contractor to furnish and install closures where closure mounts to deck and stud with no concrete.
8.        Furnishand install paintedmarkings as requiredto identify yield lines on brace framesand similar. 9.        Furnish and install all primer touch up at welding, structural steel, nuts and bolts, and metal deck. 10.        Set leveling nuts at anchor bolts to the proper elevation for structural steel installation after one nut has been set to elevation by the concrete contractor. Assume protection of block outs in slab
on grade once structural steel erection begins.
11.	Furnish and install covers at all holes in elevated decks created by your own work in which debris may fall to the level below, per Cal OSHA regulations.
12.	Furnish all roof access ladders. Coordinated blocking as required.
13.	Furnish and install all rebar welded to structural steel, angle iron, and misc. iron. 14.	Furnish and install all tube steel assemblies and angles for roof screens.
15.	Furnish and install all steel canopies complete.
16.	Furnish and install all pipe rails, handrails, drinking fountain guard rails/bollards, hold open posts / rails, and guard rails directly embedded in concrete or masonry.
17.	Furnish and install all misc. iron & angles attached to concrete and masonry.
18.	Furnish and install all components of the steel gate assemblies at CMU. Coordinate the channel attachment with plans and CMU contractor. Install channels during the CMU installations. See SD/A303 for example.
19.	Furnished and install all attachment devices for handrails / guard rails. 20.	Furnish and install all compressible material at structural steel.
21.	Furnish and install all steel stairs and rails complete. Schedule installation with steel erection to allow for use by the project for access.
22.	Furnish and install all beams and rails for stage curtain systems, including all holes if required for installation of material.

44

Rebid- AD-1

23.	Furnish and install all tube steel and angles for roll up doors, if required.
24.	Furnish and install steel closure plates for attachment of clips by framing Prime Contractor.
25.	Furnish and install all AESS (Architecturally Exposed Structural Steel) as called for on the contract documents.
26.	This contract will complete all work per the requirements of the Dust Control Plan and SWPPP Plan.
27.	Provide Dust Control for own work.
28.	Furnish / Install / Maintain safety cables, posts, temporary guardrails, and / or covers at all floor opening (per OSHA requirements) and for all leading edges throughout the project. Posts are not to be installed in a manner which would cause them to be embedded within exposed concrete. Clarification: Rails and cables are to be removed by this CES-06 Bid Package, only after all structural roof work has been completed, signed off, and coordinated with the CM and Roofing contractor.
29.	Furnish and install own floor protection.
30.	Furnish and install all miscellaneous iron required for framing.
31.	Furnish and install all structural steel support inroof framing for all HVAC equipment. HVAC Prime Contractor to provide and install support rods, angle iron, and diagonal bracing as shown in mechanical.
32.	Furnish and install all structural support as required for electrical or plumbing items to be suspended or mounted to structural steel members.
33.	Provide all Galvanizing of steel and deck components as required by contract documents. 34.	Provide All Deck and deck closures per plan.
35.	Provide all gage metal associated with structural steel or deck.
36.	Furnish and install any and all steel framing for architectural, mechanical, plumbing, and electrical openings.
37.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this Project.

FOB Items
1.	All structural steel anchor bolts and templates.
2.	Furnish FOB jobsite all bolt templates for all patterns (made 10ga or thicker of steel one of each column)foruse bytheconcretecontractor.Include (4) punched¼”holes oneach plate as directed by the building concrete contractor.
3.	Furnish FOB jobsite all associated sleeves for handrails, and guard rails, etc. for installation by this contract.
4.	FOB all counter support brackets, Structural steel / iron that attaches to framing/casework and equipment support. Count and handing to be confirmed with plans and casework. See X/A 310, and Similar at counter roll up’s, see A7, A11/ X/A411.
5.	Furnish embed plates and angles with rebar/nelson studs per contract documents FOB Jobsite for installation by others.
6.	Furnish threshold / slab edge angles FOB jobsite. See slab edge angles A1/X/A411 as an example. 7.	Access ladders
8.	Steel tube wall supports at low walls. See N1/E/A104.
9.	Furnish steel angles and grating for venting of the portable buildings. See plans for size and quantities. Grates and frames to be installed by site concrete bid package.
10.	Furnish steel stand for the safe. See details.

45

Rebid- AD-1

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.
1.	Not Applicable.

End of Bid package

46

Rebid- AD-1

THIS BID PACKAGE PREVIOUSLY BID IN INCREMENT #2

CES-07 SHEET METALS, MEMBRANE ROOFS, WALL AND ROOF PANEL SYSTEMS

Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections
Refer to additional related specifications sections for work specifically included in this bid package noted below.

Division 00 Division 01
Section 07 21 00 Insulation (As applicable to roof systems) Section 07 40 00 Metal Panels
Section 07 54 19 Elastomeric Membrane Roofing Section 07 60 00 Sheet Metal
Section 07 92 00 Sealants
Appendix “B” Interior Color Schedule Plus Drawings Appendix “C” Exterior Color Schedule
Geotechnical Engineering Report

General Items
1. See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2. Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3. Provide all backfill of excavations to original sub-grade for work included in this bid package.
4. Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5. Provide daily cleanup to keep site clean and orderly.
6. Protect identified improvements to remain on civil plan sheets.
7. Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8. Prime Contractor is required to attend all coordination meetings as required by CM.
9. Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10. Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.

47

Rebid- AD-1

11. Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12. Each bid package is responsible for dewatering as it pertains to their scope of work.
13. Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14. Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15. Monthly pay apps will not be approved if as-builts are not updated monthly.
16. Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17. There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

18. All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

19. This contract is to provide temporary power for own work until such time as building temporary power is established.
20. Furnish clean up daily and off-haul of all debris generated by this contract to disposal bins provided under CES-12. Prime Contractor must abide by the Waste Management specification.

Coordination with Other Trades
1.	Provide coordination drawings for work related to this bid package. Coordinate all drawings with the drawings of other bid packages. Note conflicts and provide potential solutions to CM for review. Coordination must occur prior to installation of work. A representative from your company must be in attendance of all coordination meetings.
2.	Coordinate all work to provide access to buildings for other trades as scheduled. Coordinate other activities in the schedule for other trades and confirm with construction schedule.
3.	Provide shop drawings for all fabrications.
4.	Coordinate downspouts with steel, Framing, and Site Plumbing package. 5.	Provide written lay-out for all backing required.
6.	Coordinate backing and reglet elevations with metal framing contractor.

Furnish and Install Items
1.	Furnish and install all flashing and sheet metal including prefinished, for metal panels.
2.	Furnish and install parapet cap at all locations and all other flashing and sheet metal on the project.
3.	Furnish and install reglet flashing where stucco or wall panels meet roofs or other surfaces. 4.	Furnish and install gutters.
5.	Furnish and install all hangers, supports and bracing necessary for installation of work included in this contract.
6.	Physically layout for own work.
7.	Furnish and install all boot flashings.
8.	Provide sheet metal cap and associated flashings for electrical and mechanical equipment platforms as shown.

48

Rebid- AD-1

9.	Furnish and install Door and Window Flashings.
10.	Furnish and install all sheet metal window sill flashings. Coordinate sizes, depths, and configurations with Storefront/window prime contractor and all plans.
11.	Furnish and install all sleeves for all utilities passing through exterior finishes where applicable. 12.	Furnish and install wall penetration flashings.
13.	Furnish and install all wall opening flashings.
14.	Furnish and install all metal wall, roof, and ceiling panel systems complete. Install Z furring as indicated. All wall rigid Insulation included in Bid Package CES-09. Clarification: This CES-07 bid package will furnish and install vapor/weather barrier and flexible flashings over insulation at areas for own work/metal panels. Extend weather barrier a minimum of one stud bay beyond limits of metal panels to ensure proper lap where materials will be continued by plaster contractor.
15.	Furnish and install all items noted in the drawings and spec’s associated with metal roof and wall panels as a complete system.
16.	Furnish and install prefinished, color matched sheet metal for all conditions shown.
17.        Furnishand install all sealants as notedabove,inaddition to the followingis alist of specific items: a. Furnish and install all sealants associated with the prefinished roof or wall systems,
including where prefinished materials abut an adjoining finished material, as shown in specific details.
18.	Furnish and install all panels, and clip systems complete, including Z furring/hat channels as detailed.
19.	Furnish and install all exterior rigid insulation at roof and under metal roof panels per plans.
20.	Furnish and install all flashings and trim at ductwork penetrations through exterior walls or roof. 21.	Furnish and install all flashing and trim at exterior wall to slab transitions.
22.	Furnish and install metal and roof panels including all closure and flashings complete. 23.	Furnish and install all sealant between metal panels and plaster.
24.	Furnish and install all field cutting of metal roof and wall panels, as required, to meet construction schedule.
25.	Furnish and install sealant at louvers and hollow metal frames.
26.	Furnish and install drip edge, flashings, and counter flashings at roof.
27.	Furnish and install watertight closures, (pre flashings) at all gang and individual pipe penetration through exterior walls.
28.	This contract will adhere to the requirements of the Dust Control Plan and SWPPP Plan. 29.	Provide Dust Control for Own Work.
30.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this Project.
31.	Furnish and install all roof jacks. Coordinate sizes and quantities with other Primes and plans. 32.	Furnish and install all sheet metal window sill flashings. Coordinate sizes, depths, and
configurations with Storefront/window Prime Contractor and all plans.
33.	Furnish and install all sleeves for all utilities passing through exterior finishes where applicable. 34.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact
Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this Project.

49

Rebid- AD-1

FOB Items
1.	Color match touch up paint.

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.

End of Bid package

50

Rebid- AD-1

THIS BID PACKAGE PREVIOUSLY BID IN INCREMENT #2

CES-08 FINISH CARPENTRY
Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections Division 00
Division 01
Section 06 22 00 Millwork
Section 06 41 23 Modular Casework
Appendix “B” Interior Color Schedule Plus Drawings Appendix “C” Exterior Color Schedule
Geotechnical Engineering Report

Refer to additional related specifications sections for work specifically included in this bid package noted below.

General Items
1.	See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2.	Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3.	Provide all backfill of excavations to original sub-grade for work included in this bid package.
4.	Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5.	Provide daily cleanup to keep site clean and orderly.
6.	Protect identified improvements to remain on civil plan sheets.
7.	Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8.	Prime Contractor is required to attend all coordination meetings as required by CM.
9.	Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10.	Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11.	Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12.	Each bid package is responsible for dewatering as it pertains to their scope of work.

51

Rebid- AD-1

13.	Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14.	Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15.	Monthly pay apps will not be approved if as-builts are not updated monthly.
16.	Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17.	Provide daily cleanup to keep site clean and orderly.
18.	There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

19.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

20.	This contract is to provide temporary power for own work until such time as building temporary power is established.
21.	Furnish clean up daily and off-haul of all debris generated by this contract to disposal bins provided under CES-12. Prime Contractor must abide by the Waste Management specification.

Coordination with Other Trades

Furnish and Install Items
1. Coordinate and install counter brackets mounted to studs furnished by building steel bidpackage. 2. Furnish and install all casework shown on the contract documents.
3. Furnish and install all drilling of holes for work performed in this bid package.

4. Furnish and install all openings in casework and tops for other trades as well as cable holes and grommets as laid out by District.
5. Furnish & install all sleepers, shims, floor anchorage devices, angles, and floor blocking for attachment of casework. Backing in wall to be provided by the framing bid package.
6. Furnish and install wood rough carpentry framing incorporated into casework including utility chases.
7. Furnish and install all supports and bracing necessary for installation of work included in this bid package. Including surface mounted counter support brackets, and those built into reception counter areas. Structural steel counter brackets by others.
8. Furnish and install casework accessories as noted in specification. 9. Furnish and install shims and wood supports.
10. Install all counter support brackets, Structural steel / iron that attaches to framing/casework support.
11. Furnish and install all counter tops.

12. Furnish and install all solid surface window sills.

13. Furnish and install all casework/Millwork, doors, trims, nosing, skirting, railings, etc. at stage. Steps to be flooring contractor.
14. Furnish and install all millwork accent wall/ceiling components. Trees and accent laminate, see X/A 316 and other specific conditions listed within the casework schedule documents.

52

Rebid- AD-1

15. Furnish and install all Wood framing incorporated into casework and laminated walls. 16. Furnish and install angle connectors.
17. Furnish and install trim.

18. Provide casework submittals and shop drawings within 14 days of Notice to Proceed. 19. Provide all accessory items normally required by this trades standard of care.
20. Furnish and install upholstery where shown. Clarification: Furnish and install all associated upholstery with Modular Casework. See J7 on X/A315 for an example.

FOB Items
1. None

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.

End of Bid package

53

Rebid- AD-1

THIS BID PACKAGE PREVIOUSLY BID IN INCREMENT #2

CES-09 METAL FRAMING, PLASTER, AND GYPSUM BOARD

Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections
Refer to additional related specifications sections for work specifically included in this bid package noted below.

Division 00 Division 01
Section 03 15 14 Drilled Anchors
Section 07 21 00 Insulation (as applicable to all exterior wall rigid insulation) Section 09 22 16 Metal Framing
Section 09 24 00 Cement Plaster Section 09 29 00 Gypsum Board
Appendix “B” Interior Color Schedule Plus Drawings Appendix “C” Exterior Color Schedule
Geotechnical Engineering Report

General Items
1. See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2. Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3. Provide all backfill of excavations to original sub-grade for work included in this bid package.
4. Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5. Provide daily cleanup to keep site clean and orderly.
6. Protect identified improvements to remain on civil plan sheets.
7. Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8. Prime Contractor is required to attend all coordination meetings as required by CM.
9. Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10. Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.

54

Rebid- AD-1

11. Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12. Each bid package is responsible for dewatering as it pertains to their scope of work.
13. Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14. Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15. Monthly pay apps will not be approved if as-builts are not updated monthly.
16. Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17. There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

18. All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

19. This contract is to provide temporary power for own work until such time as building temporary power is established.
20. Furnish clean up daily and off-haul of all general trash debris generated by this contract to the bins provided by CES-12. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.

Coordination with Other Trades
1.	Provide coordination drawings for above ceiling work for work related to this bid package. Coordinate all drawings with the drawings of other bid packages. Note conflicts and provide potential solutions to the CM architect for review. Coordination must occur prior to installation of work. Attend all coordination meetings required to coordinate all above ceiling work.
2.	Coordinate installation of blocking, backing, etc. for other bid packages from written/physical layout provided.
3.	Provide review and verification of space for ADA requirements prior to framing. Report any discrepancies.
4.	Confirm backing is installed to satisfaction of toilet accessory and toilet partition contractor prior to installation of ceramic tile.
5.	Coordinate stud layout where applicable for the installation of counter support brackets.
6.	Coordinate the installation of fire safing/insulation with the insulation contractor. Insulation contractor to provide insulating materials for all areas that would be concealed during the framing, making post framing installation not practical or possible. Framing package to install insulation in headers, trimmers, channels, and heads of walls.
7.	Provide a plaster control and expansion joint layout for architect approval prior to installation.
8.	Plaster Bid package shall coordinate with Painting Bid Package the application of the cement plaster painting system, and provide written report of the cement plaster pH prior to the painting application.
9.	Install and bolt metal studs to Steel tube wall supports at low walls. See N1/E/A104.

55

Rebid- AD-1

Furnish and Install Items
1.	Furnish and install all exterior rigid insulation at walls, including weather barrier over framing and insulation if assembly required per specs. “All exterior” is to include areas behind all wall finishes, stucco, metal panels, columns, when applicable, etc. Coordinate with metal panel contractor for specifics as necessary.
2.	Furnish and install own floor protection (i.e., Tarps, plastic, plywood, etc.).
3.	Furnish and install all drywall systems as called for in the contract documents.
4.	Furnish and install all fire rated top of wall systems. Insulation contractor to “Stuff and Spray” appropriate materials per plans.
5.	Furnish and install all cement board/green board including skim coat prep for finishes.
6.	Furnish and install all tape and texture systems. Provide adequate heating to ensure that tape/textured areas that are worked on any given day, are dry enough to resume work for the following coat, texture, priming, or paint, the following day, start of work.
7.	Furnish and install all sound board.
8.	Furnish and install all gypsum suspended ceilings.
9.	Furnish and install all insulation and fire safing as required in concealed and framing entrapped areas.
10.	Furnish and install acoustical caulking where applicable.
11.        Furnish and install all lath, plaster, drywall, and metal stud framing complete. 12.        Install insulation at metal deck voids at top of wall in entrapment conditions.
13.        Furnish and install all metal stud or flat backing for all trades, including backing for plumbing downspouts,Casework,railings, signage,electrical,restroomaccessories, kitchenequipment,etc.
14.	Furnish and install all fire rated assemblies wrapped in drywall as called for throughout the documents.
15.	Furnish, install, remove scaffolding for all work included in this trade. 16.	Furnish and install all gauge plate to install studs at metal deck.
17.	Furnish and install all gauge closure plate to connect deck to studs.
18.	Furnish and install all gauge material for attachment for metal studs and braces. 19.	Furnish and install all insulation draft / fire stops framing and drywall per plans.
20.	Furnish and install all items noted in contract documents as cement plaster. This includes but is not limited to the following: Flexible flashings and water/air barrier specified as part of the system.
21.	Furnish and install all Flexible Penetration Flashing Sheets around all items that penetrate all building exterior walls (stucco, metal panels, etc.) including but not limited to doorframes, window frames, structural steel, piping etc. as required for a complete water/airtight assembly as designed. Extend weather barrier a minimum of one stud bay beyond limits of stucco to ensure proper lap where materials will be continued by metal panels contractor.
22.	Furnish and install all metal framing attachments to Structural Steel & metal deck.
23.	Furnish and install metal stud/flat strap backing for all electrical mechanical and plumbing shown on those drawings.
24.	Furnish and install backing for plaster expansion joints and moldings as required for proper installation.
25.	Furnish and install framing and sheetrock for fire rated assemblies at electrical, plumbing, and mechanical utilities and fixtures.
26.	Furnish and install gypsum board exterior sheathing.
27.	Furnish and install primer / surface coat at gypsum board as called for in the specifications.

56

Rebid- AD-1

28.	Furnish, install and physically layout all openings, block-outs, metal backing, blocking, blocking for utility and fixture supports. Coordinated locations with related trades prior to installationof metal framing.
29.	Protect adjacent products during plaster operations.
30.	All means of temporary heat/cooling for installation of work (taping/texture) will be provided by this bid package.
31.	This contract will complete all work per the requirements of the Dust Control Plan and SWPPP Plan.
32.	Provide Dust Control for Own Work.
33.	This bid package is to provide a washout for cleanup after construction activities, reference SWPPP plan for details and requirements. Location of washout should be in a location so as to not obstruct or impede work by other trades.
34.	This bid package is to off haul all metal stud/framing scrap. All weight and recycle tags are to be delivered to the Waste Management Coordinator (CES-12).
35.	This bid package is to provide all haul off of drywall gyp scrap. All weight tags to be delivered to the Waste Management coordinator.
36.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this Project.
37.	Provide all scaffolding for own work, including all permits for scaffolding as required. Daily inspections before start of work are mandatory. Provide daily safety inspection reports to CM (CM).
38.	Furnish and install all hangers, supports and bracing necessary for installation of work included in this Contract.
39.	Prime Contractor is responsible for allwork referenced throughout the project documents related to this Prime Contractor’s scope of work.
40.	Provide complete mockups as required by the specifications.
41.	Furnish and install protection of all roofing when work under this contract requires access on the roofing systems.
42.	Furnish and install self-furring lath and smooth wall/Parged wall material over CMU for chalk board paint. See N4/SD-A304

FOB Items
1.	Provide the concrete bid package with physical layout and all bolts if required for this package, that embed into concrete and masonry for sill, wall, cap, and ceiling framing related to this scope of work. A concrete sign-off will be acknowledge prior to concrete placement.

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.

End of Bid package

57

Rebid- AD-1

THIS BID PACKAGE PREVIOUSLY BID IN INCREMENT #2

CES-10 WALL MATERIALS AND ACOUSTICAL CEILINGS
Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections Division 00
Division 01
Section 09 50 00 Acoustical Ceilings Section 09 72 00 Wall Coverings
Section 10 26 00 Wall and Corner Guards

Appendix “B” Interior Color Schedule Plus Drawings Appendix “C” Exterior Color Schedule
Geotechnical Engineering Report

Refer to additional related specifications sections for work specifically included in this bid package noted below.

General Items
1.	See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2.	Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3.	Provide all backfill of excavations to original sub-grade for work included in this bid package.
4.	Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5.	Provide daily cleanup to keep site clean and orderly.
6.	Protect identified improvements to remain on civil plan sheets.
7.	Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8.	Prime Contractor is required to attend all coordination meetings as required by CM.
9.	Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10.	Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11.	Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12.	Each bid package is responsible for dewatering as it pertains to their scope of work.

58

Rebid- AD-1

13.	Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14.	Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15.	Monthly pay apps will not be approved if as-builts are not updated monthly.
16.	Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17.	There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

18.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

19.	This contract is to provide temporary power for own work until such time as building temporary power is established.
20.	Furnish clean up daily and off-haul of all debris generated by this contract to disposal bins provided under CES-12. Prime Contractor must abide by the Waste Management specification.

Coordination with Other Trades

Furnish and Install Items
1. Furnish and install all acoustical ceiling complete. 2. Furnish and install all FRP.
3. Furnish and install all vinyl covered tack board.

4. Furnish and install all hangers, supports and bracing necessary for installation of work included in this bid package.
5. Furnishandinstall allAcoustical caulkingandsealant atalllocations where tack boardmeets other materials.
6. Furnish and install tile at electrical and low voltage devices prior to dropping of tile activity.

7. Furnish and install all “hanger wires” for work in this bid package and light fixtures, cable trays, projector mounts and air terminals per detail. Electrical and mechanical bid packages will make final connections to devices.
8. Furnish and install all compression struts.

9. Furnish and install all protective wall coverings (FRP) and corner guards complete. 10. Furnish and install all tack board and associated trims.
11. Furnish and install all corner guards.

12. Provide daily clean-up and off-haul of own debris.

FOB Items
1. None

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.
End of Bid package

59

Rebid- AD-1

THIS BID PACKAGE PREVIOUSLY BID IN INCREMENT #2

CES-11 PAINTING
Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections Division 00
Division 01
Section 03 35 10 Polished Concrete Finishing Section 07 92 00 Sealants
Section 09 67 23 Resinous Flooring Section 09 91 00 Painting
Appendix “B” Interior Color Schedule Plus Drawings Appendix “C” Exterior Color Schedule
Geotechnical Engineering Report

Refer to additional related specifications sections for work specifically included in this bid package noted below.

General Items
1.	See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2.	Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3.	Provide all backfill of excavations to original sub-grade for work included in this bid package.
4.	Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5.	Provide daily cleanup to keep site clean and orderly.
6.	Protect identified improvements to remain on civil plan sheets.
7.	Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8.	Prime Contractor is required to attend all coordination meetings as required by CM.
9.	Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10.	Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11.	Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.

60

Rebid- AD-1

12.	Each bid package is responsible for dewatering as it pertains to their scope of work.
13.	Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14.	Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15.	Monthly pay apps will not be approved if as-builts are not updated monthly.
16.	Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17.	There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

18.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

19.	This contract is to provide temporary power for own work until such time as building temporary power is established.
20.	Furnish clean up daily and off-haul of all debris generated by this contract to disposal bins provided under CES-12. Prime Contractor must abide by the Waste Management specification.

Coordination with Other Trades
1. Schedule paint coats so as to allow for completion of work with minimal damage with final coat being installed with majority of work completed. Touch up as required.
2. Plaster Bid package shall coordinate with Painting Bid Package the application of the cement plaster painting system, and provide written report of the cement plaster pH prior to the painting application.
3. Coordinate the painting of mechanical Prime Contractor provided louvers or vents, light fixture escutcheons, and other similar items designated to be painted to match at accent walls and ceilings.

Furnish and Install Items
1. Furnish and install all painting and sealing complete for the project. 2. Furnish and install finish as specified for trim, doors, and millwork.
3. Furnish and install all surface preparation and finish of all flashing to be painted. 4. Furnish and install touch-up painting.
5. Furnish and install all painting of mechanical, plumbing, and electrical utilities and equipment as required. HVAC grilles & registers as required.
6. Furnish and install painting at all new doors as required.

7. Furnish and install all accent, murals, Logo’s, and signage painting.

8. Furnish and install own floor protection (i.e., Tarps, plastic, plywood, etc.). 9. Furnish and install CFS Concrete Floor Sealers on floors as specified.
10. Furnish and install all resinous floor systems complete. Prep as required. Grind concrete at openings. Coordinate with door hardware installer. (Thresholds for extent)
11. Furnishandinstall painting of door frames as shownonthe drawings andinthe openings schedule. 12. Furnish and install Caulking and sealants of new hollow metal frames, interior and exterior.
13. Furnish and install Paint at all flashings, caps, trims, steel, steel downspouts, etc., where not noted

61

Rebid- AD-1

to have “Factory Finish”.

14. Furnish and install painting of all site items noted or scheduled. See fire equipment for example SD/X102.
15. Furnish and install Chalk Board Paint at CMU. Coordinate with CMU and Plaster. See N4/SD/A304 for reference.

FOB Items
1. None

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.

End of Bid package

62

Rebid- AD-1

THIS BID PACKAGE PREVIOUSLY BID IN INCREMENT #2

CES-12 GENERAL SPECIALTIES
Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections Division 00
Division 01
Section 01 64 00 Owner Furnished Items Section 01 74 19 Waste Management Section 03 15 14 Drilled Anchors
Section 06 10 00 Rough Carpentry Section 07 18 50 Vapor-Alkalinity Control Section 07 21 00 Insulation
Section 07 72 00 Roof Accessories Section 07 92 00 Sealants
Section 08 11 00 Metal Doors and Frames Section 08 15 13 Laminate-Faced Wood Doors Section 08 31 13 Access Doors and Frames Section 08 33 00 Coiling Doors
Section 08 41 00 Storefronts
Section 08 41 13 Folding Door System Section 08 56 59 Service Windows Section 08 70 00 Hardware
Section 08 70 00.1 Hardware Schedule Section 08 80 00 Glass
Section 09 30 00 Tile
Section 09 64 66 Resilient Wood Floor
Section 09 65 10 Resilient Base and Accessories Section 09 65 16 Resilient Sheet
Section 09 68 40 Carpet
Section 10 05 00 Miscellaneous Specialties (Building Plaque, Dimensional Letters, Cubicle Curtain System, Folding Partitions, Lock Box, Stair Stripping, Safe, Book Cart, Projection Screen)
Section 10 11 00 Visual Display Boards Section 10 14 00 Identifying Devices Section 10 21 13 Toilet Partitions Section 10 28 13 Toilet Accessories
Section 10 44 00 Fire Protection Specialties Section 10 51 13 Metal Lockers
Section 11 40 00.01 Food Service Equipment Section 11 61 43 Stage Curtains
Section 11 68 13 Play Equipment Section 14 42 00 Wheelchair Lifts
Appendix “B” Interior Color Schedule Plus Drawings

63

Rebid- AD-1

Appendix “C” Exterior Color Schedule Geotechnical Engineering Report

Refer to additional related specifications sections for work specifically included in this bid package noted below.

General Items
1.	See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2.	Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3.	Provide all backfill of excavations to original sub-grade for work included in this bid package.
4.	Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5.	Provide daily cleanup to keep site clean and orderly.
6.	Protect identified improvements to remain on civil plan sheets.
7.	Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8.	Prime Contractor is required to attend all coordination meetings as required by CM.
9.	Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10.	Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11.	Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12.	Each bid package is responsible for dewatering as it pertains to their scope of work.
13.	Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14.	Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15.	Monthly pay apps will not be approved if as-builts are not updated monthly.
16.	Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17.	There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

18.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting

64

Rebid- AD-1

requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

19.	This contract is to provide temporary power for own work until such time as building temporary power is established.
20.	Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.

Coordination with Other Trades
1. Provide coordination drawings for above ceiling work for work related to this bid package. Coordinate all drawings with the drawings of other bid packages. Note conflicts and provide potential solutions to the architect for review. Coordination must occur prior to installation of work. Attend all coordination meetings required to coordinate all underground and above ceiling work.
2. Confirm that backing by framer is installed to satisfaction of toilet accessory and toilet partitions installer prior to installation of ceramic tile.
3. Coordinate ceramic tile installation with mirror locations at toilets. 4. Provide written layout for all backing required for this bid package.
5. Coordinate at the jobsite all plumbing and electrical locations during rough-in activities to assure proper fit at time of casework and equipment installation.
6. Due to schedule constraints field measuring should be considered at framing stage in lieu of after all drywall and finishes are complete. Review the schedule to determine necessity relative to fabrication times. If measurement is required at the framing stage, providemeasurement to meet the schedule and figure all associated finishes.
7. Coordinate hollow metal and storefront openings with framing Prime Contractor. Verify all openings after framing, and before exterior finishes to ensure proper fitment.
8. Coordinate size, shape and profiles of sheet metal pans and head flashings with sheet metal package. Installations andphasingto be coordinated for besttime management of multiple trades with CM.
9. Coordinate electrical and FA with coiling doors as required.

Furnish and Install Items
1. Furnish and install all hangers, supports and bracing necessary for installation of work included in this bid package.
2. Provide daily clean-up and off-haul of own debris. 3. Furnish and install own floor protection.
4. Furnish and install fire-stopping/safing complete. 5. Furnish and install layout for your own work.
6. Furnish and install Scaffold for own work.

7. Protect existing surfaces to remain from damage from your work. 8. Furnish and install all interior insulation complete.
9. Furnish and install all fire safing and insulation at underside of roof decks at head of walls, beam pockets, and structural steel.
10. Furnish and install all fire rated top of wall systems complete. Safe, stuff, spray, etc. 11. Furnish and install floor prep for flooring. Level concrete within tolerance as required.

65

Rebid- AD-1

12. Furnish and install all flooring prep per manufacturers requirements, including filling, patching, crack control, leveling as required.
13. Furnish and install all flooring, with the exception of polished or resinous materials.
14. Furnish and install all wood steps, nosing’s, and coordinate with Finish Contractor trims. Clarification: Flooring contractor to include installation of all contrasting color stripes at steps per code and as called for per plans.
15. Furnish and install all walk off materials. 16. Furnish and install all sheet flooring.
17. Furnish and install all carpet. Clarification: All carpet specified as “Clovis Blue” and “Walk off” will be provided by the district, and installed by this bid package. Any other carpet types or colors will be furnished and installed under this bid package.
18. The flooring contractor is to include all flooring installations at the portables. This includes “Furnish Mondo and install”. New portables drawings indicates that carpet, sheet flooring, and rubber base are all by others.
19. Furnish and install all rubber base at all floor systems throughout the project per plans and finish schedules.
20. Furnish and install all tile. Walls, floors, base, and grouts.
21. Furnish and install all exterior signage shown on architectural drawings complete except for parking and street signage.
22. Furnish and install all access signage on walls and fencing. Earthwork to provide all parking lot signage.
23. Furnish and install all building lettering and signage. 24. Furnish and install all dimensional letters complete. 25. Furnish and install all interior graphics.
26. Furnish and install building plaque.
27. Furnish and install all toilet accessories and mirrors.
28. Install all owner provided Soap and paper towel dispensers. 29. Furnish and install all mop/broom/rag holders.
30. Furnish and install all new toilet partitions. 31. Furnish and install firefighting devices.
32. Furnish and Install Knox boxes.
33. Furnish and install access doors shown on the reflected ceiling plan.
34. Furnish and install all wood framing. Steps, plywood backer boards, and in electrical/data rooms per finish schedule
35. Furnish and install all plywood, including stage subfloor, and including under stage on walls listed as rough carpentry, fire rated sheathing, etc.
36. F&I all rough carpentry, in all locations as shown in plans, including those, but not limited to those associated with the furring/shim space at storefront and similar conditions. See X/A421 for examples.
37. Project final cleaning.
38. Provide project final cleaning. All buildings, inside and out, windows,doors, walls, floors, cabinets, tops, restrooms, sidewalks, parking areas, etc.
39. Furnish, install, manage, trash and waste management.
40. Provide project trash/recyclable materials dumpsters, per spec section 01 74 19. Provide for the haul off and disposal of all trash and recyclables during the course of the project. Provide Reports per specifications. Drywall and metal stud scrap will be disposed/recycled by the metal stud framing contractor, and all tags will be provided to this general Specialties contractor for tracking

66

Rebid- AD-1

and waste management reporting.
41. Furnish and install all roof accessories. Hatches, ladder ups, railings, stage roof vent, etc.
42. Furnish and install all stage roof vent rigging, pulleys, winch, proposed installation layout plan, etc. for manual testing. Coordinate all backings and blockings with metal framing, and manufacturers recommendations. Any materials thicker than the 16 ga stud materials required for backing (if applicable) will be provided and installed under this Misc. Specialties package.
43. Furnish and install all doors. Wood, aluminum, laminate faced, hollow metal, steel, roll up, etc. 44. Furnish and install all electronic access controls. Connect to power supplied by Electrical
contractor. Test and confirm operations.
45. Furnish and install all hardware and doors complete.
46. Furnish and install all Storefront systems complete, including all testing, glazing, hardware, etc. 47. Furnish and install door hold opens at concrete including coring of existing concrete as needed. 48. Furnish and install all wood doors and plastic laminate faced wood doors.
49. All and any aluminum closures, break metals, trims, flashings, sill pans, for any storefront is to be provided and installed under this package.
50. Furnish and install all glass/glazing, and associated sealants.
51. Furnish and install all hollow metal frames, doors, and windows.
52. Furnish and install all louvers and door lights as shown and per schedule. 53. Furnish and install all coiling doors.
54. Furnish and install all service windows.
55. Furnish and install all hardware. Gate and decorative fence hardware to be provided and installed under the site concrete and fence package.
56. Furnish and install all visual display/dry erase markerboards. Coordinate and confirm backing with framing, and coordinate placement with electrical and low voltage.
57. Furnish and install all lockers, including the installation of the owner furnished Bike Lockers. 58. Furnish and install all bike racks.
59. Furnish and install Flagpole assembly complete. Coordinate location, excavation, sleeve installations with Site Concrete plan and Prime Contractor.
60. Furnish and Install Safe. Coordinate installation with casework and metal stand in tall storage cabinet. Clarification: Provide AMSEC safe model UL1812E, as listed in detail N11. AD1 AX04. Disregard safe reference in both the safe specification, and the one listed in the General Specialties specification.
61. Furnish and install all food service equipment per plans, including custom fabrications, and all stainless wall panels at cooking line. Coordinate Food Service Shop drawings with plans and Framing. Clarification: Furnish and install food service equipment is to include all equipment on the Food Service Equipment Schedule, on E/A102. The faucet and drain components will be supplied under this bid package, and provided to the plumbing contractor for installation on the sinks, hose reels, dishwasher, disposal, etc.
62. Furnish and install all SS counters including pass throughs. Example A7, A11, on X/A411. 63. Provide all factory start ups for supplied equipment.
64. Furnish and install stage curtain track and all associated support items. i.e. Unistrut, bolts, angle iron, etc. This includes angle noted as “Steel And Fabrication” in detail P11 on X/A603.
65. Furnish and install sneeze guards. Coordinate size with plans, framing, and Hollow metal Primes and shop drawings.
66. Furnish and install cubicle curtains and stage curtain.
67. Furnish all playground Play structures. Coordinate delivery of the structures to the site to be installed by the CES-01 contractor.

67

Rebid- AD-1

68. Furnish and install all bleachers. (6-five row sets) at ball fields. See plans and detail E on SD/X107. Dugout benches are provided and installed under CES-01 bid package.
69. Furnish and install wheelchair lift. Coordinate layout and installation with building concrete, Framing, electrical, and low voltage.
70. Install all roof access ladders, as furnished by Struct Steel bid package. Coordinate bolting and backing with struct steel, framing, backing, drywall, etc. This may require installing ladder to establish bolting locations, tack weld nuts, then remove ladder for drywall and finishes, then reinstall ladder at finish.
71. Furnish and install all projection screens. Coordinate with framing and electrical.
72. Furnish and install operable wall/folding partition/Folding door system. Coordinate with structural steel, metal framing, and finishes.
73. Furnish and install book cart.

FOB Items
1. Deliver insulation to the metal framing Prime Contractor as needed for installations at concealed, entrapped conditions.
2. Furnish and provide playground play structures (x2) to CES-01 Bid Package for final installation.

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.

End of Bid package

68

Rebid- AD-1

THIS BID PACKAGE PREVIOUSLY BID IN INCREMENT #2

CES-13 FIRE SPRINKLERS
Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections Division 00
Division 01
Section 03 15 14 Drilled Anchors Section 07 92 00 Sealants
Section 21 05 17 Sleeves and Sleeve Seals for Fire-Suppression Piping Section 21 05 18 Escutcheons for Fire-Suppression Piping
Section 21 05 23 General-Duty Valves for Fire Protection Piping

Section 21 05 29 Hangers and Supports for Fire Suppression Piping and Equipment Section 21 05 48 Vibration & Seismic Controls for Fire-Suppression Piping & Equipment Section 21 05 53 Identification for Fire-Suppression Piping and Equipment
Section 21 11 00 Facility Fire-Suppression Water-Service Piping Section 21 11 19 Fire Department Connections
Section 21 13 13 Wet-Pipe Sprinkler Systems Appendix “B” Interior Color Schedule Plus Drawings Appendix “C” Exterior Color Schedule
Geotechnical Engineering Report

Refer to additional related specifications sections for work specifically included in this bid package noted below.

General Items
1.	See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2.	Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3.	Provide all backfill of excavations to original sub-grade for work included in this bid package.
4.	Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5.	Provide daily cleanup to keep site clean and orderly.
6.	Protect identified improvements to remain on civil plan sheets.
7.	Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8.	Prime Contractor is required to attend all coordination meetings as required by CM.

69

Rebid- AD-1

9.	Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10.	Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11.	Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12.	Each bid package is responsible for dewatering as it pertains to their scope of work.
13.	Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14.	Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15.	Monthly pay apps will not be approved if as-builts are not updated monthly.
16.	Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17.	There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

18.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

19.	This contract is to provide temporary power for own work until such time as building temporary power is established.
20.	Furnish clean up daily and off-haul of all debris generated by this contract to disposal bins provided under CES-12. Prime Contractor must abide by the Waste Management specification.

Coordination with Other Trades

Furnish and Install Items
1. Furnish and install own floor protection (i.e., Tarps, plastic, plywood, etc.).

2. Furnish and install all supports and bracing necessary for installation of work included in this bid package.
3. Furnish and install fire sprinkler system complete from the point of connection provided from the underground utilities Prime Contractor. (See site plumbing SOW for clarity)
4. Test and flush system per specifications

5. Coordinate the installation of the fire alarm safety devices with the electrical, low voltage Prime Contractor for devices associated with the sprinkler system.
6. Provide and install all signage, and ID tags as required.

FOB Items
1. Tools, keys, and extra heads per plans/spec.

70

Rebid- AD-1

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.

End of Bid package

71

Rebid- AD-1

THIS BID PACKAGE PREVIOUSLY BID IN INCREMENT #2

CES-14 BUILDING PLUMBING and HVAC

Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections
Refer to additional related specifications sections for work specifically included in this bid package noted below.

Division 00 Division 01
Section 03 15 14 Drilled Anchors
Section 05 12 00 Steel and Fabrications (For downspouts/RWL’s and support attachments) Section 07 92 00 Sealants
Section 08 91 00 Louvers
Section 22 00 00 General Plumbing Provisions Section 22 00 50 Plumbing
Section 23 01 00 General Mechanical Provisions Section 23 01 00 General Mechanical Provisions Section 23 05 00 Common Work Results for HVAC
Section 23 05 13 Common Motor Requirements for HVAC Equipment Section 23 05 29 Hangers and Supports for HVAC Piping and Equipment
Section 23 05 48 Vibration and Seismic Controls for HVAC Piping and Equipment Section 23 05 53 Identification for HVAC Piping and Equipment
Section 23 05 93 Testing, Adjusting, and Balancing for HVAC Section 23 07 00 HVAC Insulation
Section 23 08 00 Commissioning of HVAC Section 23 17 10 Variable Frequency Drives Section 23 23 00 Refrigerant Piping
Section 23 31 13 Metal Ducts Section 23 31 16 Nonmetal Ducts
Section 23 33 00 Air Duct Accessories Section 23 34 23 HVAC Power Ventilators Section 23 34 33 Air Curtains
Section 23 38 13 Commercial Kitchen Hoods

Section 23 72 00 Air to Air Energy Recovery Equipment

Section 23 74 13 Package Outdoor Central Station Air Handling Units Section 23 74 33 Packaged Outdoor Heat and Cool Makeup Air Units Section 23 81 50 Variable Refrigerant Flow Air Conditioners
Section 25 50 00 Direct Digital Control and Energy Management Systems Appendix “B” Interior Color Schedule Plus Drawings
Appendix “C” Exterior Color Schedule Geotechnical Engineering Report

72

Rebid- AD-1

General Items
1. See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2. Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3. Provide all backfill of excavations to original sub-grade for work included in this bid package.
4. Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5. Provide daily cleanup to keep site clean and orderly.
6. Protect identified improvements to remain on civil plan sheets.
7. Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8. Prime Contractor is required to attend all coordination meetings as required by CM.
9. Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10. Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11. Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12. Each bid package is responsible for dewatering as it pertains to their scope of work.
13. Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14. Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15. Monthly pay apps will not be approved if as-builts are not updated monthly.
16. Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17. There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

18. All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

19. This contract is to provide temporary power for own work until such time as building temporary power is established.
20. Furnish clean up daily and off-haul of all debris generated by this contract to disposal bins provided under CES-12. Prime Contractor must abide by the Waste Management specification.

73

Rebid- AD-1

Coordination with Other Trades
1.	Provide coordination drawings for work related to this bid package. Coordinate all drawings with the drawings of other bid package. Note conflicts and provide potential solutions to Construction Manager for review. Coordination must occur prior to installation of work. A representative from your company must be in attendance of all coordination meetings.
2.	Coordinate locations of all openings, block-outs, backing, and blocking for utility and fixture supports with related trades prior to installation of framing.
3.	Any holes made through materials to allow installation of utilities not called for in the contract documents shall be installed and reinforced by this bid package.
4.	Coordinate all work to provide access to buildings for other trades as scheduled. Provide a breakout schedule of where and when piping operations will be performed that has been coordinated with other activities in the schedule for other trades.
5.	Coordinate routing of plumbing to miss foundations.
6.	Coordinate the location of depressions, block outs, slopes, and drains with the drawings prior to pour.
7.	Housekeeping and equipment pads will be furnished and installed by the concrete bid package. Provide dimensions for pads.
8.	Coordinate alignment of all utilities between plumbing and civil drawings prior to excavation.
9.	Coordinate at the jobsite all plumbing and electrical locations during rough-in activities to assure proper fit at time of casework and equipment installation. In addition, contractor to confirm all piping will fit in walls.
10.	Coordinate individual building tie-ins or cut over with Construction Manager. Provide a written testing plan for all systems prior to start of service.
11.	Coordinate with other trades that will interface with plumbing equipment and material.
12.	Clean and disinfect all building piping and portables with water piping. Phased construction will necessitate a specific schedule of disinfection coordinated with the other building & site contractors. Create disinfection plan and coordinate with building & site contractors to allow for complete and maintained disinfection of the entire system until acceptance by Owner.
13.	Coordinate water, gas, condensate, and sewer with plans, and food service shop drawings prior to rough in.
14.	Provide dimensions for structural steel openings within 30 days of NTP. 15.	Review as-built drawings for POC prior to starting work.
16.	Layout blocking as required for hangers and supports for own work. Structural steel contractor will provide and install additional structural steel in roof framing as required and shown. Mechanical to provide and install all suspension rods, angle iron, and bracing as shown in mechanical plans.
17.	Provide all necessary openings and/or connection points for EMS and fire alarm wiring and devices.
18.	Housekeeping and equipment pads will be furnished and installed by the concrete bid package. Provide dimensions for pads.
19.        Coordinate heights of all roof curbs to confirm with roofing requirements prior to ordering curbs. 20.        Coordinate location of rough-in prior to ordering HVAC units for electrical mechanical and
plumbing utilities.
21.	Physically layout all coring, drilling, block outs, openings, holes, backing, etc.
22.	All sheet metal as required for HVAC scope, whether noted or not, used on this project shall be furnished and installed under this bid package.
23.	Provide all equipment ready for hook up by Electrical bid package. Coordinate utilities and connections with related trades.

74

Rebid- AD-1

24.	Coordinate HVAC ductwork and equipment with structural steel, fire sprinkler, electrical, and plumbing.
25.	Coordinate all work to provide access to buildings for other trades as scheduled. Provide a breakout schedule of where and when rough-in operations will be performed in the building that has been coordinated with other activities in the schedule for other trades.
26.	Provide all necessary openings and/or connection points for EMS and fire alarm wiring and devices. Fire Alarms Systems will be provided under separate contracts. EMS by this contract.
27.	Coordinate locations of all openings, block-outs backing blocking and blocking for utility and fixture supports with related trades prior to installation of framing.
28.	Layout blocking as required for hangers and supports for own work.
29.	Coordinate all utilities with food service prior to rough in of any materials. 30.	Provide dimensions for structural steel openings within 30 days of NTP.

Furnish and Install Items (Plumbing)
1.	Furnish and install all building fixtures and plumbing utilities to the POC provided by the Site Plumbing bid package, approximately 5’-0” outside of building.
2.	Furnish and install all two-way building sewer clean outs as close to the building as possible. This is a district request. Coordinate with building concrete package to avoid footing conflicts.
3.	Furnish and install water valves and boxes after POC from site utilities contractor’s pipe.
4.	Reference building Architectural sheets for all building downspout connections and details. See sheet XA531 for more information.
5.	Furnish and install all drinking fountains, interior, exterior, and site.
6.	This bid package will be responsible for all final points of connection to all site utilities.
7.	Furnish and install physical layout for all deepened foundations at utilities prior to excavation by the concrete bid package.
8.	Provide Furnish and install all access Panels required for your work.
9.	Provide all backfill of excavations to original subgrade for work included in this bid package.
10.	Furnish off-haul of all excavation spoils for work included in this bid package to one location as determined by Construction Manager.
11.	Furnish and install all attachments of equipment related to this scope of work.
12.	The Food service contractor in CES-12 will furnish and install food service equipment to include all equipment on the Food Service Equipment Schedule, on E/A102. The faucet and drain components will be supplied under that bid package, and provided to the plumbing contractor for installation on the sinks, hose reels, dishwasher, disposal, etc.
13.	Furnish and install all sleeves in foundations prior to the installation of concrete and reinforcing steel. Coordinate location with other related trades prior to excavation.
14.	Furnish and install all excavations for own work.
15.	Furnish and install all concrete required for installation of work in this bid package. 16.	Furnish and install all drilling of holes for work performed in this bid package.
17.	Furnish and install drilling of wood and metal as needed for pipes and supports.
18.	Furnish and install all rough-in for equipment supplied under other bid packages(Kitchen equipment, hvac,…) as required by the related specification sections and drawings. Connect to equipment.
19.	Furnish and install all required utilities for Owner Furnished Equipment, capped and ready for connection. Make connection when installed.
20.	Furnish and install watertight closures at all gang and individual pipe penetrationthrough exterior walls or through roof.
21.	Provide testing of floor and roof drains during installation and at completion of project.

75

Rebid- AD-1

22.	Clean and disinfect all building piping and portables with water piping. Phased construction will necessitate a specific schedule of disinfection coordinated with the other building & site contractors. Create disinfection plan and coordinate with building & site contractors to allow for complete and maintained disinfection of the entire system until acceptance by Owner. Building contractors will be responsible for cleaning and disinfection of building and portable piping.
23.	Furnish and install all identification or lettering noted for the project required for this scope of work.
24.	Furnish and install own floor protection (i.e., Tarps, plastic, plywood, etc.). 25.	Furnish and install all flues associated with own work.
26.	Furnish and install water heater, strapping and platforms complete including steel stand if specified.
27.	Furnish & install drain & overflow piping.
28.	Furnish & install all trap primers and access panels as needed.
29.	Furnish and install protection of existing finishes and roofing for own work. 30.	Insulate hot water and drain pipes under sinks per ADA/code.
31.	Furnish and install all trench drains.
32.	Furnish and install all sand/oil separators complete.
33.	Drill all holes required for curb attachment through steel.
34.	Furnish and install all fire stopping and acoustical/sound sealant assemblies complete for this scope of work.
35.	Furnish and install all condensate piping complete including hook up.
36.	Furnish and install all coring or place sleeves for utilities through masonry and concrete. Sleeves are to be installed prior to rebar and concrete. Coordinate with other contractors prior to excavation.
37.	Furnish and install all fabrication and installation of steel downspouts and brackets. Coordinate fabrication with steel specifications for reference where applicable.
38.	Furnish and install all downspouts and related support bracket assemblies as outlined in Detail A1 on X/A531. Coordinate all backing layout with metal stud framing package, and roofing contractor.
39.	Connect steel downspouts to all rain gutters and storm drains, per all disciplines of drawings.
40.	This contract is to provide temporary power for own work through completion of steel erection as required. Once temporary power has been established by Construction Manager, each contractor will only need to provide temporary utility distribution from services provided. Contractors are responsible for own distribution of power and lighting.
41.	Furnish and install all plumbing identified in the plumbing notes, food service documents, and plumbing drawings.
42.	Furnish and install covers at all holes in elevated decks created by your own work in which debris may fall to the level below, per Cal OSHA regulations.
43.	Furnish and install all roof accessories relative to this contractor’s work.
44.	Furnishand install all shut off valves, and pressure regulator for the gas systems. Connect gas lines from building to gas POC.
45.	Furnish and install all floor drains.
46.	Furnish and install all Unistrut, angles, clips, fasteners, etc. to bottom of deck, beams, etc. for hanging of utilities. Means and methods meeting detailed attachment, code, and approved manufacturers methods.
47.	Furnish and install all gas regulators. And their security cages as noted “General Specialties” see SD/A302
48.	Furnish and install all toilet and sink sensors complete.

76

Rebid- AD-1

49.	This contract will complete all work per the requirements of the Dust Control Plan and SWPPP Plan.
50.	Provide Dust Control for own work.
51.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this Project.
52.	Provide early startup/use of plumbing equipment as required by the Construction Manager/Owner for construction or building systems testing, prior to final acceptance, which will not initiate the warranty period until the filing notice of completion.
53.	The Plumbing Contractor shall include all of the following in its bid and coordinate with each of its own sub trade for a complete project. Each contractor shall submit, at time of the bid, their crewing and bid package plan as to who will be performing what scopes of work and the crew size planned for each.
54.	Any deviation from the contract documents resulting in additional design will be at the cost of this bid package.
55.	This contract shall be responsible for all fireproofing/caulking/assemblies for own work.
56.	Furnish and install all building clean outs approximately 2’ from the building, or as close to the footing as possible at wide footings. Coordinate layout and installation with structural concrete bid package. All clean outs are to be two-way clean outs, per district standards.

Furnish and Install Items (HVAC)
1.	Furnish and install all HVAC equipment, duct, hangers, backing, bracing, supports, and piping supports and curbs necessary for installation of work included in this bid package.
2.	Furnish and install EMS system complete.
3.	Furnish and install all access doors necessary to provide access to work included in this bid package.
4.	Furnish and install all drilling of holes for work performed in this bid package.
5.	Furnish and install all attachment of all equipment related to this scope of work. 6.	Furnish and install all fire stopping related to this bid package.
7.	This contract shall be responsible for all fireproofing/caulking/assemblies for own work.
8.	Furnish and install all identification and lettering called for in the contract documents related to this bid package.
9.	Provide for testing of fire smoke dampers resettable link coordinate with Fire Alarm bid package. Provide fire smoke dampers ready for power hook up.
10.	Provide start up and run equipment for acclimation and allow use of HVAC systems without effecting official start date of Warranty period upon Owner acceptance of project. Provide early startup and maintenance of HVAC equipment as required by CM, for acclimatization of buildings prior to final acceptance, which will not initiate the warranty period until the filing notice of completion. Provide for 2 filter changes for all required equipment throughout the building. If filter replacement is not required, then filters are to be turned over to the district during close out procedures.
11.	Furnish and install own floor protection (i.e., Tarps, plastic, plywood, etc.). 12.	Furnish and install all pre-manufactured roof curbs at the roof.
13.	Furnish and install all roof curb adapters as required. 14.	Furnish and install transfer air grilles as noted.
15.	Furnish and install fusible links for equipment testing if applicable. 16.	Provide all controls unless specifically called for in electrical drawings.

77

Rebid- AD-1

17.	Furnish and install all duct work and flues complete associated with own work.
18.	Furnish and install all metal louvers and screens. Provide associated attachment accessories.
19.	Furnish and install louvers at walls complete. Coordinate with exterior envelope flashing contractor/ installer.
20.	Furnish and install all fire and fire smoke dampers ready for device hook up by electrical. 21.	Furnish and install all fans.
22.	Furnish and install all exhaust systems.
23.	Furnish and install sealant as related to this package.
24.	Furnish and install Unistrut & pipe support assembly for own work.
25.	Provide all necessary openings and/or connection points for EMS and fire alarm. Provide conduit and wiring as required for unit shut down controls.
26.	Provide daily clean up. Haul off own debris.
27.	Furnish and install all unit anchorage complete as noted. 28.	Furnish and install control conduit and conductors.
29.	Install communicating smoke detector unit shutdown at the air handler as noted.
30.	Furnish and install all refrigeration piping for all HVAC equipment shown on the plans per manufacturer’s instructions, engineered calculations and Specifications.
31.	Furnish and install all HVAC and Sheet metal (as applies to mechanical equipment) work complete per plans and specs.
32.	Furnish and install all control panels and support.
33.	This contract is to provide temporary power for own work through completion of steel erection as required. Once temporary power has been established each contractor will only need to provide temporary utility distribution from services provided at the building. Contractors are responsible for own distribution of power and lighting.
34.	Furnish and install all drilling of holes, including through metal, for work performed in this contract.
35.	Furnish and install all galvanized steel supports for ductwork at roof if required. 36.	Furnish and install fire duct wrap.
37.	Furnish and install all equipment anchorage.
38.	Furnish and install all flashings associated with ductwork, fans, and hoods, through walls, decks, and roof.
39.	Furnish and install all louver assemblies complete including all clips, screws, and angles necessary to attach louvers except for hollow metal frame to be provided by other Prime Contractors
40.	Furnish and install all mechanical noted in the mechanical notes throughout the food service documents complete.
41.	Furnish and install all Ansul system complete. Provide gas valve to plumber for installation.
42.	Furnish and install all Roof Accessories and/or Curbs/Platforms/Stands/Supports/Steel Backing/Bolts/Angles (wood/ steel / pre-manufactured / framed) for all Mechanical equipment provided under this contract.
43.	Furnish and install all roof mounted pipe supports when required.
44.	Furnish and install covers at all holes in elevated decks created by your own work in which debris may fall to the level below, per Cal OSHA regulations.
45.	Install all duct mounted smoke detector housings provided by the fire alarm Prime Contractor. 46.	Provide all equipment ready for hook up by EMS and Electrical Prime Contractors. Coordinate
utilities and connections with related trades.
47.        All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting

78

Rebid- AD-1

requirements as defined within the Monitoring and Reporting Schedule within the ISR for this Project.
48.	Furnish and install EMS system complete including all conduit, wire, controls, and control panels. 49.	Furnish Air Balancing with report (to include modular buildings).
50.	This contract will complete all work per the requirements of the Dust Control Plan and SWPPP Plan.
51.	Provide Dust Control for own work.
52.	The Mechanical Prime Contractor shall include all of the following in its bid and coordinate with each of its own sub trade for a complete project. Each Prime Contractor shall submit, at time of bid, their crewing and bid package plan as to who will be performing what scopes of work and the crew size planned for each.
53.	This contract shall be responsible for all fireproofing patch back as a result of own work. 54.	Furnish and Install sealant for HVAC work included in this contract abutting other materials.
55.	Furnish and install all sleeves for work passing through masonry and concrete work where required. Coordinate with Respective Prime Contractors.
56.	Furnish and install protection of all roofing when work under this contract requires access on the roofing systems.
57.	Furnish and install all hangers, supports, Unistrut and bracing necessary for installation of work included in this contract.
58.	Furnish and install all sleeves in foundations prior to the installation of concrete and reinforcing steel. Coordinate location with other related Prime Contractors prior to excavation.
59.	All Prime Contractors will provide their own temporary and task lighting needed for this scope of work.
60.	This contract is responsible for holes through metal deck and installation of hanger wires for own work where applicable and approved.
61.	All work will need to be completed as per the supplied bid schedule.
62.	Coordination must occur prior to installation of work. A representative from your company must be in attendance at all coordination meetings.

FOB Items
1.	Furnish all starters at HVAC units. Electrical connections shall be made by Electrical bid package.

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.
1.	Install Duct Detectors provided by Fire Alarm Prime Contractor. Wiring to be completed by electrical Prime Contractor.

End of Bid package

79

Rebid- AD-1

CES-15  BUILDING ELECTRICAL

Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

Specification Sections
Refer to additional related specifications sections for work specifically included in this bid package noted below.

Division 00 Division 01
Section 03 15 14 Drilled Anchors Section 07 92 00 Sealants
Section 10 05 00 Miscellaneous Specialties (Projector Support Panel) Section 26 05 00 Common Work Results for Electrical
Section 26 05 26 Grounding

Section 26 05 53 Electrical Identification

Section 26 20 00 Low Voltage Electrical Transmission Section 26 50 00 Lighting Fixtures
Section 27 00 00 Telecommunication Systems

Section 27 05 28 Communications Infrastructure System Section 27 10 00 Structured Cabling System
Section 27 20 10 Uninterruptible Power Supply Section 27 42 00 Classroom Audio-Visual Systems Section 27 53 13 Analog Synchronous Clocks
Section 27 70 00 Intercom Clock Public Address System Section 27 80 00 Video Surveillance
Section 28 31 00 Fire Alarm and Detection Appendix “B” Interior Color Schedule Plus Drawings Appendix “C” Exterior Color Schedule
Geotechnical Engineering Report

General Items
1. See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2. Furnish and install all layout for own work from survey provided. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3. Provide all backfill of excavations to original sub-grade for work included in this bid package.
4. Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5. Provide daily cleanup to keep site clean and orderly.
6. Protect identified improvements to remain on civil plan sheets.

80

Rebid- AD-1

7. Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8. Prime Contractor is required to attend all coordination meetings as required by CM.
9. Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10. Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11. Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12. Each bid package is responsible for dewatering as it pertains to their scope of work.
13. Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14. Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15. Monthly pay apps will not be approved if as-builts are not updated monthly.
16. Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17. There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

18. All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

19. This contract is to provide temporary power for own work until such time as building temporary power is established.
20. Furnish clean up daily and off-haul of all debris generated by this contract to disposal bins provided under CES-12. Prime Contractor must abide by the Waste Management specification.

Coordination with Other Trades
1.	Provide coordination drawings for underground and above ceiling work for work related to this bid package. Coordination must occur prior to excavation and/or installation of the work. Attend all coordination meetings required to coordinate all underground and above ceiling work.
2.	Provide use and maintenance of electrical equipment and devices as required by the District/or CM for construction and testing of other equipment prior to final acceptance, which will not initiate the warranty period until filing of notice of completion.
3.	Coordinate all work to provide access to buildings for other trades as scheduled. Provide an underground utility schedule of where and when piping operations will be performed.
4.	Coordinate locations of all openings, block-outs, backing, and blocking for utility and fixture supports with related trades prior to installation of framing.
5.	Coordinate location of UG utilities to be out of angle of repose of foundations.
6.	Poured in place housekeeping and equipment pads to be supplied by the concrete contractor.

81

Rebid- AD-1

7.	Review as-builts and pothole existing utilities prior to starting work.
8.	Verify continuity of electrical and low voltage conduits for work in this contract.
9.	Provide shop drawings for equipment layout in electrical rooms to confirm that dimensions are adequate prior to rough in and pouring of footings and curbs.
10.	Connect “hanger wires” provided by the Acoustical Prime Contractor to hang light fixtures. 11.	Coordinate all locations of kitchen equipment for the kitchen and electrical drawings.
12.	Provide dimensions for structural steel openings within 30 days of NTP. 13.	Coordinate all utilities with food service prior to rough in of any materials.
14.	Coordinate wall sizes with pipe sizes prior to installation to confirm all piping will fit in walls.
15.	Coordinate locations of all openings, block-outs, backing and blocking for utility and fixture supports with related trades prior to installation of framing.
16.	Layout above ceiling blockings/backings as required for hangers and support of own work. 17.	Coordinate all underground utilities to miss foundation.
18.	Provide Safe off of all electrical equipment as required for trade work.

Furnish and Install Items
1.	Furnish and install all building and site electrical, wiring and equipment complete, with exception to that being provided in Inc #1, Site Electrical conduit, Rule 16 conduit, switchgear pad, and the installation of the owner supplied switchgear. This bid package CES-15 will provide and install all transformers, disconnects, panels, IDF cabinets, Environmental exterior cabinets, mini unit substation, etc., including concrete footings, equipment pedestal, precast pads, etc.
2.	Furnish and install all conduit from the POC where the Inc 1 electrical Prime Contractors installations stop. Continue all conduits to their final installations into the buildings per plans. Continue all fire conduit to fire sprinkler systems for all fire alarm completion in this package.
3.	Continue all site lighting conduits to all lights and light poles.
4.	Furnish and install all light poles, bases, templates, bolts, forms, groundings, and concrete to complete the site lighting.
5.	Provide installation of final conduit and all connections to pump(s), and irrigation controllers. The site electrical contractor will provide conduit to within 5’ of “Coaches switches” locations. This contract will connect and finish conduit and provided and install a housing box per plan, provide receptacle, wiring and all connections for coaches switches controller to plug in to.
6.	Furnish and install all wiring. Power, lighting, low voltage, data, Fire. EMS and Irrigation to be provided under those prime packages.
7.	Furnish/install/disconnect job site temporary power as required.
8.	Furnish and install temp power cords and connections to the CM office trailer, and the inspector’s trailer, from the CM rented generator.
9.	Furnish and install temp power from CM rented generator to each building. Install two spider boxes in each building, evenly distributed within the space for maximum accessibility.
10.	Furnish and install temp power from CM rented generator to the 480 3-phase irrigation booster pump.
11.	See attached Site Plan Sketch at the end of this section for Temp Power Plan for clarification.
12.	Furnish and install temporary lighting in the main areas of each building equal to a minimum of a continuous temp light stringer the long length of each building, or equal. Connect temp lighting to temp power distribution box, and power, also provided under this package.
13.	Furnish and install physical layouts for all deepened foundations at utilities prior to excavation. 14.	All excavation spoils to be deposited at one location on site as determined by CM.

82

Rebid- AD-1

15.	Furnish and install all sleeves in foundation prior to the installation of reinforcing steel and concrete. Coordinate layout and location with other related bid package trades prior to excavation.
16.	Furnish and install all sleeves for work passing through masonry and concrete work. Coordinate with respective bid packages.
17.	Provide all backfill of excavations to original subgrade for work included in this bid package. 18.	Furnish and install all floor boxes solid for install of slab on grade.
19.	Furnish and install drilling of holes for work performed in this bid package.
20.	Furnish and install fire stopping and fire caulking of own penetrations for own work. 21.	Furnish and install pull strings/rope in all empty or future conduits for own work.
22.	Furnish and install all concrete required for installation of vaults, boxes, underground structures for work related to this bid package.
23.	Provide conduit path/raceway for reception panic button, and dedicated principals phone if required by the district.
24.	Furnish and install all access panels and doors necessary to provide access to work included in this bid package.
25.	Furnish and install all required utilities for Owner furnished equipment hook up as required.
26.	Furnish and install all rough-in for all equipment of other bid packages as required by the related specification sections and drawings. Connect and or stub as described.
27.	Furnish and install all conduit and sleeves for future low voltage and telecommunications wiring. Install fire stopping as required.
28.	Furnish and install disconnects and associated supports not provided on factory equipment installed by other bid packages.
29.	Furnish and install all supports and bracing required for electrical work except for ceiling hanger wires to lights in new ceilings.
30.	Provide connection of “Hanger Wires” to light fixtures, layout of wires will be by this bid package. Connect “Hanger Wires” provided by the Acoustical Bid package to light fixtures, cable trays and projector mounts.
31.	Furnish and install watertight closures and sealants at all gang and individual pipe penetration thru exterior walls.
32.	Furnish and install all identification and lettering called for in the contract documents related to the work of this bid package.
33.	Furnish and install all roof accessories relative to this bid package’s work. 34.	Furnish and install own floor protection (i.e., Tarps, plastic, plywood, etc.). 35.	Furnish and install all clocks and speakers.
36.	Furnish and install all power and fire alarm to smoke and fire dampers as called for in the documents.
37.	Furnish and install all physical layout for your own work.
38.	Core penetrations through CMU wall as required for conduit installation.
39.	Furnish and install all power requirements for owner supplied equipment per plans and specs. 40.	Furnish and install all anchor bolts and templates for light poles and equipment. Form and pour
all light pole bases.
41.	Furnish and install electrical to HVAC units per plans and specs.
42.	Furnish and install protection of all roofing when work under this bid package requires access on the roofing systems.
43.	Provide all power testing for own work.
44.	Furnish duct detector for fan shut-down and signal to fire alarm system at noted Air Handlers, AC Units, Makeup Air Units and Supply, and exhaust Fans.

83

Rebid- AD-1

45.	Furnish and install all lighting and controls as required.
46.	Furnish communicating smoke detector unit shutdown at the air handler and furnish and install fire alarm monitoring as noted.
47.	Furnish and install all power and low-voltage systems complete except for EMS controls. This includes but is not limited to all buildings and site wiring, cable trays and conduit for power clock and speaker, data, fire alarm, lighting controls, security, etc.
48.	Furnish and install all rough in conduit, and power for security and electronic access control per plans and specs.
49.	Furnish and install all Unistrut for electrical work and lighting fixture supports. This includes Unistrut for projector support.
50.	Furnish and install all chain mounted fixtures complete.
51.	Furnish and install all electrical panel mounting complete at roofs except flashing.
52.	Furnish and install all electrical required for kitchen hoods complete including hook up.
53.	Furnish and install all electrical, data, and fire alarm connections required for the stage elevator including testing.
54.	Furnish and install covers at all holes in elevated decks created by your own work in which debris may fall to the level below, per Cal OSHA regulations.
55.	Furnish layout and Unistrut as necessary for backing and supports required for pendent light fixtures.
56.	Furnish and install all power and fire alarm conduit and wiring complete to rollup doors including connections and testing.
57.	Furnish and install all conduit, wiring, and connections for all powered roll up doors.
58.	Furnish and install all power to water heaters, recirculating pumps, and thermo switch complete, in collaboration with the plumbing Prime Contractors installations.
59.	Furnish and install all projectors, projector mounts. Clarification: See specification section 01 64 00 for Owner supplied Contractor installed items. This electrical package will be responsible for the installation and programming of the Owner supplied projectors to interface with the AV equipment supplied and installed within this package.
60.	Furnish and install all required utilities for Owner Furnished Equipment, capped and ready for connection. Make connections as required upon arrival per plans and specs.
61.	Furnish and install all roof curbs associated with electrical work.
62.	Furnish and install all rough-in for all equipment of other trade as required by the related specification sections and drawings. Connect and or stub as described.
63.	Furnish and install all site lighting including bases, poles, and fixtures.
64.	Furnish and install data infrastructure, wiring and cabling per plans and specifications. 65.	Furnish and install disconnects and associated supports.
66.	Furnish and install fire alarm including connection to all fire sprinkler devices.
67.	Furnish and install sealant system as required to provide watertight condition at all exterior devices.
68.	Furnish, install, and coordinate all conduit and wiring within casework. Coordinate with casework Prime Contractor for chase requirements.
69.	Furnish and install all speakers and associated brackets.
70.	Proved power and make connections to owner furnished equipment. 71.        Provide for any and all electrical testing for modular buildings.
72.	Provide low voltage work at modular buildings. including but not limited to, pulling of wire, fire alarm system, security system.
73.	Provide Dust Control for own work.

84

Rebid- AD-1

74.	This contract will complete all work per the requirements of the Dust Control Plan and SWPPP Plan.
75.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this Project.
76.	All excavation spoils to be deposited at one location on site as determined by CM.
77.	Furnish and install all sleeves for work passing through masonry and concrete work. Coordinate with respective bid packages.
78.	Provide all backfill of excavations to original subgrade for work included in this bid package. 79.	Furnish and install drilling of holes for work performed in this bid package.
80.	Furnish and install pull strings/rope in all empty or future conduits.
81.	Furnish and install all attachment of all equipment related to this scope of work.
82.	Furnish and install all identification and lettering called for in the contract documents related to the work of this bid package.
83.	Furnish and install all physical layout for your own work.
84.	This contract shall be responsible for holes at metal deck for installation of hanger wires for own work.
85.	Furnish and install all conduit, wiring, and connections for all powered roll up doors per plans and specs.
86.	Installation of Owner provided television and mount in Building A.
87.	Installation of Owner provided laptop charging towers in Buildings B, C, and D.

85

Rebid- AD-1

86

Rebid- AD-1

FOB Items
1.	Duct Detector Work: These items are provided by Fire Alarm, to be installed by Mechanical Prime Contractors and wired by this contract. Provide additional circuits as needed for mechanical equipment, coordinate with mechanical Prime Contractor.

Installation of FOB Items
Note: Coordinate all deliveries to jobsite with CM. Prime Contractor to Unload, inventory, store and notify CM of any deficiencies for all items delivered to the jobsite FOB.
1.	Install all switches for equipment provided by others i.e., coiling doors, fly fans, exhaust fans, etc. 2.	Install all Owner furnished Electrical equipment and switches where applicable.

End of Bid package

87

Rebid- AD-1

THIS BID PACKAGE PREVIOUSLY BID IN INCREMENT #2

CES-16 OFF SITE IMPROVEMENTS

Furnish and install all work specifically required throughout the project documents to complete the work of this bid package that specifically includes, but is not limited to the following:

PG&E drawings and specifications
City of Fresno codes, and requirements for all utility and street improvements.
Refer to additional related specifications sections for work specifically included in this bid package noted below.

Specification Sections

Division 00 Division 01
City Of Fresno Off Site Street Improvement Plans and Specifications City of Fresno Street Lighting Plans and specifications
City of Fresno Off Site Water Main Improvements Plans and Specifications City of Fresno Off Site Landscape improvements Plans and Specifications PG&E Gas and Electrical Off-Site Plans
Section 32 84 00 Landscape Irrigation System (For Backflow Preventor and installation) Appendix “B” Interior Color Schedule Plus Drawings
Appendix “C” Exterior Color Schedule Geotechnical Engineering Report

City of Fresno specification for sidewalks, curbs, gutters, drive approaches, asphalt paving, sewer, storm, water, patch backs, etc. for all work associated with the Off-Site Improvements.

General Items
1.	See General Notes at the beginning of the Summary of Work Specification Section for other items to be included in this Bid Package.
2.	Furnish and install all layout for own work from survey provided within this Bid Package. Prime Contractor will be responsible for all additional layout not performed by the survey contractor. Prime Contractors are responsible for protection of all requested survey. Any needed re-staking of already provided points will be subject to deductive change order.
3.	Provide all backfill of excavations to original sub-grade for work included in this bid package.
4.	Obtain all permits required to perform the work specified in the bid package. CM will submit the Dust Control plan to the Air Board. Prime Contractor will be responsible for all other permits required to perform the work identified. Prime Contractor will be responsible for dust control for their own work.
5.	Provide daily cleanup to keep site clean and orderly.
6.	Protect identified improvements to remain on civil plan sheets.
7.	Should the Prime Contractor damage and/or otherwise alter work installed under separate contracts, Prime Contractor shall be responsible for the correction/repair of work installed under separate contracts.
8.	Prime Contractor is required to attend all coordination meetings as required by CM.

88

Rebid- AD-1

9.	Phasing is projected to be as shown on the Bid Schedule. However, the Construction Manager reserves the right to revise the schedule, as necessary.
10.	Promptly submit written notice to CM of observed variance of Contract Documents from legal requirements.
a. Appropriate modifications to Contract Documents will adjust necessary changes.
b. Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
11.	Provide material, equipment, mobilizations, and manpower to meet Construction Schedule provided in Contract Documents.
12.	Each bid package is responsible for dewatering as it pertains to their scope of work.
13.	Provide trenching plan and permits for excavations over 5’ per OSHA requirements to the Construction Manager.
14.	Each Prime Contractor is to provide all equipment and manpower as necessary to offload all materials required to complete their respective scope of work.
15.	Monthly pay apps will not be approved if as-builts are not updated monthly.
16.	Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.
17.	There will be one wash out area as designated by CM. Bid package will be responsible for removal from the site of all construction debris generated by Prime Contractor’s work. Extra spoils to be stockpiled at the direction of CM.

18.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.
19.	Furnish clean up daily and off-haul of all debris generated by this contract. Prime Contractor must abide by the Waste Management specification. This includes, but is not limited to, providing recycling tags for each haul off removed from the project site.

20.	All construction equipment shall meet the requirements of the SJVAPCD ISR Report (Air Impact Assessment- AIA) under the Construction Fleet Summary. This shall include reporting requirements as defined within the Monitoring and Reporting Schedule within the ISR for this project.

21.	This contract is to provide temporary power for own work.

Coordination with Other Trades

1. This Prime Contractor will be responsible for the setup of SWPPP BMP’s, as shown in the SWPPP plan drawings for all Off-Site work areas including but not limited to, silt fencing, track outs and fiber rolls surrounding existing drain inlets.
2. Allow for twoadditional mobilizations for movement orrelocationof track outs as requiredduring construction.
3. Any survey requests require a minimum of 48-hour notice.
4. Coordinate dimensions with other related Prime Contractors.
5. Coordinate installation of all sleeves for work passing through concrete work with respective Prime Contractors prior to excavation.
6. Review as-builts prior to starting work.

89

Rebid- AD-1

Furnish and install items
1. Furnish and install all off-site improvements for water, sewer, storm. All utilities will be brought on to the site as shown for connection by site utilities contractor, or to the location provided by the site utilities contractor, should that scope of work be installed prior.
2. Furnish and install all Surveying for all Off Site improvements.

3. Furnish and install all back flow and Detector Check Valves for fire and domestic water entering the site.
4. Furnish and install all Off-Site irrigation back flow preventors. 5. Furnish and install all Off-Site Fire Hydrants.
6. Furnish and install all offsite piping and connections for water, sewer, storm, and gas. 7. Furnish and install all gas on to site, ready for meter assembly.
8. Furnish and install all PG&E utilities work per plans.

9. Furnish and install all street lighting, traffic lighting, controls, connections, complete. 10. Furnish and install all trail and lighting complete.
11. Furnish and install all cut, patch back, grading and paving of roadways per Off-Site improvement plans, and for water tie-in along Weldon Ave for Fire Water, including back flow device.
12. Furnish and install all curb, gutter, sidewalks, trail, lighting, per Off-Site drawings, including those shown in the attached highlighted site plan sketch, to help show separation from project Site Concrete Bid Package.
13. Furnish and install all off-site landscape irrigation and planting complete.

90

Rebid- AD-1

91