No. C23724

PROJECT:

ADDENDUM NO. 4	.......................................................................................................DATE: 02/11/2022 PAGE 2

PROJECT:

ADDENDUM NO. 4...........................................................................................................DATE: 02/11/2022 PAGE 3

“Add Alternate 1 Revisions

The Alternate Shade Structure has been deleted from the project and is no longer part of Add Alternative 1. The base Bid Shade Structure will be the only shade structure considered. Add Alternative 1 will now be the Dive Tower Demolition”

2. Alternate Bid 1: Demolition of Dive Tower

PROJECT:

ADDENDUM NO. 4...........................................................................................................DATE: 02/11/2022 PAGE 4

ALTERNATE BID NO. 1: Demolition of Dive Tower a.	BASE BID: Leave the dive tower, protect.
b.	ALTERNATE BID: Remove the dive tower, and all .”

“1. Perforated Panels (Type 1 ):
a. Manufacturer: DIAMOND PERFORATED PANELS.
b. Quantity: Continuous Sheet with no joints, curved to profile on drawings. c. Material: Carbon Steel, Hot-Dipped Galvanized after Fabrication.
d. Thickness: 3/16".
e. Width and Length: 48" x 120".
f. Perforation: 1/4" dia. With 1/2 inch staggered centers, 30% open area. g. Panel Ends and Edges: 1" margin at perimeter with hemmed edges. h. Hot Dipped Galvanized after fabrication of panels.”

“1. Perforated Panels (Type 1 ):
a. Manufacturer: DIAMOND PERFORATED PANELS.
b. Quantity: Continuous Sheet with no joints, curved to profile on drawings. c. Material: Carbon Steel, Powder Coated.
d. Thickness: 3/16".
e. Width and Length: 48" x 120".
f. Perforation: Custom hole pattern to fit Architects design.
g. Panel Ends and Edges: 1" margin at perimeter with hemmed edges. h. Powder Coated after fabrication of panels.”

“ADDITIVE ALTERNATE BID 1: DEMOLITION OF DIVE TOWER
•	Demolition of the Concrete Columns, Spiral Stairs, and all other elements of the 10M Concrete Dive tower. “

PROJECT:

ADDENDUM NO. 4...........................................................................................................DATE: 02/11/2022 PAGE 5

“31. REMOVE EXISTING SURFACE CONDUIT AT HARDSCAPE AND RUN NEW 1-1/2"C. 6#12,1#12G. UNDERGROUND FROM POWER PANEL TO SCOREBOARD. RECONNECT SCOREBOARD AND OUTLETS. SAW-CUT AND REPLACE EXISTING CONCRETE AS REQUIRED.”

“31. EXISITING POWER CONDUIT TO REMAIN.”

“18A. EXISTING CONDUIT TO REMAIN. EXTEND TO NEW PULLBOX AS REQUIRED. CONNECT SCOREBOARD WITH 6-STR FIBER OPTIC CABLE.”

“1. PLASTER TO REMAIN”

3.

“1. RE-PLASTER ENTIRE TEACHING POOL”

AD4

AD4

AD4

AD4

AD4

AD4

AD4 REVISED PROPOSAL FORM FOR BID 2875

Date	, 2022

Company Name ____________________________________________________

Bid Package Number and Title__________________________________________

CLOVIS UNIFIED SCHOOL DISTRICT PURCHASING
1450 HERNDON CLOVIS, CALIFORNIA 93611

The undersigned doing business under the firm name of _______________________________________ hereby propose and agree to enter into an agreement, to furnish any and all labor, materials, equipment, and services for the completion of work described hereinafter and in the contract documents entitled construction of:
CLOVIS WEST HIGH SCHOOL SWIMMING POOL RENOVATION

for the sum(s) quoted below.

Base Bid__________________________________________________	Dollars $________________

If written notice of the acceptance of this bid is mailed, telegraphed, or delivered to the undersigned within sixty (60) days after the date of opening of the bids, or any time thereafter before this bid is withdrawn, the undersigned will, within ten (10) days after the date of such mailing, telegraphing, or delivering of such notice, execute and deliver a contract in the form of agreement present in these contract documents and give Performance and Payment Bonds in accordance with the specifications and bid as accepted.

The undersigned hereby designates as the office to which such notice of acceptance may be mailed, telegraphed, or delivered:

Our Public Liability and Property Damage Insurance is placed with:

Our Workers’ Compensation Insurance is placed with:

The following must be completed without exception:

1.	Name of Foreman / Superintendent for this Project 	

2.	Acknowledge receipt and review of full set of bid documents 	(Initial)

3.	Crewing for this Project - Minimum Crew 	Maximum Crew 	

4.	Summary of Work has been reviewed and is included 	(Initial)

AD4

5.	Bid Schedule has been reviewed and accepted 	(Initial)

6.	The following items are attached to this bid form
a. Bid Bond	                  (Initial) b. Non-Collusion Affidavit	                  (Initial) c. Subcontractor Listing	                  (Initial) d. Job References	                  (Initial) e. Insurance Rating Submittal form	                  (Initial) f.	Student Safety Declaration	                  (Initial)

7.	Proper Prevailing wages included in this bid	                  (Initial)
*2015-2018 requirements for Certified Payroll Reporting is acknowledged.

Circular letters, bulletins, addenda, etc., bound with specifications or issued during the time of bidding are included in the proposal, and, in completing the contract, they are to become part thereof.

The receipt of the following addenda to the specifications is acknowledged:

Addendum No. 	Dated:

Addendum No.	Dated:

Addendum No. 	Dated:

Addendum No. 	Dated:

Note: Any exclusion to the scope of work or items noted in this bid form will be considered as cause to deem this bid non-responsive.

This bid may be withdrawn at any time prior to the scheduled time for the opening of bids or any authorized postponement thereof.

NOTE:	 Each bid must give the full business address of the bidder and be signed by him with his usual signature. Bids by partnerships must furnish the full name of all partners and must be signed by one of the members of the partnership, or by an authorized representative, followed by the signature and designation of the person signing. Bid by corporations must be signed with the legal name of the corporation, followed by the name of the state of incorporation and by the signature and designation of the president, secretary, or other person authorized to bind it in the matter. The name of each person signing shall also be typed or printed below the signature. Satisfactory evidence of the authority of the officer signing on behalf of a corporation shall be furnished.

Dated 	, 2022

Signed 	

Print or Type Name 	

Business Address

Phone #

Fax #

License #

Email Address to send contracts 	

DIR NUMBER_____________________________

Additional Signature Lines if Applicable:

AD4

Signed 	

Print or Type Name 	

Business Address

Signed 	

Print or Type Name 	

Business Address

Signed 	

Print or Type Name 	

Business Address

State of Incorporation if Applicable  

( )	Evidence of authority to bind corporation is attached.

Print or Type Name 	

Business Address

Phone Number: 	

FAX Number: 	

Contractor's License Number 	

Email Address 	

82"
82"
wall.
	
MC
	-1

		
	MC
	-2

		
	MC
	-3

MCM
	-1

		
	MCM
	-2

		
	MCM
	-3
		
Project
2/10/2022 4:48:17 PM
E:\Users\andrewv\Documents\1944_CWHS_Aquatics_Improvments_V18_andrewv.rvt
1	2	3	4	5	6	7	8	9	10	11	12	13	14	15	16	17	18	19	20

R	A.A	A.B	A.C

35' - 0" TOS

J1

DSA File No.: 10-H3

R

DSA Application No.: 02-119318
Agency Approval

EXTERIOR COLOR LEGEND

SD/A203 Q

P

N

NORTH

STEEL AND FABRICATIONS, Steel, Column. See Structural.

20' - 0" TOS

0'-0" F.F.

Metal Colors	            MCM Colors	

XXX	XXX
Unless Noted Otherwise	Unless Noted Otherwise

XXX	XXX

XXX	XXX

All Hollow Metal Frames to be match adjacent All MCM Panels to be MCM-1, UNO.

All Steel and Fabrications to match adjacent wall, UNO.
All METAL DECKING to be MC-1, UNO. All Metal columns to be MC-1, UNO.

Metal Panel Colors

XXX
Unless Noted Otherwise

XXX
	
MP
	-1

	MP
	-2

		
XXX
	
	MP
	-3

Q

P

N

M	A1	A2	A3	A4	A5	A6	A7	A8	A9	A10

J7

SD/A203

Color Notes	                      M

XX-
	X
	
1.	Color Designation.	4.	Horizontal soffits adjacent to fascia 2.           Parapet caps to match                        board shall be PC-1.
color of wall below, UNO.	Fascia Board

3.	Soffits to match color of	PC-1 outer face wall, UNO.

L

		O
S In

			

uter Face Wall

offit	L ner Face Wall

														

			

AST

																																	

																																	

																																												

																																				

E

																																													

SYMBOLS

ELECTRICAL, Horn	Glass

ELECTRICAL, Speaker

ELECTRICAL, Outlet

K

0'-0" F.F.

J

A.C	A.B	A.A	35' - 0" TOS

H

ELECTRICAL, Light Fixture, +10'-0" B.O. Fixture UNO

ABBREVIATIONS

AFF        Above Finished Floor BO	Bottom of
CJ           Control Joint DS          Downspout
EJ	Expansion Joint

HB	PLUMBING, Hose Bibb. OH	Opposite Hand
Sim.        Similar TO          Top of
TOM       Top of Masonry

TOP        Top of Parapet Framing TOF        Top of Framing
TOR        Top of Roof TOS        Top of Steel TPL	Top of Plate Typ.        Typical
UNO       Unless Noted Otherwise

NOTES

K

J

H

	
STEEL AND FABRICATIONS, Steel,
						
Column. See Structural.

								

						

								

3.	Refer to Specifications Section Appendix "C" Exterior Color Schedule.

4.	Refer to Exterior Finish Schedule on Sheet X/A201.

G

E18

No Scale

GCeneral Notes	G Exterior Elevations Legend

F	F

0'-0" F.F.

SOUTH

E	Consultant	E

A10	A9	A8	A7	A6	A5	A4	A3	A2	A1 35' - 0" TOS

Clovis West High School - Aquatic Improvements Clovis Unified School District
1070 E Teague Ave. Fresno, CA 93720

D

J8 SD/A207

J7

SD/A203

SHADE STRUCTURE ELEVATIONS		D Drawing

20' - 0" TOS

C

STEEL AND FABRICATIONS, Steel, Column. See Structural

B

4

STEEL AND FABRICATIONS, Perforated Panel, Type 1, 3/16" x 48" x 120" Panels with Custom Perforation. Attach with #12 TEK @ 12" O.C.

ELECTRICAL, Pool Clock, See Electrical, Typ

Architect

No.	Revision/Submission

4	AD4

No. C23724	C

Date 02/11/22

B

0'-0" F.F.

WEST	DesignedDesigner

Revision

Copyright 2021 Darden Architects

A 	 Scale:	As indicated     Drawn By: Author

A1	Exterior Elevations	Project Number:     1944 Checked BChecker

SD/A206	A

1/8" = 1'-0"	Date:	02/04/2022 ReviewedApprover	Sheet: 	         of: 	

1	2	3	4	5	6	7	8	9	10	11	12	13	14	15	16	17	18	19	20

AD4-AX01