ADDENDUM NO. 01

PROJECT:

Clovis West High School Classroom Wing 1070 East Teague Ave.
Fresno, CA

CLIENT:

Clovis Unified School District 1450 Herndon Ave.
Clovis, CA 93611

Date :

TETER Project No.:

Client Project No.: DSA File No.:
DSA Appl. No.:

09/23/2021

A 21-11972 D

2864 10-H3
02-119258

The following additions, deletions and revisions to the plans, specifications and Addenda shall become a part of the plans and specifications. It is the responsibility of the General Contractor to submit the information contained in this addendum to all subcontractors and suppliers.	The Bidder shall acknowledge receipt of the Addendum in the Bid Proposal. (Addendum number of pages: 1 pages + 4 attachments = 61 total pages).

PROJECT MANUAL:

1 – 01:	PROJECT MANUAL, DIVISION 00 – “CONTRACT REQUIREMENTS”, revise as follows:

A. Add “BID PACKAGE FOR BID 2864” to the project specifications (40 Pages).

1 – 01:	PROJECT MANUAL, SPECIFICATION SECTION 011100 – “SUMMARY OF WORK”, revise as follows:

B. Remove and Replace with attached Specification 011100 – “SUMMARY OF WORK” (5 Pages).

1 – 01:	PROJECT MANUAL, SPECIFICATION SECTION 088000 – “GLAZING”, revise as follows:

A. Remove and Replace with attached Specification 088000 – “GLAZING” (12 Pages).

1 – 02:	PROJECT MANUAL, SPECIFICATION – “SCHEDULE”, revise as follows:

A. Remove and Replace with attached Specification – “SCHEDULE” (3 Pages).

Aya Shitanishi Architect of Record

J:\119\11972 Clovis USD - Clovis West Classroom Wing\D-Bidding & CA\Bidding\Addenda\Addendum 01 Storefront\Bid 2864 Addendum 01 Draft.doc

CLOVIS UNIFIED SCHOOL DISTRICT

BID PACKAGE FOR

BID 2864

CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

Eimear O’Farrell, Ed.D. Superintendent

Clovis Unified School District 1450 Herndon Avenue Clovis, California 93611 (559) 327-9475

CLOVIS UNIFIED SCHOOL DISTRICT

BIDDING PACKAGE TABLE OF CONTENTS

DESCRIPTION

1. Notice To Contractors 2. Instructions To Bidders

3. To be included with bid on bid day

a. Bid Proposal Form b. Bid Bond Form
c. Non-Collusion Affidavit d. List of Sub-Contractors e. Job References
f. Insurance Rating Submittal Form g. DVBE Good Faith Declaration
h. Student Safety Declaration
i. Health Screen Requirements
j. Federal Procurement Requirements

4. To be submitted after bid by Low contractor

a. Payment and Performance Bonds

5. Sample Agreement

6. Addenda

7. General Conditions

8. Specifications

9. Drawings

NOTICE TO CONTRACTORS

Notice is hereby given that CLOVIS UNIFIED SCHOOL DISTRICT, (hereinafter referred to as "Owner") will receive sealed bids prior to the date and time stated for the Bid Opening for construction of:

BID 2864 – CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

as per drawings and specifications which may be obtained from the Construction Manager:

MARK WILSON CONSTRUCTION 5799 E CLINTON AVENUE FRESNO, CALIFORNIA 93727 (559) 348-0421

Upon receipt of the contract documents provide the following information: 1.      Organization/Contact Person for each Prime Contractor
2.	Mailing address and P.O. Box Number for each Prime Contractor 3.	Phone Number for each Prime Contractor
4.	FAX Number for each Prime Contractor

The project will be bid as multiple prime contracts according to the list below:

Bid Form Bid

Package #
	Bid Package

Description
	Contractor License

Requirement
	
CWHS-02
	ALUMINUM STOREFRONT
	C17

A job walk is not scheduled for this project.

Time of completion for this project shall 310 calendar days (per construction manager’s work schedule) from the start of the project as established within the Owner’s Notice to Proceed. All procurement, coordination, milestones, durations, activities and sequences for the bid packages shall be performed as shown in the Construction Management Bid Schedule and Section 01320 of the specification and as modified by a monthly schedule update, if any.

Bids will be sealed and filed at the following address: Bids will NOT be accepted at the bid opening location.
Clovis Unified School District PURCHASING
1450 Herndon Avenue Clovis, California 93611
before 11:00 a.m. on September 29, 2021

Bids will be opened in public at the following address: Bids will NOT be accepted at the bid opening location.
Clovis Unified School District CONSTRUCTION SERVICES OFFICE 1470 Herndon Avenue Clovis, California 93611

The DVBE Declaration of Good Faith Efforts to use Disabled Veteran Business Enterprises must be signed and filed in the Clovis Unified School District Construction Services Office located at 1470 Herndon Avenue, Clovis, California, before 11:00 am on September 29, 2021, at which time the bids (including the DVBE Declaration of Good Faith Efforts to Use Disabled Veteran Business Enterprises) will be opened in public – include with bid packet.

Bids must be accompanied by a bidder's bond, cashier's check, or certified check for at least ten per cent (10%) of the amount of the base bid and made payable to the Owner, issued by an Admitted Surety (an insurance organization authorized by the Insurance Commissioner to transact business of insurance in the State of California during this calendar year), which shall be given as a guarantee that the bidder will enter

into a contract if awarded the work and will be declared forfeited, paid to, or retained by the Owner as liquidated damages if the bidder refuses or neglects to enter into the contract provided by the Owner after being requested to do so.

The Contractor shall be required to satisfy the conditions set forth in the contract and Education Code section 45125.2 regarding fingerprinting requirements and student safety prior to permitting any contact with students. Upon award of the contract and before beginning work, the Contractor shall be required to provide a verification of compliance with the student safety provisions of the contract and Education Code section 45125.2.

Upon award of the bid, require signature on the enclosed declaration to ensure compliance with the general Conditions and the Education Code.

The successful bidder will be required to furnish a Payment (Labor and Material) Bond in the amount of one hundred per cent (100%) of the contract price, and a Faithful Performance Bond in the amount of one hundred per cent (100%) of the contract price, said bonds to be secured from an Admitted Surety (an insurance organization authorized by the Insurance Commissioner to transact business of insurance in the State of California during this calendar year), and satisfactory to the Owner. The bidder will be required to give satisfactory proof to the Owner of the maintenance of Public Liability and Property Damage Insurance in an amount with a combined single limit of not less than $2,000,000 per occurrence.

The successful bidder will be allowed to substitute securities or establish an escrow in lieu of retainage, pursuant to Public Contract Code Section 22300, and as described in the General Conditions.

The Owner will not consider or accept any bids from contractors who are not licensed to do business in the State of California, in accordance with the California Public Contract Code, providing for the licensing of contractors. In accordance with Section 3300 of said Code, the Contractor shall have a license classification as described in the MULTIPLE PRIME CONTRACT SCHEDULE.

Pursuant to Labor Code sections 1725.5 and 1771.1, all contractors and subcontractors that wish to bid on, be listed in a bid proposal, or enter into a contract to perform public work must be registered with the Department of Industrial Relations. No bid will be accepted nor any contract entered into without proof of the contractor’s and subcontractors’ current registration with the Department of Industrial Relations to perform public work. If awarded a Contract, the Bidder and its subcontractors, of any tier, shall maintain active registration with the Department of Industrial Relations for the duration of the Project.

This Project is subject to compliance monitoring and enforcement by the Department of Industrial Relations. In bidding on this project, it shall be the Bidder’s sole responsibility to evaluate and include the cost of complying with all labor compliance requirements under this contract and applicable law in its bid.

The lowest bid shall be determined as follows: The lowest total of the prime bid on the base contract and the bids on all additive items and all deductive items. (Public Contract Code section 20103.8, subd. (b)). The District reserves the right to add or deduct any of the additive or deductive items from the project or contract after the lowest responsible and responsive bidder is determined.

The Director of the Department of Industrial Relations of the State of California, in the manner provided by law, has ascertained the general prevailing rate per diem wages and rate for legal holidays and overtime work as set forth in the Agreement. The Contractor must pay for any labor therein described or classified in an amount not less than rates specified. Copies of the required rates are on file at the Owner's business office and are available to any interested party on request.

The Owner reserves the right to waive any irregularity and to reject any or all bids.

Unless otherwise required by law, no bidder may withdraw its bid for a period of sixty (60) days after date set for the opening thereof.

Dated: Advertise:

September 15, 2021 September 15, 2021 September 20, 2021

Clovis Unified School District By: MICHAEL JOHNSTON
ASSISTANT SUPT OF BUSINESS SERVICES

INSTRUCTIONS TO BIDDERS

SECURING DOCUMENTS:
Drawings and Specifications are available at:
MARK WILSON CONSTRUCTION 5799 E CLINTON AVENUE FRESNO, CALIFORNIA 93727 (559) 348-0421
DEPOSIT: None Required

Pre Bid Meeting or Job Walk is not scheduled for this project

PROPOSALS:

Proposals to receive consideration shall be made in accordance with the following instructions:

1.	 Proposals shall be made on a form therefor, obtained from the Construction Manager or Architect or Owner. Bids not made on the proper form shall be disregarded. Numbers must be stated in words and figures, and the signatures of all individuals must be in longhand. The completed form should be without interlineation, alterations, or erasures.

2.	 No proposal will be considered which makes exceptions, changes, or in any manner makes reservations to the terms of the drawings or specifications, except that explanations or alternate proposals may be made on a separate sheet attached to the bid form. They will not, however, be considered in determining low bid.

3.	 Questions regarding documents, discrepancies, omissions, or doubt as to meanings shall be referred immediately to the Architect who will send written instructions clarifying such questions to each bidder.

4.	 Each bid must give the full business address of the bidder, and the name of each person signing shall also be typed or printed below the signature. Bids by individuals must be signed by the individual. Bids by partnerships must furnish the full names of all partners and must be signed in the partnership name by one of the partners, or by an authorized representative, followed by the signature and designation of the person signing. Bid by corporations must be signed with the legal name of the corporation, followed by the name of the state of incorporation and by the signature and designation of the president, secretary, or other person authorized to bind the corporation in the matter. Satisfactory evidence of the authority of the officer signing on behalf of a corporation shall be attached.

5.	 Pursuant to the provisions of Sections 4100 to 4114, inclusive, of the Public Contract Code of the State of California, which are hereby incorporated and made a part hereof, every bidder shall set forth in its bid:

A.	 The name and location of the place of business of each subcontractor who will perform work or labor or render service to the bidder in or about the construction of the work or improvement, or a subcontractor licensed by the State of California who, under subcontract to the bidder, specially fabricates and installs a portion of the work or improvement according to detailed drawings contained in the plans and specifications, in an amount in excess of one-half (1/2) of one percent (1%) of the bidder's total bid.

B.	 The portion of the work which will be done by each such subcontractor. If the bidder fails to specify a subcontractor for any portion of the work to be performed under the contract in excess of one-half (1/2) of one percent (1%) of the bidder's total bid, the bidder agrees to perform that portion itself. The successful bidder shall not, without the consent of the Owner:

1)	 Substitute any person as subcontractor in place of the subcontractor designated in the original bid.

2)	 Permit any subcontract to be assigned or transferred or allow it to be performed by anyone other than the original subcontractor listed in the bid.

3)       Sublet or subcontract any portion of the work in excess of one-half (1/2) of one percent (1%) of the total bid as to which the original bid did not designate a subcontractor.

6.	 The Director of the Department of Industrial Relations of the State of California, in the manner provided by law, has ascertained the general prevailing rate of per diem wages and rate for legal holidays and overtime work as set forth in Article IX of the Agreement. The Contractor must pay for any labor therein described or classified in an amount not less than the rates specified. Copies of the required rates are on file at the Owner’s business office and are available to any interested party on request.

Pursuant to Labor Code sections 1725.5 and 1771.1, all contractors and subcontractors that wish to bid on, be listed in a bid proposal, or enter into a contract to perform public work must be registered with the Department of Industrial Relations. No bid will be accepted nor any contract entered into without proof of the contractor’s and subcontractors’ current registration with the Department of Industrial Relations to perform public work. If awarded a Contract, the Bidder and its subcontractors, of any tier, shall maintain active registration with the Department of Industrial Relations for the duration of the Project. To this end, Bidder shall sign and submit with its Bid the Public Works Contractor Registration Certification on the form provided, attesting to the facts contained therein. Failure to submit this form may render the Bid non-responsive. In addition, each Bidder shall provide the registration number for each listed subcontractor in the space provided in the Designation of Subcontractors Form.

7.	All proposals must be accompanied by a completed Noncollusion Declaration. The bidder must certify that the Bid is genuine and is not sham or collusive, or made in the interest of or on behalf of any bidder not named in the bid, and that the bidder has not directly or indirectly induced or solicited any other bidder to put in a sham bid, or any other possible bidder to refrain from bidding, and that the bidder has not in any manner sought by collusion to secure for itself an advantage over any other bidder.

8.	 Proposals must be accompanied by a certified check, cashier's check, or bidder's bond, for an amount not less than ten percent (10%) of the amount of the base bid, made payable to the order of the Owner. If a bidder's bond accompanies the proposal, said bond shall be secured by an Admitted Surety (an insurance organization authorized by the Insurance Commissioner to transact business of insurance in the State of California during this calendar year) and satisfactory to the Owner. Said check or bond shall be given as a guarantee that the bidder will enter into the contract if awarded the work, and in case of refusal or failure to enter into said contract, the check or bond, as the case may be, shall be payable to the Owner and retained as liquidated damages.

9.	 Proposals shall be sealed and filed as indicated in the Notice to Contractors. Note regarding facsimiles: EXCEPT FOR BID SECURITY, all submitted before the bid opening documents may be in the form of facsimiles which have been sent elsewhere and sealed before filing with the Owner. (Any bidder who uses or attempts to use the Owner’s facsimile equipment will be disqualified immediately.) The originals of the faxed documents must be mailed to the Owner, postmarked the same as the bid opening, via certified mail, return receipt requested, or hand-delivered to the Owner by the close of business on the day of the bid opening.

Facsimiles of the bid security are not acceptable - the original of the check or bond must be submitted before the bid opening.

10.	 Bidders shall possess a valid California Contractors License as listed in the Notice to Bidders. A General Building Contractors License (B) shall be acceptable in accordance with the California Business and Professional Code Section 7057, paragraph (b): A general building contractor may take a prime contract or a subcontract for framing or carpentry project. However, a general building contractor shall not take a prime contract for any project involving trades other than framing or carpentry unless the prime contract requires at least two unrelated building trades or crafts other than framing or carpentry, or unless the general building contractor holds the appropriate specialty

license or subcontracts with an appropriately licensed specialty contractor to perform the work. Owner reserves the right to reject any bid as nonresponsive if a listed subcontractor is not licensed at the time the bidder’s bid is submitted to Owner, whether or not the bidder listed the unlicensed subcontractor inadvertently. Owner reserves the right to reject any bid as nonresponsive is a listed subcontractor is not licensed to perform the work for which it is listed at the time the bidder’s bid is submitted to Owner, whether or not the bidder listed the subcontractor for that particular work inadvertently

WITHDRAWAL OF PROPOSALS:

Proposals may be withdrawn by the bidder prior to the time fixed for the submittal of bids. A successful bidder shall not be relieved of the bid unless by consent of the Owner or bidder's recourse to Public Contract Code § 5100 et seq.

OPENING OF PROPOSALS:

Opening of proposals shall be as soon after the hour set as will be possible; opening and declaration to be as set forth in the Notice to Contractors. Any and all bidders will be permitted to attend. The Owner is allowed the number of days set forth in the Notice to Contractors in which to determine low bidder.

EXAMINATION OF CONTRACT DOCUMENTS AND SITE:

Before submitting a proposal, bidders shall examine the drawings, read the specifications, the form of contract, and other contract documents. They shall visit the site of the proposed work; examine the building, or buildings, if any, and any work that may have been done thereon. They shall fully inform themselves of all conditions, in, at, and about the site, the building or buildings, if any, and any work that may have been done thereon.

FORM OF CONTRACT:

The form of contract which the successful bidder will be required to execute, if awarded the work, is attached hereto and is made a part hereof.

ADDENDA OR BULLETINS:

Any addenda or bulletins, issued during the time of bidding, shall form a part of the drawings and specifications loaned to the bidder for the preparation of its proposal, shall be covered in the proposal, and shall be made a part of the Contract Documents. All addenda or bulletins shall be signed by the Architect and approved by the Division of State Architect.
AWARD OF CONTRACT:

Rejection of any or all proposals, to contract work with whomever and in whatever manner, to abandon work entirely, and/or to waive any informality in receiving of bids is reserved as the right of the Owner. Before the contract or contracts are awarded, the Owner may at its sole discretion require from the proposed Contractor on each project further evidence of the reasonable qualifications of such contractor to faithfully, capably, and reasonably perform such proposed contract and may consider such evidence before making its decision on the award of such proposed contract.

The lowest bid shall be determined as follows: The lowest total of the prime bid on the base contract and the bids on all additive items and all deductive items. The District reserves the right to add or deduct any of the additive or deductive items from the project or contract after the lowest responsible and responsive bidder is determined.
The contract shall be awarded to the lowest and most responsible bidder as interpreted by the Owner and specified herein and shall be entered into by the successful bidder within ten (10) days after being notified by the Owner. Identity of lowest bidder will be determined by adding to or subtracting from the base bid the cost of such alternatives as Owner decides to include in the work and contract. The award, if made, will be made within sixty (60) days after the opening of proposals.

EXECUTION OF CONTRACT:

The Contract shall be signed by the successful bidder in as many originals as the Owner deems necessary and returned, together with the contract bonds and insurance certificates, within ten (10) days after the bidder has received notice that the contract has been awarded.

CONTRACT BONDS:

Two bonds, as itemized below and in the forms presented in these contract documents, shall be furnished by the successful bidder at the time of entering into the contract and filed with the Owner. They shall be in the form of surety bonds issued by an Admitted Surety (an insurance organization authorized by the Insurance Commissioner to transact business of insurance in the State of California during this calendar year) and satisfactory to the Owner.

Performance Bond in the amount of one hundred percent (100%) of the contract sum to insure Owner during construction and for one year after completion against faulty or improper materials or workmanship and to assure Owner of full and prompt performance of the contract.

Payment Bond (Labor and Material) in the amount of one hundred percent (100%) of the contract sum in accordance with the laws of the State of California to secure payment of any and all claims for labor and materials used or consumed in performance of this contract.

DRAWINGS, SPECIFICATIONS AND ADDENDA OR BULLETINS:

Return by each bidder of all drawings, specifications and addenda or bulletins in an unmutilated condition and without any marks or annotations is demanded within the time limit indicated under DEPOSIT in this section.

SUBSTITUTION OF MATERIALS:

All materials are mentioned as standards. Should a Contractor desire to substitute materials or methods for those specified, the Contractor shall follow the guidelines stated herein, and in accordance with Section 01-640. Each review of a substitution request by the Architect or its consultants will be billed to the Contractor at an hourly rate as indicated in Section 01-640.

Substitutions can be submitted in two ways: (1) Prior to Bid Opening, and (2) After Award of the Contract. Either submittal of substitutions is further described herein and must conform to the requirements indicated.

(1)	Prior to Bid Opening: The Contractor must insure that proposed substitutions of materials by the Contractor or its subcontractors are submitted to the Architect's office a minimum of fourteen (14) calendar days prior to the Bid Opening for review and possible approval of any equipment or materials thought to be equal to or better than those specified in the drawings or specifications. An Addendum will be issued seven (7) calendar days prior to Bid Opening including all equipment and materials deemed equivalent to those specified and approved by the Architect. Submittals must include comparative spec-data of that specified equipment or material and the proposed substitution as indicated on the completed "Substitution Request Form" in accordance with Section 01-640. Submittals without this information will be automatically rejected.

(2)	After Award of the Contract: In accordance with the provisions of Section 3400 of the California Public Contract Code, the Contractor awarded the Contract will be provided a period of (40) calendar days after the award of the Contract for submission of data substantiating a request for a substitution of "an equal" item or items. Substitution requests must be made as provided in Article 3.11.4 of the General Conditions.

PAYMENTS:

Payments to the Contractor on account of the contract shall be made in accordance with the terms of the contract.

TAXES:

The Owner is exempt from payment of Federal Excise Tax on materials. The Owner will furnish exemption certificates to the Contractor to be used to obtain materials ordinarily subject to Federal Excise Tax without payment of the tax. Bidders shall deduct Federal Excise Taxes from their bid prices before submitting bids, so that such taxes will not be included in the Contract Sum.

TIME OF COMPLETION AND LIQUIDATED DAMAGES:

Time of completion for this project shall 310 calendar days (per construction manager’s work schedule) from the start of the project as established within the Owner’s Notice to Proceed. All procurement, coordination, milestones, durations, activities and sequences for the bid packages shall be performed as shown in the Construction Management Bid Schedule and Section 01320 of the specification and as modified by a monthly schedule update, if any.

Should said work not be completed within the time limit as may be extended as herein provided, damages will be sustained by the Owner. It is understood and agreed that it is and will be impracticable or extremely difficult to determine the actual amount of damages which the Owner will sustain in the event of and by reason of such delay, and it is therefore agreed that the Contractor will pay the Owner the sum of One Thousand ($1,000.00) Dollars per calendar for each and every day's delay beyond the time specified as and for liquidated damages; in case the Contractor fails to make such payment, the Owner may deduct the amount thereof from any money due or that may become due the Contractor under the contract. Should such money not be sufficient to cover the agreed liquidated damages, the Owner shall have the right to recover the balance from the Contractor or his sureties.

The Contractor shall be required to satisfy the conditions set forth in the contract and Education Code section 45125.2 regarding fingerprinting requirements and student safety prior to permitting any contact with students. Upon award of the contract and before beginning work, the Contractor shall be required to provide a verification of compliance with the student safety provisions of the contract and Education Code section 45125.2.

Upon award of the bid, require signature on the enclosed declaration to ensure compliance with the general Conditions and the Education Code.

The bid is subject to DVBE requirements.

END OF SECTION REV. 3.97 (8.98)

CALIFORNIA SENATE BILL 854 (2014) – APPLIES TO THIS BID PROJECT

Senate Bill 854, signed into law June 20, 2014, became effectively immediately. It established a new public works contractor registration program which will collect fees to fund compliance monitoring and enforcement, determine prevailing wage and public works coverage, and hear enforcement appeals.

All contractors and subcontractors intending to bid or perform work on public works projects will be required to register, and annually renew, online for the program. The cost to register for the program is currently $400.00 and is non-refundable. This is a DIR fee paid to the State. The District will not register a contractor, nor collect funds.

Contractors or subcontractors submitting bids must be registered by March 1, 2015. The requirement to use only registered contractors and subcontractors on public works projects, greater than $1,000, applies to all projects awarded on or after April 1, 2015. No bid can be accepted nor any contract or subcontract entered into nor purchase order issued without proof that the contractor or subcontractor is registered.

Public works refers to construction, alteration, demolition, installation, or repair work (including maintenance) done under contract and paid by public funds. For a more detailed explanation of public works projects, refer to California Labor Code 1720 -1720.6.

This memo is being sent to all vendors currently contracted with the District’s Plant Operations and/or Construction Department. What are we asking you to do? If the services you are providing the District, or may provide the District in the future, fall under the definition of “public works”, please ensure you are registered with the DIR prior to March 1, 2015. Effective immediately, the District will be required to fill out a form alerting the DIR of the services you are providing the District. Detailed information is required to complete this form. If the services you are currently providing the District fall under “public works” you may be asked to provide information needed to complete the DIR form. We ask that you complete this in a timely manner to avoid interruption in the services you are providing.

More	information	can	be	found	at	The	Department	of	Industrial	Relations	website; http://www.dir.ca.gov/Public-Works/PublicWorks.html.

Effective July 1, 2018, Senate Bill 96 (SB96) increased the thresholds for submitting a PWC-100 form to DIR. The $1,000 threshold was increased to $25,000 for Construction Project and $15,000 for Maintenance Projects. Public Contract Code defines Construction and Maintenance. These terms are not defined by the contractor or the district.

Please note – Contractors are required to pay prevailing wage on ALL projects exceeding $1,000 and are subject to DIR audit and public record requests on all work provided for a public agency. Contractors are required to keep certified records on file for all work performed for a public agency.

The District may require PWC-100 submittal for amounts lower than those stated in SB96.

PROPOSAL FORM FOR BID 2864

Date	, 2021

Company Name ____________________________________________________

Bid Package Number and Title__________________________________________

CLOVIS UNIFIED SCHOOL DISTRICT PURCHASING
1450 HERNDON CLOVIS, CALIFORNIA 93611

The undersigned doing business under the firm name of _______________________________________ hereby propose and agree to enter into an agreement, to furnish any and all labor, materials, equipment and services for the completion of work described hereinafter and in the contract documents entitled construction of:

CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

for the sum(s) quoted below.

Base Bid___________________________________________	Dollars $________________

If written notice of the acceptance of this bid is mailed, telegraphed, or delivered to the undersigned within sixty (60) days after the date of opening of the bids, or any time thereafter before this bid is withdrawn, the undersigned will, within ten (10) days after the date of such mailing, telegraphing, or delivering of such notice, execute and deliver a contract in the form of agreement present in these contract documents and give Performance and Payment Bonds in accordance with the specifications and bid as accepted.

The undersigned hereby designates as the office to which such notice of acceptance may be mailed, telegraphed, or delivered:

Our Public Liability and Property Damage Insurance is placed with:

Our Workers’ Compensation Insurance is placed with:

The following must be completed without exception:

1.	Name of Foreman / Superintendent for this Project 	

2.	Acknowledge receipt and review of full set of bid documents 	(Initial)

3.	Crewing for this Project - Minimum Crew 	Maximum Crew 	

4.	Summary of Work has been reviewed and is included 	(Initial)

5.	Bid Schedule has been reviewed and accepted 	(Initial)

6.	The following items are attached to this bid form
a. Bid Bond	                  (Initial) b. Non Collusion Affidavit	                  (Initial) c. Subcontractor Listing	                  (Initial) d. Job References	                  (Initial) e. Insurance Rating Submittal form	                  (Initial) f.	DVBE Good Faith Effort	                  (Initial) g. Student Safety Declaration	                  (Initial) h. Federal Bid Requirements	                  (Initial)

7.	Proper Prevailing wages included in this bid	                  (Initial)
*2015-2018 requirements for Certified Payroll Reporting is acknowledged.

Circular letters, bulletins, addenda, etc., bound with specifications or issued during the time of bidding are included in the proposal, and, in completing the contract, they are to become part thereof.

The receipt of the following addenda to the specifications is acknowledged:

Addendum No. 	Dated:

Addendum No.	Dated:

Addendum No. 	Dated:

Addendum No. 	Dated:

Note: Any exclusion to the scope of work or items noted in this bid form will be considered as cause to deem this bid non-responsive.

This bid may be withdrawn at any time prior to the scheduled time for the opening of bids or any authorized postponement thereof.

NOTE:	 Each bid must give the full business address of the bidder and be signed by him with his usual signature. Bids by partnerships must furnish the full name of all partners and must be signed by one of the members of the partnership, or by an authorized representative, followed by the signature and designation of the person signing. Bid by corporations must be signed with the legal name of the corporation, followed by the name of the state of incorporation and by the signature and designation of the president, secretary, or other person authorized to bind it in the matter. The name of each person signing shall also be typed or printed below the signature. Satisfactory evidence of the authority of the officer signing on behalf of a corporation shall be furnished.

Dated 	, 20	

Signed 	

Print or Type Name 	

Business Address

Phone #

Fax #

License #

Email Address 	

DIR NUMBER_____________________________

Additional Signature Lines if Applicable:

Signed 	

Print or Type Name 	

Business Address

Signed 	

Print or Type Name 	

Business Address

Signed 	

Print or Type Name 	

Business Address

State of Incorporation if Applicable  

( )	Evidence of authority to bind corporation is attached.

Print or Type Name 	

Business Address

Phone Number: 	

FAX Number: 	

Contractor's License Number 	

Email Address 	

Cost Analysis Form Bid 2864
CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

Base Bid – Design Phase as outlined in Summary of Work Base bid currently scheduled for October 6, 2021 Board Award
_____________________________________________________ Dollars $____________

Add Alternate 1 – Construction Phase as outlined in Summary of Work To be awarded at subsequent Board Meeting
_____________________________________________________ Dollars $____________

Total Bid	$__________________

Low bid to be determined by total of base bid plus add Alternate. Project to be awarded to one contractor.

Do not substitute Bid Bond Form

The Bid Bond Form in this packet must be used.

Failure to use the Bid Bond form in this bid packet may result in rejection of bid.

BID BOND

KNOW ALL MEN BY THESE PRESENTS that we the undersigned

	as Principal and

                                                                                                                                    as Surety, are hereby held and firmly bound unto the Clovis Unified School District, acting on behalf of the State Allocation Board, State
of California, hereinafter called the "Owner", in the sum of	
	Dollars ($	
		) for payment of which sum, well and truly to be made, we hereby jointly and severally find ourselves, our heirs, executors, administrators, successors, and assigns.

The condition of the above obligation is such that whereas the Principal has submitted to the Owner a certain bid, attached hereto and hereby made a part hereof, to enter into a contract in writing for the

Bid 2864
CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

in strict accordance with the Contract Documents.

NOW, THEREFORE,

a.	If said bid shall be rejected, or, in the alternate;

b.	 If said bid shall be accepted and the Principal shall execute and deliver a contract in the form of agreement attached hereto and shall execute and deliver Performance and Payment Bonds in the forms attached hereto (all properly completed in accordance with said bid), and shall in all other respects perform the agreement created by the acceptance of said bid;

Then this obligation shall be void, otherwise the same shall remain in force and effect, it being expressly understood and agreed that the liability of the Surety for any and all default of the Principal hereunder shall be the amount of this obligation as herein stated.

Surety, for value received, hereby stipulates and agrees that no change, extension of time, alteration or addition to the terms of the contract on the call for bids, or to the work to be performed thereunder, or the specifications accompanying the same, shall in anyway affect its obligation under this bond, and it does hereby waive notice of any such change, extension of time, alteration or addition to the terms of said contract or the call for bids, or to the work, or to the specifications.

In the event suit is brought upon this bond by the Owner and judgment is recovered the Surety shall pay all costs incurred by the Owner in such suit, including a reasonable attorney's fee to be fixed by the court.

IN WITNESS WHEREOF, the above-bounden parties have executed this instrument under several seals this ____ day of 	,20	, the name and corporate party being hereto affixed and these presents duly signed by its undersigned representative, pursuant to authority of its governing body.

In presence of:
		(Seal) (Individual Principal)

(Address)	(Business Address)

		(Seal) (Individual Principal)

(Address)	(Business Address)

Attest:

(Corporate Principal)

(Business Address)

By:	

(Affix Corporate Seal)

Attest:

(Corporate Principal)

(Business Address)

By:	

(Affix Corporate Seal)

The rate or premium on this bond is 	per thousand.

Total amount of premium charged, $ 	
(The above must be filled in by Corporate Surety)

END OF SECTION lf:10/97 (8.98)

BID 2864

NONCOLLUSION DECLARATION

I, 	, declare that I am 	
(Name of Representative)	(Title of Representative) of                                                                                        ,
(Business Name of Bidder)

the party making the foregoing bid, that the bid is not made in the interest of, or on behalf of, any undisclosed person, partnership, company, association, organization, or corporation; that the bid is genuine and not collusive or sham; that the bidder has not directly or indirectly induced or solicited any other bidder to put in a false or sham bid, and has not directly or indirectly colluded, conspired, connived, or agreed with any bidder or anyone else to put in a sham bid, or that anyone shall refrain from bidding; that the bidder has not in any manner, directly or indirectly, sought by agreement, communication, or conference with anyone to fix the bid price of the bidder or any other bidder, or to fix any overhead, profit, or cost element of the bid price, or of that of any other bidder, or to secure any advantage against the public body awarding the contract of anyone interested in the proposed contract; that all statements contained in the bid are true; and, further, that the bidder has not, directly or indirectly, submitted his or her bid price or any breakdown thereof, or the contents thereof, or divulged information or date relative thereto, or paid, and will not pay, any fee to any corporation, partnership, company association, organization, bid depository, or to any member or agent thereof to effectuate a collusive or sham bid.

I declare under penalty of perjury under the laws of the State of California that the foregoing is true and correct.

Executed this 	day of 	, 20	at 	 , California.

(Signature of Representative)

NOTE: A declaration does not have to be notarized.

Bid 2864
CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

Bidder _____________________________

DESIGNATION OF SUBCONTRACTORS

In compliance with the provisions of Sections 4100 to 4114, inclusive, of the Public Contract Code of the State of California, and any amendments thereof, each bidder shall set forth below the name and the location of the mill, shop or office of each subcontractor who will perform work or labor or render service to the Contractor in or about the construction of the work or improvement to be performed under these specifications, in an amount in excess of one-half of 1 percent (0.5%) of the bidder’s total bid, and the portion of the work which will be done by each subcontractor.

If the Contractor fails to specify a subcontractor for any portion of the work to be performed under the contract, the Contractor shall be deemed to have agreed to perform such portion itself, and shall not be permitted to subcontract that portion of the work except under the conditions hereinafter set forth.

Subletting or subcontracting of any portion of the work as to which no subcontractor was designated in the original bid shall only be permitted in cases of public emergency or necessity, and then only after a finding reduced to writing as a public record of the legislative body of the Owner.

Note:	Reproduce for additional listings needed beyond the length of this form.

Portion of Work
	Name of Subcontractor
	Location & License # of Subcontractor*
	DIR registration #

				

				

				

*	 If there are similarly named subcontractors in a particular location, list enough information in this column to differentiate. LOCATION OF SUBCONTRACTOR MUST BE PROVIDED IN BID RESPONSE

END OF SECTION 3.97 (8.98)

Listing Subcontractors. As required pursuant to the Subletting and Subcontracting Fair Practices Act, each bidder shall submit with its bid a list of the names, license numbers, DIR registration numbers, and locations of the places of business of each subcontractor that will perform work or labor or render service to the bidder in or about the Project, or that, under subcontract to the bidder, will specially fabricate and install a portion of the work, in an amount in excess of one-half of 1 percent of the total amount of the bidder’s bid. A bidder may not list more than one subcontractor for any one portion of the work. A bidder that fails to list a subcontractor for any portion of the work represents that it is fully qualified to and shall perform such work using its own forces. If the bid documents require the bidder to submit alternate bids and the bidder intends to use different or additional subcontractors for the alternates, the bidder must submit a separate list of subcontractors for each such alternate. A bidder shall submit the lists of subcontractors only on the form included in the bid documents.

CLOVIS UNIFIED SCHOOL DISTRICT

Bid 2864
CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

JOB REFERENCES

Bidders must submit a list of at least three (3) projects of similar dollar volume completed within the last 24 months for reference purposes.

DATE
	
JOB SITE
	
CONTACT PERSON
	
TELEPHONE NUMBER

				

				

NAME OF BIDDER 	

3.97 (8.98)

INSURANCE RATING SUBMITTAL FORM

Bid 2864
CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

Attach report of Insurance Rating to this form. Rating Report information to be obtained from A.M. Best Company – http://www.ambest.com

Name of Bidder: ______________________________________________________________

This form and needed report to be submitted with bid proposal at due date and time established in bid aperwork

Bid 2864
CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

DECLARATION OF GOOD FAITH EFFORTS TO USE DISABLED VETERAN BUSINESS ENTERPRISES (DVBE)

I,	_______________________,	declare	that (Name of Representative)

I	am	___________________________ (Title of Representative)

of ____________________________. (Business Name of Bidder)

The party making the foregoing bid declares that the bidder has made good faith efforts to meet the

participation goal of not less than three percent (3%) of the bid amount to include disabled veteran business

enterprises (“DVBE”) in the work to be performed. (Education Code section 17076.11) Good faith efforts

may be met in one of two ways, either: (1) by complying with the safe harbor provisions of Public Contract

Code section 10115.2, subdivision (b), or (2) by complying with Public Contract Code section 10115.2,

subdivision (a) by making good faith efforts other than by following the safe harbor language in Public

Contract Code section 10115.2, subdivision (b). Under Public Contract Code section 10115.2 subdivision (a),

the District will exercise its discretion as to whether the good faith effort has been made. The bidders will

document the good faith efforts and make those documents available upon request by the District.

I declare under penalty of perjury under the law of the State of California that the DVBE requirement for this

bid was met through one of the two foregoing methods and that the foregoing is true and correct.

Executed this __________day of ______________, 20____at______________, California.

_____________________________ (Signature of Representative)

NOTE: This declaration does not have to be notarized.

END OF SECTION TB:lf w/LS 3.02

Bid 2864
CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

STUDENT SAFETY DECLARATION Construction, Rehabilitation or Repair Contractors (Education Code section 45125.2)

I, _______________________________________, declare as follows:

1.	I am a representative of ____________________________, and am authorized to make this declaration on its behalf;

2.	Pursuant to Education Code section 45125.2, I shall not permit any employee, agent or subcontractor to have more than limited contact with pupils without taking protective steps as set forth in that section and this declaration.

3.	I declare that I have taken one or more of the following protective measures pursuant to Education Code section 45125.2:

a.	Neither I, my employees, agents nor subcontractors will have more than limited contact with students.

b.	I have installed or will install a physical barrier at the worksite such that no employee, agent or subcontractor will have more than limited contact with students.

c.	An employee, agent or subcontractor will continually monitor and supervise all employee(s), agent(s) and subcontractor(s) who will have more than limited student contact. I have submitted fingerprints to the Department of Justice for the supervisory employee(s), agent(s) or subcontractor(s). I have received a response from the Department of Justice, and I certify that none of these supervisory employees, agents or subcontractors have been convicted of a felony as defined in Education Code section 45122.1. A list of these supervisors is attached hereto.

I know the above of my own personal knowledge and if called as a witness could competently testify thereto. I declare under penalty of perjury that the foregoing is true and correct and that this declaration was executed on ______________, ______, at ________________, California.

____________________________________________ Name of Contractor

By :________________________________________

clovis\FINGERPRINTING.11.1999

Health Screening

Contractor shall require each service provider who provides services to Clovis Unified School District to conduct screening and/or testing for symptoms of COVID-19.

Such screening or testing, at a minimum, shall:
(1) be conducted at least daily and before a service provider renders services to the District; and

(2) comply with requirements or recommendations by federal, state, and/or local health officials that are in effect at the time the service provider is providing services to the District.

(3) The screening may be in the form of the COVID-19 Service Provider Screening Tool included in this packet, which the District may modify to reflect developing requirements or recommendations from federal, state, and/or local health officials. If any service provider tests positive on any indicators of the self-screening tool, he/she must contact the contractor’s assigner and remove himself/herself from service until he/she has no positive indicators on the self-screening or he/she has tested negative for COVID-19. It is the responsibility of the contractor’s assigner to replace that service provider with a new service provider, who has no positive indicators on the self-screening tool or has tested negative for COVID-19. Contractor shall also require each service provider who provides services to the District to wear face coverings and/or other personal protective equipment as required or recommended by federal, state, and/or local health officials. In the event that the requirements or recommendations of federal, state, and local health official’s conflict, contractor shall require each service provider to comply with the requirement/recommendation that is stricter. Contractor shall not allow any service provider who has tested positive for COVID-19, has symptoms of COVID19, or has any positive indicators on the self-screening tool to provide services for the District
(4) If service provider has no fever or respiratory symptoms, they can provide service AFTER washing their hands and need to follow social distancing as appropriate for service being provided
(5) Masking with cloth mask and physical distancing (6 feet apart) is required when providing service in district, especially when around district students and staff.

SUBMIT FORM WITH BID RESPONSE COVID-19 SERVICE PROVIDER SCREEN TOOL

All constractor service providers are required to “self certify” by answering the questions below prior to entering their assigned Clovis Unified School District service location and coming into contact with students and staff.

SPECIAL INSTRUCTIONS AND INFORMATION
BID PROJECT EXPENDITURES MAY INCLUDE FEDERAL FUNDING

1. Project may be funded in part or in total with Federal Funds.

2. City of Clovis, City of Fresno and County of Fresno are jurisdiction areas of Clovis USD

3. If State of California prevailing wage rates are higher than Federal Davis-Bacon rates, project to be bid utilizing State of California prevailing wage rates as mandated by California bid laws and regulations.

4. Information related to Federal Procurement Guidelines - :
a. Federal Regulation Codes https://www.ecfr.gov/cgi-bin/text-idx?node=2:1.1.2.2.1

b. 34 Code of Federal Regulations CFR 75.609 related to safety and health https://www.ecfr.gov/cgi-bin/text-idx?SID=cd37bda54b7e6822ae66876ae2b5034c&pitd=20190619&node=se34.1.75_ 1609&rgn=div8

c. 34 Code of Federal Regulations CFR 75.616 related to energy conservation https://www.ecfr.gov/cgi-bin/text-idx?SID=6b0336c285fb183779141ccaf8b81df8&pitd=20200602&node=se34.1.75_1 616&rgn=div8
d. Davis Bacon Wage Rate https://www.dol.gov/agencies/whd/government-contracts/construction

5. Awarded contractor CANNOT be on the US General Services Administration Lists of Parties Excluded from Federal Procurement or Non-Procurement Programs https://sam.gov/content/exclusions

6.	 ** BIDDER MUST INCLUDE PROOF OF SEARCH RESULTS INDICATING THEY ARE NOT ON THE FEDERAL EXCLUSION LISTING - - SEE SAMPLE SCREEN SHOTS BELOW THAT IS TO BE SUBMITTED WITH BID

Type in your company name and hit search. Then go to Excluded Entity link on left of page and type in company name a second time and hit enter on keyboard.

7. PRINT OUT THIS SCREEN SHOT INDICATING NO MATCHES FOUND WITH SEALED BID PROPOSAL AT DUE DATE AND TIME OF BID SUBMITTAL. THIS INDICATES YOUR COMPANY IS NOT EXCLUDED FROM FEDERAL CONTRACTS

8. THANK YOU FOR YOUR TIME IN COMPLETING THIS PROCESS AND INCLUDING DOCUMENTATION WITH BID PACKET. THIS ENSURES THE
DISTRICT IS MEETING FEDERAL GRANT REQUIREMENTS. THESE GRANTS BRING FEDERAL TAX DOLLARS TO OUR COMMUNITY FOR PROJECTS THAT BENEFIT OUR STUDENTS.

RETURN WITH BID SUBMITTAL PACKET

ALONG WITH COPY OF SCREEN SHOT INDICATING COMPANY IS NOT ON FEDERAL CONTRACT EXCLUSION LISTING

DECLARATION OF GOOD FAITH EFFORT TO MEET PROVISIONS OF FEDERAL FUNDING REQUIREMENTS – INCLUDING, BUT NOT LIMITED TO SAFETY & HEALTH STANDARDS, ENERGY CONSERVATION, DAVIS-BACON PREVAILING WAGE RULES AND RELATED ACT PROVISIONS

I,	_______________________,	declare	that (Name of Representative)
Representative)

I           am           ___________________________ (Title                    of

of ____________________________. (Business Name of Bidder)

The party making the foregoing bid declares that the bidder has made good faith efforts to meet the provisions of Federal

funding requirements, including, but not limited to Davis-Bacon and related Act provision, the District will exercise its

discretion as to whether the good faith effort has been made. The bidders will document the good faith efforts and make

those documents available upon request by the District.

I declare under penalty of perjury under the law of the State of California that the Federal funding requirement for this

bid was met is true and correct.

Executed this __________day of ______________, 20____at______________, California.

_____________________________ (Signature of Representative)

NOTE: This declaration does not have to be notarized.

END OF SECTION

AGREEMENT BETWEEN OWNER AND CONTRACTOR

THIS AGREEMENT, dated the _______ day of _________________, 2021, in the

County of Fresno, State of California, is by and between Clovis Unified School District (hereinafter referred to as "DISTRICT"), and _______________________ (hereinafter referred to as "CONTRACTOR").

The DISTRICT and the CONTRACTOR, for the consideration stated herein, agree as follows:
1.	The complete contract includes all of the Project documents described in the General Conditions. The Project documents are complementary, and what is called for by any one shall be as binding as if called for by all.

2.	CONTRACTOR shall perform within the time set forth in Paragraph 4 of this Agreement everything required to be performed, and shall provide and furnish all the labor, materials, necessary tools, expendable equipment, and all utility and transportation services as described in the complete contract and required for construction of

Bid 2864 - CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

All of said work to be performed and materials to be furnished shall be completed in a good workmanlike manner in strict accordance with the plans, drawings, specifications and all provisions of the complete contract as hereinabove defined. The CONTRACTOR shall be liable to the DISTRICT for any damages arising as a result of a failure to fully comply with this obligation, and the CONTRACTOR shall not be excused with respect to any failure to so comply by any act or omission of the Architect, Engineer, Inspector, Division of State Architect, or representative of any of them, unless such act or omission actually prevents the CONTRACTOR from fully complying with the requirements of the Project documents, and unless the CONTRACTOR protests at the time of such alleged prevention that the act or omission is preventing the CONTRACTOR from fully complying with the Project documents. Such protest shall not be effective unless reduced to writing and filed with the DISTRICT within three (3) working days of the date of occurrence of the act or omission preventing the CONTRACTOR from fully complying with the Project documents.

3.	DISTRICT shall pay to the CONTRACTOR, as full consideration for the faithful performance of the contract, subject to any additions or deductions as provided in the Project documents, the sum of ________________________________________________	($ ).
4.	The work shall be commenced on or before the fifth (5th) day after receiving the DISTRICT's Notice to Proceed – total project shall be completed within 310 calendar days (per construction manager’s work schedule).	Individual project trades to be completed in accordance with construction manager’s work schedule.

5.	Time is of the essence. If the work is not completed in accordance with Paragraph 4 above, it is understood that the DISTRICT will suffer damage.	It being impractical and infeasible to determine the amount of actual damage, in accordance with Government Code Section 53069.85, it is agreed that CONTRACTOR shall pay to DISTRICT as fixed and liquidated damages, and not as a penalty, the sum One Thousand Dollars ($1000.00) for each calendar day of delay until work is completed and accepted. This amount shall be deducted from any payments due to or to become due to

CONTRACTOR. CONTRACTOR and CONTRACTOR'S surety shall be liable for the amount thereof. Time extensions may be granted by the DISTRICT as provided in the General Conditions.

6.	In the event CONTRACTOR for a period of ten (10) calendar days after receipt of written demand from DISTRICT to do so, fails to furnish tools, equipment, or labor in the necessary quantity or quality, or to prosecute said work and all parts thereof in a diligent and workmanlike manner, or after commencing to do so within said ten (10) calendar days, fails to continue to do so, then the DISTRICT may exclude the CONTRACTOR from the premises, or any portion thereof, and take possession of said premises or any portion thereof, together with all material and equipment thereon, and may complete the work contemplated by this Agreement or any portion of said work, either by furnishing the tools, equipment, labor or material necessary, or by letting the unfinished portion of said work, or the portion taken over by the DISTRICT to another contractor, or by a combination of such methods. In any event, the procuring of the completion of said work, or the portion thereof taken over by the DISTRICT, shall be a charge against the CONTRACTOR, and may be deducted from any money due or to become due to CONTRACTOR from the DISTRICT, or the CONTRACTOR shall pay the DISTRICT the amount of said charge, or the portion thereof unsatisfied. The sureties provided for under this Agreement shall become liable for payment should CONTRACTOR fail to pay in full any said cost incurred by the DISTRICT.

7. The CONTRACTOR agrees to and does hereby indemnify and hold harmless the DISTRICT, its governing board, officers, agents, and employees from every claim or demand made, and every liability, loss, damage, or expense, of any nature whatsoever, which may be incurred by reason of:

(a) Liability for damages for (1) death or bodily injury to persons; (2) injury to, loss or theft of property; or (3) any other loss, damage or expense arising under either (1) or (2) above, sustained by the CONTRACTOR upon or in connection with the work called for in this Project, except for liability resulting from the sole active negligence, or willful misconduct of the DISTRICT.

(b) Any injury to or death of any person(s) or damage, loss or theft of any property caused by any act, neglect, default or omission of the CONTRACTOR, or any person, firm, or corporation employed by the CONTRACTOR, either directly or by independent contract, arising out of, or in any way connected with the work covered by this Agreement, whether said injury or damage occurs on or off District property.

The CONTRACTOR, at CONTRACTOR's own expense, cost, and risk shall defend any and all actions, suits, or other proceedings that may be brought or instituted against the DISTRICT, its governing board, officers, agents or employees, on any such claim, demand or liability, and shall pay or satisfy any judgment that may be rendered against the DISTRICT, its governing board, officers, agents or employees in any action, suit or other proceedings as a result thereof.

8.	Contractor shall provide the insurance set forth in the General Conditions. The amount of general liability insurance shall be not less than $1,000,000 per occurrence for bodily injury, personal injury and property damage and the amount of automobile liability insurance shall be not less than $2,000,000 per accident for bodily injury and property damage combined single limit.

9.	Public Contract Code Section 22300 permits the substitution of securities for any monies withheld by a public agency to ensure performance under a contract. At the request and expense of the CONTRACTOR, securities equivalent to the amount withheld shall be deposited with the public agency, or with a state or federally chartered bank in California as the escrow agent, who shall then pay such monies to the CONTRACTOR. The District retains the sole discretion to approve the bank selected by the CONTRACTOR to serve as escrow agent.	Upon satisfactory completion of the contract, the securities shall be returned to the CONTRACTOR. Securities eligible for investment shall include those listed in Government Code Section 16430 or bank or savings and loan certificates of deposit. The CONTRACTOR shall be the beneficial owner of any securities substituted for monies withheld and shall receive any interest thereon.

In the alternative, under Section 22300, the CONTRACTOR may request DISTRICT to make payment of earned retentions directly to the escrow agent at the expense of the CONTRACTOR.	Also at the CONTRACTOR's expense, the CONTRACTOR may direct investment of the payments in securities, and the CONTRACTOR shall receive interest earned on such investment upon the same conditions as provided for securities deposited by CONTRACTOR.	Upon satisfactory completion of the contract, CONTRACTOR shall receive from the escrow agent all securities, interest and payments received by escrow agent from DISTRICT pursuant to the terms of Section 22300. CONTRACTOR shall pay to each subcontractor, not later than 20 days after receipt of such payment, the respective amount of interest earned, net of costs attributed to retention withheld from each subcontractor, on the amount of retention withheld to insure performance of the CONTRACTOR.

10.	Each and every provision of law and clause required by law to be inserted in this Agreement shall be deemed to be inserted herein and the Agreement shall be read and enforced as though it were included herein, and if through mistake or otherwise any such provision is not inserted, or is not currently inserted, then upon application of either party the Agreement shall forthwith be physically amended to make such insertion or correction.

11.	The complete contract as set forth in Paragraph 1 of this Agreement constitutes the entire Agreement of the parties. No other agreements, oral or written, pertaining to the work to be performed, exists between the parties. This Agreement can be modified only by an amendment in writing, signed by both parties and pursuant to action of the Governing Board of the District.

12.	CONTRACTOR shall comply with those provisions of the Labor Code requiring payment of prevailing wages, keeping of certified payroll records, overtime pay, employment of apprentices, and workers' compensation coverage, as further set forth in the General Conditions, and shall file the required workers' compensation certificate before commencing work.

The Contractor and each subcontractor shall furnish a certified copy of all payroll records directly to the Labor Commissioner. Submittal of said records to meet DIR submittal process instructions and requirements.

For public works contracts awarded on and after January 1, 2015, those public works projects shall be subject to compliance monitoring and enforcement by the Department of Industrial Relations.

As of March 1, 2015, a contractor or subcontractor shall not be qualified to submit a bid or to be listed in a bid proposal subject to the requirements of Public Contract Code section 4104 unless currently registered and qualified under Labor Code section 1725.5 to perform public work as defined by Division 2, Part 7, Chapter 1 (§§1720 et seq.) of the Labor Code.

As of April 1, 2015, a contractor or subcontractor shall not be qualified to enter into, or engage in the performance of, any contract of public work (as defined by Division 2, Part 7, Chapter 1 (§§1720 et seq.) of the Labor Code) unless currently registered and qualified under Labor Code section 1725.5 to perform public work.

13.	The Contractor must comply with the applicable requirements of the Division of State Architect (“DSA”) Construction Oversight Process (“DSA Oversight Process”), including but not limited to (a) notifying the Owner’s Inspector of Record/Project Inspector (“IOR”) upon commencement and completion of each aspect of the work as required under DSA Form 156; (b) coordinating the Work with the IOR’s inspection duties and requirements; (c) submitting verified reports under DSA Form 6-C; and (d) coordinating with the Owner, Owner’s Architect, any Construction Manager, any laboratories, and the IOR to meet the DSA Oversight Process requirements without delay or added costs to the Project.

Contractor shall be responsible for any additional DSA fees related to review of proposed changes to the DSA-approved construction documents, to the extent the proposed changes were caused by Contractor’s wrongful act or omissions. If inspected work is found to be in non-compliance with the DSA-approved construction documents or the DSA-approved testing and inspection program, then it must be removed and corrected. Any construction that covers unapproved or uninspected work is subject to removal and correction, at Contractor’s expense, in order to permit inspection and approval of the covered work in accordance with the DSA Oversight Process.

IN WITNESS WHEREOF, the parties hereto have caused this Agreement to be executed.

DISTRICT

By: __________________________________ Signature

Michael Johnston Associate Superintendent Title

CONTRACTOR

By: __________________________________ Signature* (see next p.)

_____________________________________ Title

(Second signature required only for corporation)

By: __________________________________ Signature** (see next p.)

_____________________________________ Print Name _____________________________________ Title

(CORPORATE SEAL OF CONTRACTOR, if corporation)

_____________________________________ Contractor's License No.

_____________________________________ Tax ID/Social Security No.

*If CONTRACTOR is a corporation, the first signature must be by one of the following officers of the corporation: Chairman of the Board, President, or any Vice President.

**If CONTRACTOR is a corporation, the second signature must be by a different person from the first signature and must be by one of the following officers of the corporation: Secretary, any Assistant Secretary, the Chief Financial Officer, or any Assistant Treasurer.

Purch Bid fr.lf 9 98

Health Screening	CONTRACT ATTACHMENT

Contractor shall require each service provider who provides services to Clovis Unified School District to conduct screening and/or testing for symptoms of COVID-19.

Such screening or testing, at a minimum, shall:
(6) be conducted at least daily and before a service provider renders services to the District; and

(7) comply with requirements or recommendations by federal, state, and/or local health officials that are in effect at the time the service provider is providing services to the District.

(8) The screening may be in the form of the COVID-19 Service Provider Screening Tool included in this packet, which the District may modify to reflect developing requirements or recommendations from federal, state, and/or local health officials. If any service provider tests positive on any indicators of the self-screening tool, he/she must contact the contractor’s assigner and remove himself/herself from service until he/she has no positive indicators on the self-screening or he/she has tested negative for COVID-19. It is the responsibility of the contractor’s assigner to replace that service provider with a new service provider, who has no positive indicators on the self-screening tool or has tested negative for COVID-19. Contractor shall also require each service provider who provides services to the District to wear face coverings and/or other personal protective equipment as required or recommended by federal, state, and/or local health officials. In the event that the requirements or recommendations of federal, state, and local health official’s conflict, contractor shall require each service provider to comply with the requirement/recommendation that is stricter. Contractor shall not allow any service provider who has tested positive for COVID-19, has symptoms of COVID19, or has any positive indicators on the self-screening tool to provide services for the District
(9) If service provider has no fever or respiratory symptoms, they can provide service AFTER washing their hands and need to follow social distancing as appropriate for service being provided
(10)	Masking with cloth mask and physical distancing (6 feet apart) is required when providing service in district, especially when around district students and staff.

COVID-19 SERVICE PROVIDER SCREEN TOOL

All constractor service providers are required to “self certify” by answering the questions below prior to entering their assigned Clovis Unified School District service location and coming into contact with students and staff.

PAYMENT BOND (Labor and Material)

KNOW ALL MEN BY THESE PRESENTS:

That WHEREAS,

and

Hereinafter designated as the “Principal”, have entered into a contract for the furnishing of all materials and labor, services and transportation, necessary, convenient, and proper to construct

Bid 2864
CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

Which said agreement dated	, 2021 and all of the contract documents attached to or forming a part of said agreement, are hereby referred to and made a part hereof; and

WHEREAS, the Principal is required, before entering upon the performance of the work, to file a good and sufficient bond with the body by whom the contract is awarded to secure the claims arising under said agreement.

NOW, THEREFORE, THESE PRESENTS WITNESSETH:

That the said Principal and the undersigned

are held and firmly bound unto all laborers, material men, and other persons referred to in said statutes in the sum of	Dollars ($	) which sum well and truly be made, we bind ourselves, our heirs, executors, administrators, successors, or assigns, jointly and severally, by these presents.

The condition of this obligation is that if the said Principal or any of its subcontractors, or the heirs, executors, administrators, successors, or assigns of any, all, or either of them, shall fail to pay for any materials, provisions, provender or other supplies, or teams, used in, upon, for, or about the performance of the work contracted to be done, or for any work or labor thereon of any kind or for amounts due under the Unemployment Insurance Act with respect to such work or labor, that said Surety will pay the same in an amount not exceeding the amount hereinabove set forth, and also in case suit is brought upon this bond, will pay a reasonable attorney’s fee to be awarded and fixed by the Court, and to be taxed as costs and to be included in the judgment therein rendered.

It is hereby expressly stipulated and agreed that this bond shall inure to the benefit of any and all persons, companies, and corporations entitled to file claims so as to give a right of action to them or their assigns in any suit brought upon this bond.

Should the condition of this bond be fully performed, then this obligation shall become null and void, otherwise it shall be and remain in full force and effect.

And the said Surety, for value received, thereby stipulates and agrees that no change, extension of time, alteration, or addition to the terms of said contract or the specifications accompanying the same shall in any manner affect its obligations on this bond, and it does hereby waive notice of any such change, extension, alteration, or addition.

IN WITNESS WHEREOF, this instrument has been duly executed by the Principal and Surety

this 	day of 	, 2021

(To be signed by	) (Principal and Surety,     )
(and acknowledged and) (Notarial Seal attached )

Principal

Surety

By:
Attorney-in-Fact

The above bond is accepted and approved this 	day of 	, 2021

END OF SECTION 3.97 (8.98)

PERFORMANCE BOND

KNOW ALL MEN BY THESE PRESENTS that we
	 as Principal, and
as Surety, are held and firmly bound unto Clovis Unified School District, in the County of Fresno, State of California, hereinafter called the “Owner”, acting on behalf of the State Allocation Board, State of California, in the sum of	Dollars ($	) for the payment of which sum well and truly made, we bind ourselves, our heirs, executors, administrators, and successors, jointly and severally, firmly by these presents.

The condition of this obligation is such, that whereas the Principal entered into a certain contract with the Owner, dated 	, 2021 for construction of

Bid 2864
CLOVIS WEST HIGH SCHOOL CLASSROOM BUILDING - ALUMINUM STOREFRONT

NOW, THEREFORE, if the Principal shall well and truly perform and fulfill all the undertakings, covenants, terms, conditions, and agreements of said contract during the original term of said contract and any extensions thereof that may be granted by the Owner, with or without notice to the Surety, and during the life of any guaranty required under the contract, and shall also well and truly perform and fulfill all the undertakings, covenants, terms, conditions, and agreements of any and all duly authorized modifications of said contract that may hereafter be made, then this obligation to be void, otherwise to remain in full force and virtue.

And the said Surety, for value received, hereby stipulates and agrees that no change, extension of time, alteration or addition to the terms of the contract or to the work to be performed thereunder or the specifications accompanying the same, shall in any way affect its obligation on this bond, and it does hereby waive notice of any such change, extension of time, alteration or addition to the terms of the contract, or to the work, or to the specifications.

IN WITNESS WHEREOF, the above-bounden parties have executed this instrument under their several seals this day of                             , 2021 hereto affixed and these presents duly signed by its undersigned
representative, pursuant to authority of its governing body.

(To be signed by	) (Principal and Surety,     )
(and acknowledged and) (Notarial Seal attached )

(Affix Corporate Seal)	
(Individual Principal)

(Business Address)

(Affix Corporate Seal)	
(Corporate Principal)

(Business Address)

(Affix Corporate Seal)	
(Corporate Surety)

(Business Address)

By: 	

The rate or premium on this bond is 	per thousand.

The total amount of premium charged is	.

The above must be filled in by Corporate Surety.

END OF SECTION 3.97 (8.98)

01110 SUMMARY OF WORK
PAGE 1

PART 1 - GENERAL

1.01     SUMMARY

A. General: Construction of BASE BID and Alternate portions of the work for Clovis Unified School District Clovis West Classroom Addition ALUMINUM STOREFRONT Fresno, CA. BASE BID and Alternate portions of the work is defined as all material, labor, equipment and services necessary to do all work shown on the drawings and called for in the Specifications.

General Summary of the Project
The following information applies to all prime-contractors and shall be reviewed carefully for inclusion in each bid. Following are critical logistics related to the Project:
1.	Abatement work is not included in this contract.
2.	All work for the project will be performed while school is in session during the hours of 7:00 a.m. to 3:30 p.m. Utility tie-ins to be performed after hours.
3.	Submittals and material procurement shall begin immediately upon award or letter of intent from the District. 4.	Material procurement is critical and shall be diligently pursued to meet the contract schedule.
5.	Contractors shall review the project and schedule completely prior to bidding the work.
6.	 Substitutions must be noted in each bid with all costs for the specified product included in the bid and the substitution cost noted separately
7.	 Coordination of work during the preconstruction period is equally as critical to resolving all issues prior to the start of work. Prime-contractor shall review the project, coordinate and question any issues to allow resolution prior to the start of work.

Site access and conduct
1.	All classrooms will be in session on all 4 sides of the project.
2.	While construction noise is expected, strong language will not be tolerated. 3.	Interactions with students will not be tolerated.
4.	All workers will be required to obtain a badge to be onsite.

5.	All foreman will be required to be fingerprinted as called for in the documents

Schedule
The prime-contractor will be required to provide a schedule and crew sizing showing how the work will be accomplished within the given time frame of the contract schedule.

This project will involve work with other contracts to allow for proper student safety and access. See site access plan and schedule for phasing. In general, A sperate project will remove and replace the large planter on the south side of the side in the Month of September to allow for student access. Students will use the walk way on the north side of the site until the planter work has been completed. Once complete the north side of the site will be closed off for construction only and students will use the newly created south access walk way. Access to toilets on the east side must remain open through out the project.

Storm Water Pollution Prevention Plan

Follow all best management practices as called for by code.

Contract
Please be advised that all successful bidders will be required to enter into a subcontract agreement with Clovis Unified School District.

Addendum 01 Storefront Package

01110

SUMMARY OF WORK PAGE 2

Alternates

Additive Alternates for the work are as follows. Please provide a base bid for the project then list all additive alternates: 1.	As called for on the plans and specifications

Crew Sizes
All prime-contractors shall review the schedule and confirm that they can crew the project accordingly prior to submitting a bid. Include with each bid minimum and maximum crew sizes projected for the project

Site Logistics, Work and Coordination (applies to each prime-contractor): 1.	Review and verify all existing conditions.
2.	 Provide all necessary temporary utility distribution from services provided at the building by the Construction Manager.
3.	 All contractors shall attend coordination meetings and provide coordination drawings for underground and above ceiling work for work related to this subcontract and for coordination of utilities, openings and other areas that require interface between trades. Coordinate all drawings with the drawings of this subcontract. Note conflicts and provide potential solutions to the architect for review. Coordination and drawing approval must occur prior to excavation (and/or) overhead work. Contractor shall attend a pre-installation meeting prior to the start of its work onsite. All contractors shall be available for pre-installation meetings of other contractors for coordination of related work.
4.	 Only company vehicles are allowed onsite. No tool drop off or parking by personal vehicles will be allowed. Contractor to make provisions for transport or tool distribution needs.
5.	Lunch and breaks shall be at designated areas only. No other areas will be allowed. 6.	Protect all work, new and existing, from damage until acceptance by owner.
7.	 Storage areas will be confined to the areas designated by the Construction Manager. Staging areas around the building shall be coordinated with the Construction Manager. Storage onsite will be controlled due to limited space available.
8.	Furnish all access to roof for own work.
9.	 Work under each contract shall comply with the Storm Water Pollution standards and as set forth in these Contract Documents.
10. All work under each contract shall comply with Air Pollution Control District standards. Provide dust control for own work.
11. Provide written request for information through the Construction Manager for layout information from related subcontracts for all rough-in, embedded items, openings and block-outs, etc.
12. Request and reviewallassociated shop drawingsfor coordination andlayoutpurposesprior to installation ofrelated materials.
13. Furnish and Install specified and/or approved sealant for work abutting other materials. 14. Furnish and install protection of all roofing for own work.
15. Furnish and install all physical layout for own work.
16. There will be one wash out area for each contractor as designated by The Construction Manager. Each contractor will be responsible for removal from the site of all debris and spoils generated by each bid package.
17. Secure all ladders and lifts each evening.
18. Provide caution tape and/or barriers for open area work and traffic control.
19. Coordinate all work with mechanical, plumbing and electrical prime-contractor for shut down of services as needed. 48 hours notice is required prior to all shut down activities.

Addendum 01 Storefront Package

01110 SUMMARY OF WORK
PAGE 3

Glass, Glazing, and Storefronts

Furnish and install all work specifically required throughout the project documents to complete the work of this prime-contractor that specifically includes, but is not limited to the following:

Specification Sections Division 1
084113	ALUMINUM FRAMED STOREFRONTS 085113	ALUMINUM WINDOWS
087100	DOOR HARDWARE 088000	GLAZING
07900	JOINT SEALANTS

Refer to additional related specifications sections for work specifically included in this prime-contractor noted below.

NOTE: This bid package will perform work in 2 phases

DESIGN PHASE: The design phase consists of providing deferred approval shop drawings as called for in the documents to gain approval through DSA. The entire project is currently going through the DSA process and should gain approval by December 2022 2021. (ADM 1) This process will act in parallel with the entire project. The purpose is to gain approval through DSA to allow for timely fabrication and delivery of the aluminum frames and glass so as not to delay the project. Delivery is anticipated for May 2022 to allow for the project to be complete by August 1, 2022

CONSTRUCTIONPHASE: As soon asDSA approvalhasbeen received, procurement, fabrication and installation shallproceed so as not to delay the project schedule.

AWARD: Clovis Unified School District will award the design phase only. Once DSA has approved the entire project, the construction phase will be awarded, and fabrication can proceed. The bid form has a line for design costs and construction costs with a total for both. This will be awarded to one contract for both phases based on the Base Bid plus any alternates. (ADM 1)

General Items
1.	 Any substitution of details or materials must be pre-approved by the Architect, engineers and DSA. All substitution requests must be submitted to CONSTRUCTION MANAGER prior to or with prime-contractor bid. This contractor is responsible for all costs and time delays required for DSA approval.
2.	See General Notes at beginning of summary of work specification section for other items.

Coordination with Other Trades –
1.	Coordinatelocationsofwindowand door framesinstalled by thisprime-contractor relativeto thelocation of plaster molding and drywall termination (ADM 1) adjacent to the frames to insure a good fit. Provide physical layout for the plaster /drywall (ADM 1) contractor for the plaster molding and drywall. (ADM 1) This will allow for work to proceed if frames are not available.
2.	Submit shop drawings & procure material so as not to delay the scheduled installation of plaster and drywall.
3.	Order windows based on guaranteed rough opening dimensions from the framing contractors. This contract is responsible for all furring and shims after rough framing. (ADM 1)

Furnish and Install Items
1.	Provide all design required for deferred approval by DSA.
2.	Furnish and install all glass and glazing shown throughout the contractor documents 3.	Furnish and install all storefront and windows systems complete
4.	Furnish an install glass at door lights remove and reinstall screws for stops.

Addendum 01 Storefront Package

01110

SUMMARY OF WORK PAGE 4

5.	Furnish and install all shims and 1x (ADM 1) wood backing / furring(ADM 1) necessary for plumb installation of work included in this prime-contractor. Install prior to drywall on separate move in from windows. (ADM 1)
6.	Furnish and install sealants at all aluminum windows and storefront at interior and exterior. This includes windows to flashing, windows to plaster and flashing to plaster. (ADM 1)
7.	Furnish and install all aluminum flashing and break metal.
8.	Furnish and install all galvanized and aluminum flashing at windows at head sill and jamb as required. (ADM 1) 9.	Furnish and install all reinforcing for the storefront system as required by DSA
10. Furnish and install all hardware for aluminum storefront doors and frames. 11. Provide all water testing of windows per the specifications (ADM 1)
12. Provide 1 mock up with incoordination with the plaster bid package to confirm all flashing and sealant systems. (ADM 1)

FOB Items
1.	None

End of Prime-contractor

1.03  WORK UNDER OTHER CONTRACTS:

A.	General Requirements:
1) Work under separatecontractsmay occur throughout theduration oftheproject. The work beinginstalled under separate contracts will occur around adjacent to the Contract project site including offsite work.
Contractor shall be responsible for coordinating access to and from the site throughout the duration of the project. Access points to and from the site may vary, based upon timing and duration of separate contracts.
2) Contractor shall cooperate and coordinate all work under this Contract with all work under separate contracts.
3) Should the Contractor damage and/or otherwise alter work installed under separate contracts, Contractor responsible for the correction repair of work installed under separate contracts.
4) Prior to the installation of the Work, coordinate the work installed or to be installed by separate contracts relative to own work.

B.	Separate Contracts by Owner: 1.	Coordinate as awarded.
C.	Separate Contracts by Others:

1.	Adjacent Properties: Residential D.	Phasing:

E.	Phasing is projected to be as shown on the Bid Schedule. However, the owner reserves the right to revise start times pending the review and award of bids.

1.04     CONTRACTOR'S DUTIES:
A.	Except as specifically noted, provide and pay for: 1.	Labor, material and equipment.
2.	Tools, construction equipment and machinery.
3.	Other facilities and services necessary for proper execution and completion of Work. 4.	Water: See Specification Section – TEMPORARY FACILITIES AND CONTROLS.
B.	Pay legally required sales, consumer and use taxes.
C.	Secure and pay for all site specific, as necessary for proper execution and completion of Work, and as applicable at time of receipt of bids.

Addendum 01 Storefront Package

01110 SUMMARY OF WORK
PAGE 5

1.	Licenses.
2.	Permits and Fees. 3.	Governmental Fees. 4.	Royalties.
C.	Give required notices.
E.	Comply with codes, ordinances, rules, regulations, orders and other legal requirements of public authorities which bear on performance of Work.
1.	 The Contractor shall certify in writing that no materials containing Asbestos are incorporated in the work, in accordance with the Asbestos Hazard Emergency Regulations Act.
F.	Promptly submit written notice to Construction Manager of observed variance of Contract Documents from legal requirements.
1.	Appropriate modifications to Contract Documents will adjust necessary changes.
2.	 Assume responsibility for work known to be contrary to such requirements and without written notice to Architect of observed variance.
G.	Enforce strict discipline and good order among employees. Do not employ on Work: 1.	Unfit persons.
2.	Persons not skilled in assigned task.
H.	Provide material, equipment and manpower to meet Construction Schedule provided in Contract Documents.

1.05     CONTRACTOR USE OF PREMISES:
A.	Confine operations at sites to areas permitted by: 1.	Laws.
2.	Ordinances. 3.	Permits.
3.	Contract Documents.
B.	Do not unreasonably encumber site with materials or equipment. C.	Do not load structure with weight that will endanger structure.
D.	 Assume full responsibility for protection and safekeeping of Contractor's and Owner's material stored on premises, and keep the site and building secure at all times.
E.	Obtain and pay for use of additional storage or Work areas needed for operations. F.	Limit use of site for Work and storage.

PART 2 - PRODUCTS (Not Applicable)

PART 3 - EXECUTION (Not Applicable)

END OF SECTION

Addendum 01 Storefront Package

SECTION 088000 GLAZING

PART 1 - GENERAL

1.1	RELATED DOCUMENTS

A.	 Drawings and general provisions of the contract, including General and Supplementary Conditions and Division 01 Specification Sections, apply to this Section.

1.2	SUMMARY

A.	Section includes:

1.	Glass for windows, doors, and storefront framing.

a.	 Glass Types are indicated in glass type schedules at the end of this Section.

2.	Glazing sealants and accessories.

B.	Related Sections include the following:

1.	 Division 07 Section "Joint Sealants" for joint sealants other than those specified in this section.
2.	Division 08 Section “Aluminum Windows”.

1.3	DEFINITIONS

A.	 Glass Manufacturers: Firms that produce primary glass, fabricated glass, or both, as defined in referenced glazing publications.

B.	 Glass Thicknesses: Indicated by thickness designations in millimeters according to ASTM C 1036.

C.	Interspace: Space between lites of an insulating-glass unit.

1.4	SUBMITTALS

A.	 Product Data: For each type of product; include statement of VOC content for any adhesives or sealants.

B.	 Glass Samples: For each type of glass product, other than clear monolithic glass, in 12-inch square samples for the following:

1. 2.

21-11972

Tinted glass. Insulating glass.

GLAZING                                           088000 - 1 of 12 Addendum 01 Storefront Package

C.	 Glazing Accessory Samples: For sealants and colored spacers in 12-inch lengths. Install sealant Samples between two strips of material representative in color of the adjoining framing system.

D.	 Glazing Schedule:	List glass types and thicknesses for each size opening and location. Use same designations indicated on Drawings.

E.	 Product Certificates: Signed by manufacturers of glass and glazing products certifying that products furnished comply with requirements.

1.5	QUALITY ASSURANCE

A.	 Installer Qualifications: A qualified installer who has completed glazing similar in material, design, and extent to that indicated for this Project; whose work has resulted in installations with a record of successful in-service performance; and who employs glass installers for this Project who are experienced in installing glazing similar in material, design, and extent to that indicated for this Project.

B.	 Glass Testing Agency Qualifications: A qualified independent testing agency accredited according to the NFRC CAP 1 Certification Agency Program.

1.6	COORDINATION

A.	 Coordinate glazing channel dimensions to provide necessary bite on glass, minimum edge and face clearances, and adequate sealant thicknesses, with reasonable tolerances.

1.7	DELIVERY, STORAGE, AND HANDLING

A.	 Protect glazing materials according to manufacturer's written instructions and as needed to prevent damage to glass and glazing materials from condensation, temperature changes, direct exposure to sun, or other causes.

B.	 Comply with insulating-glass manufacturer's written instructions for venting and sealing units to avoid hermetic seal ruptures due to altitude change.

FIELD CONDITIONS

C.	 Environmental Limitations: Do not proceed with glazing when ambient and substrate temperature conditions are outside limits permitted by glazing material manufacturers and when glazing channel substrates are wet from rain, frost, condensation, or other causes.

1.	 Do not install liquid glazing sealants when ambient and substrate temperature conditions are outside limits permitted by glazing sealant manufacturer or below 40 deg F.

21-11972                                                      GLAZING                                           088000 - 2 of 12 Addendum 01 Storefront Package

1.8	WARRANTY

A.	 Manufacturer's Special Warranty on Insulating Glass: Manufacturer agrees to replace insulating-glass units that deteriorate within specified warranty period. Deterioration of insulating glass is defined as failure of hermetic seal under normal use that is not attributed to glass breakage or to maintaining and cleaning insulating glass contrary to manufacturer's written instructions. Evidence of failure is the obstruction of vision by dust, moisture, or film on interior surfaces of glass.

1.	Warranty Period: 10 years from date of Substantial Completion.

B.	 Manufacturer's Special Warranty for Coated-Glass Products: Manufacturer agrees to replace coated-glass units that deteriorate within specified warranty period. Deterioration of coated glass is defined as defects developed from normal use that are not attributed to glass breakage or to maintaining and cleaning coated glass contrary to manufacturer's written instructions.	Defects include peeling, cracking, and other indications of deterioration in coating.

1.	Warranty Period: 10 years from date of Substantial Completion.

PART 2 - PRODUCTS

2.1	MANUFACTURERS

A.	 Basis-of-Design Products: Where products are identified by manufacturer and product names, Design, Drawings, and Specifications are based on the product indicated; subject to compliance with requirements, provide the named product or a comparable product by one of the following:

1.	Guardian Industries.
2.	Oldcastle Building Envelope.
3.	Pilkington Building Products North America.
4.	Vitro Architectural Glass (Formerly PPG Industries, Inc.) 5.	Viracon, Inc.

B.	 Source Limitations for Glass:	Obtain glass from a single source from a single manufacturer for each glass type.

1.	Obtain tinted glass from a single source from a single manufacturer.

2.	Obtain reflective-coated glass from a single source from a single manufacturer.

C.	 Source Limitations for Glazing Accessories: Obtain accessories from a single source from a single manufacturer for each product and installation method.

2.2	PERFORMANCE REQUIREMENTS

A.	 General: Installed glazing systems shall withstand normal thermal movement and wind and impact loads (where applicable) without failure, including loss or glass breakage attributable to the following: defective manufacture, fabrication, or installation; failure of

21-11972                                                      GLAZING                                           088000 - 3 of 12 Addendum 01 Storefront Package

sealants or gaskets to remain watertight and airtight; deterioration of glazing materials; or other defects in construction.

B.	California Code of Regulations, Title 24, Part 6, California Energy Code.

1.	NFRC 100: Procedure for Determining Fenestration Product U-factors.”
2.	 NFRC 200 Procedure for Determining Fenestration Product Solar Heat Gain Coefficients at Normal Incidence.”
3.	NFRC 400: Procedure for Determining Fenestration Product Air Leakage.”

C.	 Structural Performance: Glazing shall withstand the following design loads within limits and under conditions indicated determined according to the California Building Code and ASTM E 1300.

1.	Design Wind Pressures: As indicated on Drawings.
2.	 Maximum Lateral Deflection: For glass supported on all four edges, limit center-of-glass deflection at design wind pressure to not more than 1/50 times the short-side length or 1 inch, whichever is less.
3.	 Differential Shading:	Design glass to resist thermal stresses induced by differential shading within individual glass lites.

D.	 Safety Glazing: Where safety glazing is indicated, provide glazing that complies with 16 CFR 1201, Category II.

E.	 Thermal and Optical Performance Properties:	Provide glass with performance properties specified, as indicated in manufacturer's published test data, based on procedures indicated below:

1.	For monolithic-glass lites, properties are based on units with lites 6 mm thick.
2.	 For insulating-glass units, properties are based on units of thickness indicated for overall unit and for each lite.
3.	 U-Factors:	Center-of-glazing values, according to NFRC 100 and based on LBL's WINDOW 5.2 computer program, expressed as Btu/sq. ft. x h x deg F.
4.	 Solar Heat-Gain Coefficient and Visible Transmittance: Center-of-glazing values, according to NFRC 200 and based on LBL's WINDOW 5.2 computer program.
5.	Visible Reflectance: Center-of-glazing values, according to NFRC 300.

2.3	GLASS PRODUCTS, GENERAL

A.	 Glazing Publications:	Comply with published recommendations of glass product manufacturers and organizations below unless more stringent requirements are indicated. Refer to these publications for glazing terms not otherwise defined in this Section or in referenced standards.

1.	GANA Publication: "Glazing Manual."
2.	 IGMA Publication for Insulating Glass: SIGMA TM-3000, "North American Glazing Guidelines for Sealed Insulating Glass Units for Commercial and Residential Use."

21-11972                                                      GLAZING                                           088000 - 4 of 12 Addendum 01 Storefront Package

B.	 Safety Glazing Labeling: Where safety glazing is indicated, permanently mark glazing with certification label of the SGCC or another certification agency acceptable to authorities having jurisdiction; label shall indicate manufacturer's name, type of glass, thickness, and safety glazing standard with which glass complies.

C.	 Insulating-Glass Certification Program: Permanently marked either on spacers or on at least one component lite of units with appropriate certification label of IGCC.

D.	 Thickness: Where glass thickness is indicated, it is a minimum. Provide glass that complies with performance requirements and is not less than the thickness indicated.

1.	Minimum Glass Thickness for Exterior Lites: 6 mm.
2.	 Thickness of Tinted Glass: Provide same thickness for each tint color indicated throughout Project.

E.	 Strength: Where annealed float glass is indicated, provide annealed float glass, heat-strengthened float glass, or fully tempered float glass as needed to comply with "Performance Requirements" Article. Where heat-strengthened float glass is indicated, provide heat-strengthened float glass or fully tempered float glass. Where fully tempered float glass is indicated, provide fully tempered float glass.

2.4	GLASS PRODUCTS

A.	Clear Annealed Float Glass: ASTM C 1036, Type I, Class I (clear), Quality-Q3.

B.	 Ultraclear Float Glass: ASTM C1036, Type I, Class I (clear), Quality-Q3; and with visible light transmission of not less than 91 percent.

C.	Tinted Annealed Float Glass: ASTM C 1036, Type I, Class 2 (tinted), Quality-Q3.

D.	 Heat-Strengthened Float Glass: ASTM C 1048, Kind HS (heat strengthened), Type I, Condition A (uncoated) unless otherwise indicated, Type I, Class 1 (clear) or Class 2 (tinted) as indicated, Quality-Q3.

1.	 Fabrication Process: By horizontal (roller-hearth) process with roll-wave distortion parallel to bottom edge of glass as installed unless otherwise indicated.

E.	 Fully Tempered Float Glass: ASTM C 1048, Kind FT (fully tempered), Condition A (uncoated) unless otherwise indicated, Type I, Class 1 (clear) or Class 2 (tinted) as indicated, Quality-Q3.

1.	 Fabrication Process:	By horizontal (roller-hearth) process with roll-wave distortion parallel to bottom edge of glass as installed unless otherwise indicated.

21-11972                                                      GLAZING                                           088000 - 5 of 12 Addendum 01 Storefront Package

2.5	INSULATING GLASS
A.	 Insulating-Glass Units: Factory-assembled units consisting of sealed lites of glass separated by a dehydrated interspace, qualified according to ASTM E 2190.

1.	 Sealing System: Dual seal, with manufacturer's standard primary and secondary seals.
2.	 Spacer: Manufacturer's standard spacer material and construction, aluminum with mill or clear anodic finish.
3.	Desiccant: Molecular sieve or silica gel, or blend of both.

B.	 Glass:	Comply with applicable requirements in Part 3 Article "Insulating Glass Schedule."

1.	 Provide Kind HS (Heat-strengthened) or Kind FT (Fully tempered) float glass in place of annealed glass where needed to resist thermal stresses induced by differential shading of individual glass lites and to comply with glass design requirements specified in Part 1 "Performance Requirements" Article.

2.6	GLAZING SEALANTS

A.	 General:	Provide products of type indicated, complying with the following requirements:

1.	 Compatibility:	Compatible with one another and with other materials they contact, including glass products, seals of insulating-glass units, and glazing channel substrates, under conditions of service and application, as demonstrated by sealant manufacturer based on testing and field experience.
2.	 Suitability: Comply with sealant and glass manufacturers' written instructions for selecting glazing sealants suitable for applications indicated and for conditions existing at time of installation.
3.	 VOC Content: Field applied sealants shall have a VOC content of not more than 250 g/L.
4.	 Colors of Exposed Glazing Sealants:	As selected by Architect from manufacturer's full range.

B.	 Glazing Sealant: Neutral-curing silicone glazing sealant complying with ASTM C 920, Type S, Grade NS, Class 100/50, Use NT.

1.	Products: Subject to compliance with requirements, provide one of the following:

a.	Dow Corning Corporation; 790.
b.	GE Advanced Materials - Silicones; SilPruf LM SCS2700. c.	Tremco Incorporated; Spectrem 1.

21-11972                                                      GLAZING                                           088000 - 6 of 12 Addendum 01 Storefront Package

2.7	GLAZING TAPES

A.	 Back-Bedding Mastic Glazing Tapes:	Preformed, butyl-based, 100 percent solids elastomeric tape; nonstaining and nonmigrating in contact with nonporous surfaces; with or without spacer rod as recommended in writing by tape and glass manufacturers for application indicated; and complying with ASTM C 1281 and AAMA 800 for products indicated below:

1.	AAMA 806.3 tape, for glazing applications in which tape is subject to continuous pressure.
2.	AAMA 807.3 tape, for glazing applications in which tape is not subject to continuous pressure.

B.       Expanded Cellular Glazing Tapes: Closed-cell, PVC foam tapes; factory coated with adhesive on both surfaces; and complying with AAMA 800 for the following types:

1.	AAMA 810.1, Type 1, for glazing applications in which tape acts as the primary sealant.
2.	AAMA 810.1, Type 2, for glazing applications in which tape is used in combination with a full bead of liquid sealant.

2.8	MISCELLANEOUS GLAZING MATERIALS

A.	 General: Provide products of material, size, and shape complying with referenced glazing standard, requirements of manufacturers of glass and other glazing materials for application indicated, and with a proven record of compatibility with surfaces contacted in installation.

B.	 Cleaners, Primers, and Sealers:	Types recommended by sealant or gasket manufacturer.

C.	 Setting Blocks:	Type recommended by sealant or glass manufacturer; EPDM, Silicone, Neoprene, or Santoprene; with a Shore A durometer hardness of 85, plus or minus 5.

D.	 Spacers: Type recommended by sealant or glass manufacturer; neoprene blocks or continuous extrusions of hardness required by glass manufacturer to maintain glass lites in place for installation indicated.

E.	 Edge Blocks: Type recommended by sealant or glass manufacturer; EPDM, Silicone, Neoprene, or Santoprene; with a Shore A durometer hardness per manufacturer’s written instructions.

F.	 Cylindrical Glazing Sealant Backing: ASTM C1330, Type O (open-cell material), of size and density to control glazing sealant depth and otherwise produce optimum glazing sealant performance.

21-11972                                                      GLAZING                                           088000 - 7 of 12 Addendum 01 Storefront Package

2.9	FABRICATION OF GLAZING UNITS

A.	 Fabricate glazing units in sizes required to fit openings indicated for Project, with edge and face clearances, edge and surface conditions, and bite complying with written instructions of product manufacturer and referenced glazing publications, to comply with system performance requirements.

1.	Allow for thermal movements from ambient and surface temperature changes acting on glass framing members and glazing components.

a.	Temperature Change: 120 deg F ambient; 180 deg F material surfaces.

PART 3 - EXECUTION

3.1	EXAMINATION

A.	 Examine framing, glazing channels, and stops, with Installer present, for compliance with the following:

1.	 Manufacturing and installation tolerances, including those for size, squareness, and offsets at corners.
2.	Presence and functioning of weep system. 3.	Minimum required face or edge clearances.
4.	Effective sealing between joints of glass-framing members.

B.	Proceed with installation only after unsatisfactory conditions have been corrected.

3.2	PREPARATION

A.	 Clean glazing channels and other framing members receiving glass immediately before glazing. Remove coatings not firmly bonded to substrates.

B.	 Examine glazing units to locate exterior and interior surfaces. Label or mark units as needed so that exterior and interior surfaces are readily identifiable. Do not use materials that will leave visible marks in the completed work.

3.3	GLAZING, GENERAL

A.	 Comply with combined written instructions of manufacturers of glass, sealants, gaskets, and other glazing materials, unless more stringent requirements are indicated, including those in referenced glazing publications.

B.	 Protect glass edges from damage during handling and installation. Remove damaged glass from Project site and legally dispose of off Project site. Damaged glass is glass with edge damage or other imperfections that, when installed, could weaken glass and impair performance and appearance.

C.	Apply primers to joint surfaces where required for adhesion of sealants.

21-11972                                                      GLAZING                                           088000 - 8 of 12 Addendum 01 Storefront Package

D.	 Install setting blocks in sill rabbets, sized and located to comply with referenced glazing publications, unless otherwise required by glass manufacturer. Set blocks in thin course of compatible sealant suitable for heel bead.

E.	 Do not exceed edge pressures stipulated by glass manufacturers for installing glass lights.

F.	Provide spacers for glass lights where length plus width is larger than 50 inches.

1.	 Locate spacers directly opposite each other on both inside and outside faces of glass. Install correct size and spacing to preserve required face clearances, unless gaskets and glazing tapes are used that have demonstrated ability to maintain required face clearances and to comply with system performance requirements.
2.	 Provide 1/8-inch minimum bite of spacers on glass and use thickness equal to sealant width.	With glazing tape, use thickness slightly less than final compressed thickness of tape.

G.	 Provide edge blocking where indicated or needed to prevent glass lites from moving sideways in glazing channel, as recommended in writing by glass manufacturer and according to requirements in referenced glazing publications.

H.	 Set glass lites in each series with uniform pattern, draw, bow, and similar characteristics.

I.	 Set glass lites with proper orientation so that coatings face exterior or interior as specified.

J.	 Where wedge-shaped gaskets are driven into one side of channel to pressurize sealant or gasket on opposite side, provide adequate anchorage so gasket cannot walk out when installation is subjected to movement.

K.	 Square cut wedge-shaped gaskets at corners and install gaskets in a manner recommended by gasket manufacturer to prevent corners from pulling away; seal corner joints and butt joints with sealant recommended by gasket manufacturer.

3.4	TAPE GLAZING

A.	 Position tapes on fixed stops so that, when compressed by glass, their exposed edges are flush with or protrude slightly above sightline of stops.

B.	 Install tapes continuously, but not necessarily in one continuous length. Do not stretch tapes to make them fit opening.

C.	 Cover vertical framing joints by applying tapes to heads and sills first and then to jambs. Cover horizontal framing joints by applying tapes to jambs and then to heads and sills.

D.	 Place joints in tapes at corners of opening with adjoining lengths butted together, not lapped. Seal joints in tapes with compatible sealant approved by tape manufacturer.

21-11972                                                      GLAZING                                           088000 - 9 of 12 Addendum 01 Storefront Package

E.	 Do not remove release paper from tape until immediately before each glazing unit is installed.

F.	 Center glass lites in openings on setting blocks and press firmly against tape by inserting dense compression gaskets formed and installed to lock in place against faces of removable stops.	Start gasket applications at corners and work toward centers of openings.

G.	Apply cap bead of elastomeric sealant over exposed edge of tape.

3.5	GASKET GLAZING (DRY)

A.	 Cut compression gaskets to lengths recommended by gasket manufacturer to fit openings exactly, with allowance for stretch during installation.

B.	 Insert soft compression gasket between glass and frame or fixed stop so it is securely in place with joints miter cut and bonded together at corners.

C.	 Installation with Drive-in Wedge Gaskets: Center glass lites in openings on setting blocks and press firmly against soft compression gasket by inserting dense compression gaskets formed and installed to lock in place against faces of removable stops. Start gasket applications at corners and work toward centers of openings. Compress gaskets to produce a weathertight seal without developing bending stresses in glass. Seal gasket joints with sealant recommended by gasket manufacturer.

D.	 Installation with Pressure-Glazing Stops: Center glass lites in openings on setting blocks and press firmly against soft compression gasket. Install dense compression gaskets and pressure-glazing stops, applying pressure uniformly to compression gaskets.	Compress gaskets to produce a weathertight seal without developing bending stresses in glass. Seal gasket joints with sealant recommended by gasket manufacturer.

E.	Install gaskets so they protrude past face of glazing stops.

3.6	SEALANT GLAZING (WET)

A.	 Install continuous spacers, or spacers combined with cylindrical sealant backing, between glass lights and glazing stops to maintain glass face clearances and to prevent sealant from extruding into glass channel and blocking weep systems until sealants cure. Secure spacers or spacers and backings in place and in position to control depth of installed sealant relative to edge clearance for optimum sealant performance.

B.	 Force sealants into glazing channels to eliminate voids and to ensure complete wetting or bond of sealant to glass and channel surfaces.

C.	Tool exposed surfaces of sealants to provide a substantial wash away from glass.

21-11972                                                      GLAZING                                         088000 - 10 of 12 Addendum 01 Storefront Package

3.7	CLEANING AND PROTECTION

A.	Immediately after installation remove nonpermanent labels and clean surfaces.

B.	 Protect glass from contact with contaminating substances resulting from construction operations. Examine glass surfaces adjacent to or below exterior concrete and other masonry surfaces at frequent intervals during construction, but not less than once a month, for buildup of dirt, scum, alkaline deposits, or stains.

1.	 If, despite such protection, contaminating substances do come into contact with glass, remove substances immediately as recommended in writing by glass manufacturer. Remove and replace glass that cannot be cleaned without damage to coatings.

C.	Remove and replace glass that is damaged during construction period.

3.8	MONOLITHIC GLASS SCHEDULE

A.	Glass Type TG: Clear fully tempered float glass.

1.	Thickness: 6.0 mm.

2.	Safety glazing required.

3.9	INSULATING-GLASS SCHEDULE

A.	Glass Type IG: Ultra clear, fully tempered insulating glass.

1.	Basis of Design: Drawings and Specifications are based on the following:

a.	Ultraclear Float Glass

2.	Overall Unit Thickness: 1-inch (25mm).
3.	Minimum Thickness of Each Glass Lite: 6.0 mm. 4.	Indoor Lite: Clear, fully tempered float glass.
5.	Indoor Lite: Clear, fully tempered float glass. 6.	Interspace Content: Clean-Dry-Air.
7.	Low-E Coating: Pyrolytic or sputtered on second surface. 8.	Visible transmittance: 91 Percent
9.	Winter Nighttime U-Factor: 1.02 maximum. 10.	Solar Heat Gain Coefficient: 0.90
11.	Provide safety glazing labeling.

B.	Glass Type IT: Low-e coated, fully tempered insulating glass.

1.	Basis of Design: Drawings and Specifications are based on the following:

a.	PPG Industries, Inc.; Solarban 70XL

2. 3.

21-11972

Overall Unit Thickness: 1-inch (25mm). Thickness of Each Glass Lite: 6.0 mm.

GLAZING

088000 - 11 of 12 Addendum 01 Storefront Package

4.	Interspace Content: Clean-Dry-Air.
5.	Outdoor Lite: Heat strengthened Solargray Glass, fully tempered float glass. 6.	Indoor Lite: Clear float glass, fully tempered float glass.
7.	Low-E Coating: Pyrolytic or sputtered on second surface. 8.	Visible transmittance: 64 Percent
9.	Winter Nighttime U-Factor: 0.28 maximum. 10.	Summer Daytime U-Factor: 0.26 maximum. 11.	Solar Heat Gain Coefficient: 0.27.
12.	Provide safety glazing labeling where tempered glass is specified.

END OF SECTION

21-11972                                                      GLAZING                                         088000 - 12 of 12 Addendum 01 Storefront Package

ID	TaskTask Name Mod

1	NTP Project Prep 2
3

4	Site Utilities Cut/Cap/Relocate

5	Analyze Existing system

DuratioStart

1 day	Mon 8/9/21

17 days Wed 8/11/21

Finish

Mon 8/9/21

Thu 9/2/21

Pred

021	Qtr 4, 2021	Qtr 1, 2022	Qtr 2, 2022	Qtr 3, 202
     Aug	Sep	Oct	Nov	Dec	Jan	Feb	Mar	Apr	May	Jun	Jul	

1

6	Design relocation of low voltage and 5 days electrical

7	Install new conduits	7 days

Fri 8/27/21

Fri 9/3/21

Thu 9/2/21	5FF

Mon 9/13/21     6

8	pull new wire

9	cut over to existing system 10	remove eisting wire
11 12
13	Student Access South Pathway 14	Locate UG utilities
15	Remove existing trees 16	demo existing planter 17	Excavate foundations 18	Rebar foundations
19	Pour foundation

20	form / rebar retaining wall 21	Pour wall
22	Cure wall 23	Strip wall 24	Grade walk
25	For and Pour walk way 26	Install gas line stub
27	Install water stub

2 days	Tue 9/14/21

2 days	Thu 9/16/21

3 days	Mon 9/20/21

1 day	Thu 9/2/21

1 day	Thu 9/2/21

3 days	Fri 9/3/21

2 days	Wed 9/8/21

3 days	Fri 9/10/21

1 day	Wed 9/15/21

4 days	Thu 9/16/21

1 day	Wed 9/22/21

2 days	Thu 9/23/21

1 day	Mon 9/27/21

1 day	Tue 9/28/21

3 days	Wed 9/29/21

4 days	Wed 9/15/21

4 days	Tue 9/21/21

Wed 9/15/21     7

Fri 9/17/21	8

Wed 9/22/21     9

Thu 9/2/21	1

Thu 9/2/21	14SS

Tue 9/7/21	15

Thu 9/9/21	16

Tue 9/14/21	17

Wed 9/15/21     18

Tue 9/21/21	19

Wed 9/22/21     20

Fri 9/24/21	21

Mon 9/27/21     22

Tue 9/28/21	23

Fri 10/1/21	24

Mon 9/20/21     18

Fri 9/24/21	26

Project: CW Scheudle ADM 1	Task Date: Thu 9/23/21

Page 1

ID	TaskTask Name Mod

28	Install irrigation sleeve 29
30	Increment 1 - Earthwork / Demo

DuratioStart

1 day?	Mon 9/27/21

Finish

Mon 9/27/21

Pred

021	Qtr 4, 2021	Qtr 1, 2022	Qtr 2, 2022	Qtr 3, 202
     Aug	Sep	Oct	Nov	Dec	Jan	Feb	Mar	Apr	May	Jun	Jul	
27

31	Mobilize

32	Temp Facilities

2 days	Mon 10/4/21

3 days	Wed 10/6/21

Tue 10/5/21	10,1,

Fri 10/8/21	31

33                Cut and Cap Utilities                                2 days      Mon 10/11/21 Tue 10/12/21 32 34                Tree removal                                            3 days      Wed 10/13/21 Fri 10/15/21      33

35	Remove storm drain 36	Site demolition
37	Survey Building Pad

2 days	Mon 10/18/21 Tue 10/19/21 34

4 days	Wed 10/20/21 Mon 10/25/21 34,35

1 day	Tue 10/26/21 Tue 10/26/21 36

38	Building Pad	8 days	Wed 10/27/21 Fri 11/5/21	37

39	Relocate Fire Hydrant

40	Sewer

4 days	Mon 11/8/21

4 days	Fri 11/12/21

Thu 11/11/21 38

Wed 11/17/21 39

41	Storm Drain 42	Water
43 44
45	Projected Building Phase

3 days	Thu 11/18/21 Mon 11/22/21 40

3 days	Tue 11/23/21 Thu 11/25/21 41

46	Bid Period	20 days Fri 10/15/21	Thu 11/11/21

47                Letter of Intent                                         5 days      Fri 11/12/21      Thu 11/18/21 46 48                Procurement Period                                20 days Fri 11/19/21      Thu 12/16/21 47

49	DSA approval

50	Board Approval

1 day	Wed 12/1/21     Wed 12/1/21     38

Wed 12/8/21

51	Foundations

52	Underground utilities

15 days Fri 12/17/21

10 days Fri 1/7/22

Thu 1/6/22	48,42

Thu 1/20/22	51

53	Slab on grade	5 days	Fri 1/21/22	Thu 1/27/22	52

54	Structural Steel

55	Rough Carpentry

10 days Fri 1/28/22

35 days Fri 2/11/22

Thu 2/10/22	53

Thu 3/31/22	54

Project: CW Scheudle ADM 1	Task Date: Thu 9/23/21

Page 2

ID	TaskTask Name Mod

56	Exterior Finishes 57	Interior rough in 58	Interior Finishes
59	Exterior site work

DuratioStart

45 days Fri 4/1/22

25 days Fri 4/1/22

60 days Fri 5/6/22

23 days Fri 6/3/22

Finish

Thu 6/2/22

Thu 5/5/22

Thu 7/28/22

Tue 7/5/22

Pred

021	Qtr 4, 2021	Qtr 1, 2022	Qtr 2, 2022	Qtr 3, 202
     Aug	Sep	Oct	Nov	Dec	Jan	Feb	Mar	Apr	May	Jun	Jul	
55,70

55

57

56

60	Project Complete	1 day?	Fri 7/29/22	Fri 7/29/22	58 61
62

63	Aluminum Window Package

64	Bid Period	13 days Mon 9/13/21     Wed 9/29/21

65	Letter of Intent	5 days	Thu 9/30/21	Wed 10/6/21     64 66	Design Period	20 days Thu 10/7/21	Wed 11/3/21     65 67	DSA approval	35 days Thu 11/4/21	Wed 12/22/21 66 68	Board Approval of Design	7 days	Thu 10/7/21	Fri 10/15/21	65 69	Board Approval for Construction	7 days	Thu 12/23/21 Fri 12/31/21	67 70	Procurement and Fabrication	60 days Mon 1/3/22	Fri 3/25/22	69

Project: CW Scheudle ADM 1	Task Date: Thu 9/23/21

Page 3