CLOVIS UNIFIED SCHOOL DISTRICT
615 W. STUART AVENUE
COLE ELEMENTARY SCHOOL REROOF
NOT TO SCALE
SYLMAR
3/9/2023 1:29 PM G:\Clovis USD-1087\108722001-Reroof of Cole Elementary\300 CAD\340 Sheet Sets\01_General\G1 COVER.dwg -Stephen Grisez
COVER
GENERAL
615 W. STUART AVENUE
CLOVIS UNIFIED SCHOOL DISTRICT
COLE ELEMENTARY SCHOOL REROOF

APPLICABLE CODES

ALL WORK AND MATERIALS SHALL BE PERFORMED AND INSTALLED IN COMPLIANCE WITH THE FOLLOWING CODES AS ADOPTED AND AMENDED BY THE GOVERNING JURISDICTION.

APPLICABLE SECTIONS OF THE CALIFORNIA ENERGY CONSERVATION STANDARDS

Title 24 CCR, PART 1, 2022 Building Standards Administrative Code Title 24, CCR, Part 2, 2022 CBC
Title 24, CCR, Part 3, 2022 CEC Title 24, CCR, Part 4, 2022 CMC Title 24, CCR, Part 5, 2022 CPC Title 24, CCR, Par 9, 2022 CFC
Title 24, CCR, Part 12, 2022 California Referenced Standards Code Title 19, CCR, 2022, Public Safety, State Fire Marshall Regulations
	
GENERAL NOTES
	
PROVIDE THE LABOR, MATERIALS, ADMINISTRATION, FACILITIES, EQUIPMENT, TRANSPORTATION, INSURANCE, LICENSES, PERMITS, & EXPERTISE NECESSARY TO INTEGRATE THE WORK INTO THE TOTAL BUILDING SO THAT NO LEAKAGE INTO THE ROOF SYSTEM OR BUILDING OCCURS.

2. DO NOT ALLOW ANY ROOF LEAK TO INTERRUPT SCHOOL.

3. ALL WORK IS TO BE COORDINATED WITH CLOVIS UNIFIED.

4. SECURE & PAY FOR REQUIRED PERMITS, LICENCES, & INSPECTIONS. SECURE & PAY FOR REQUIRED PERMITS, LICENCES, & INSPECTIONS.

5. SUPERVISE & DIRECT THE WORK USING THE BEST SKILL & ATTENTION.

SHEET LIST
	
NO	SHEET	DESCRIPTION
	
GENERAL
1	G1	COVER
2	G2	SHEET INDEX ARCHITECTURAL
3	A1-R	LIBRARY
4	A2-R	MPR - MULTI PURPOSE ROOM 5	A3-R               WING NO 1 & WING NO 2
6	A4-R	WING NO 3 & MODULAR NO 1 7	A5-R	WING NO 4
8	A6-R	ADMIN
9	A7-R	CORRIDOR
10	A500	CONSTRUCTION DETAILS
11	A501	CONSTRUCTION DETAILS

GENERAL SCOPE OF REROOF WORK

1.	REMOVE EXISTING ASPHALT SHINGLE AND BUILT-UP ROOFING SYSTEMS & INSULATION AT LOCATIONS INDICATED ON DRAWINGS DOWN TO THE PLYWOOD SUBSTRATE. REMOVE ALL DEBRIS RESULTING FROM WORK FROM SITE AND DISPOSE OF.

2.	 REMOVE EXISTING SHEET METAL FLASHINGS WHERE INDICATED ON DRAWINGS. INSTALL NEW 24 GA. GALVANIZED IRON AND/OR PBC-CLAD METAL FLASHINGS WHERE INDICATED ON DRAWINGS OR WHERE REQUIRED BY ROOFING MATERIALS MANUFACTURER FOR THEIR FULLY WARRANTED ROOF SYSTEMS.

3.	 REMOVE AND CAREFULLY STORE EXISTING SHEET METAL FLASHINGS AND ROOFTOP ELEMENTS WHERE INDICATED ON DRAWINGS. REINSTALL EXISTING ELEMENTS AS PART OF NEW MEMBRANE ROOFING OR SHINGLE UNDERLAYMENT IN ACCORANCE WITH DETAILS ON DRAWINGS. TOUCH-UP DAMAGED PAINT AS REQUIRED TO RESTORE TO PREVIOUS CONDITION. REPLACE STORED ELEMENTS WHICH ARE DAMAGED DURING CONSTRUCTION AT CONTRACTOR’S EXPENSE.
PROJECT LOCATION	4.	REMOVE AND DISPOSE OF EXISTING SHEET METAL EXPANSION JOINTS. INSTALL NEW EXPANSION JOINTS IN ACCORDANCE WITH DRAWINGS.

5.	DISASSEMBLE EXISTING ROOF DRAINS AND REASSEMBLE IN WATERTIGHT CONDITION AS PART OF NEW ROOF SYSTEM. REPLACE EXISTING DRAIN BOLTS AND WASHERS WITH NEW, STAINLESS-STEEL PARTS. REPLACE DAMAGED OR MISSING DRAIN STRAINERS.
CLOVIS
6.	INSTALL NEW LOW-PROFILE ROOF VENTS AS PART OF ASPHALT SHINGLE ROOFING SYSTEMS IN HIGH AND LOW CONFIGURATION AS REQUIRED TO PROPERLY VENT ATTIC SPACES. COLOR TO COMPLEMENT SHINGLE ROOF SYSTEM COLOR.

7.	REPLACE DAMAGED OR DEFECTIVE PLYWOOD PANELS AS DIRECTED BY OWNER’S REPRESENTATIVE. CONTRACTOR TO PROVIDE UNIT PRICE PER 4’ X 8’ DAMAGED PLYWOOD PANEL OF MATCHING THICKNESS (INCLUDES LABOR AND MATERIAL) ON BID FORM. CONTRACTOR TO INCLUDE SPECIFIED NUMBER OF PLYWOOD PANELS OF EQUAL THICKNESS IN BASE BID. CONTRACTCOR TO PROVIDE UNIT PRICE PER 4’ X 8’ PLYWOOD PANEL ON BID FORM FOR INSTALLATION AS APPROVED BY OWNER.

8.	INSTALL MINIMUM ¼” THICKNESS GYPSUM COVERBOARD OVER PLYWOOD ROOF DECKS AT AREAS INDICATED ON
DRAWINGS. SECURE GYPSUM COVERBOARDS TO SUBSTRATE USING APPROVED MECHANICAL FASTENERS PER PROJECT LOCATION	SPECIFICATIONS AND MANUFACTURER REQUIREMENTS. INSTALL ½” THICKNESS PRODUCT WHERE REQURIED BY
MANUFACTURER BASED ON MANUFACTURER WARRANTY.
FRESNO	9.	INSTALL FULLY-ADHERED 80 MIL. THERMOPLASTIC PVC SINGLE-PLY ROOF SYSTEM AT LOCATIONS INDICATED ON DRAWINGS IN ACCORDANCE WITH SPECIFICATIONS AND MANUFACTURER REQUIRMENTS. ROOF TO HAVE CLASS “A” FIRE-RATING.

10.      REMOVE EXISTING COPING WHERE INDICATED ON DRAWINGS AND INSTALL NEW ENGINEERED (ES-1) COPING SYSTEM. COLOR TO BE APPROVED BY BUILDNG OWNER.

11.      POWERWASH EXISTING METAL ROOFS TO REMOVE SURFACE DIRT AND CONTAMINATION. APPLY PRIMER TO METAL ROOF SURFACES (INCLUDING RIBS) AND SILICONE COATING SYSTEM WITH POLYESTER FABRIC ON ALL FIELD SEAMS AND RIBS. SEE SPECS FOR REQUIREMENTS. REPLACE GUTTERS AND DOWNSPOUTS WHERE INDICATED ON DRAWINGS.
VICINITY MAP	12.      INSTALL NEW LAMINATED ASPHALT SHINGLE ROOF SYSTEMS AND RELATED FLASHINGS AT LOCATIONS INDICATED
NOT TO SCALE	 ON DRAWINGS OVER SYTHETIC ROOF UNDERLAYMENT. REPLACE EXISTING VALLEY FLASHINGS WITH NEW VALLEY METAL PER CODE REQUIREMENTS. PROVIDE MANUFACTURER LIMITED LIFETIME WARRANTY AND CONTRACTOR
3-YEAR, LEAKPROOF GUARANTEE.

13.      INSTALL NEW 24 GAUGE GALVANIZED FLASHINGS AT LOCATIONS INDICATED ON DRAWINGS, OR AS REQUIRED TO PROVIDE PROPER FLASHING OF ROOF SYSTEMS IN COMPLIANCE WITH PROJECT DESIGN DOCUMENTS, MANUFACTURER AND CODE REQUIREMENTS.

14.      INSTALL NEW CLAD METAL FLASHINGS AT LOCATIONS WHERE INDICATED ON DRAWINGS. HEAT-WELD PVC MEMBRANE TO FLASHINGS IN WATERTIGHT CONDITION.

15.      ATTENDANCE AT SCHEDULED PRE-BID WALK-THROUGH IS MANDATORY TO SUBMIT A BID FOR THE PROJECT. W. STUART
16.      QUALITY ASSURANCE SHALL BE PROVIDED BY BROOKS & ASSOCIATES, A DIVISION OF PROVOST & PRITCHARD
SITE MAP	CONSULTING GROUP, THE OWNER’S REPRESENTATIVE.
17.      CONTRACTOR SHALL PROVIDE A GUARANTEE TO MAINTAIN THE ROOF SYSTEM IN WATERTIGHT CONDITION FOR A
PERIOD OF THREE (3) YEARS IN ACCORDANCE WITH THE PROJECT SPECIFICATIONS.

18.      PROVIDE MANUFACTURER’S NO-DOLLAR LIMIT ROOF SYSTEM GUARANTEE FOR PVC ROOF SYSTEMS FOR PERIOD OF TWENTY (20) YEARS.

19.      PROVIDE MANUFACTURER LIFETIME SHINGLE WARRANTY.

20.      ALL INFORMATION CONTAINED IN THE PROJECT SPECIFICATIONS, DRAWINGS, AND ADDENDA SHALL BE CONSIDERED A PART OF AND SUPPLEMENTARY TO THE OUTLINE OF THE PROJECT AND SHALL INCLUDED IN THE BID FOR THE WORK.

21.      ALL DIMENSIONS INDICATED ON THE DRAWINGS ARE NOMINAL. CONTRACTOR SHALL BE RESPONSIBLE FOR ACCURATE MEASUREMENTS AT THE PROJECT SITE.

			

			

		
	DESIGN CONSULTANT: TROY BROOKS
	
	DRAFTED BY: SG
	CHECKED BY: TT
	
	DATE: 3/9/23
	
	JOB NO: 108722001
	
	PROJECT NO:
	
	PHASE:
	
	0	1"
ORIGINAL SCALE SHOWN IS ONE INCH. ADJUST SCALE FOR REDUCED OR ENLARGED PLANS.
	
	SHEETG1
	
	1	OF	11

3/9/2023 1:29 PM G:\Clovis USD-1087\108722001-Reroof of Cole Elementary\300 CAD\340 She
eneral\G2 SHEET INDEX.dwg -Stephen Grisez
SHEET INDEX
GENERAL
615 W. STUART AVENUE
CLOVIS UNIFIED SCHOOL DISTRICT
COLE ELEMENTARY SCHOOL REROOF
ADMIN, SEE SHEET A6-R
CORRIDOR, SEE SHEET A7-R

LIBRARY, SEE SHEET A1-R

WING NO 4, SEE SHEET A5-R

WING NO 1 & WING NO 2, SEE SHEET A3-R

SCALE IN FEET

0	10	20	40

			

			

		
	DESIGN CONSULTANT: TROY BROOKS
	
	DRAFTED BY: SG
	CHECKED BY: TT
	
	DATE: 3/9/23
	
	JOB NO: 108722001
	
	PROJECT NO:
	
	PHASE:
	
	0	1"
ORIGINAL SCALE SHOWN IS ONE INCH. ADJUST SCALE FOR REDUCED OR ENLARGED PLANS.
	
	SHEETG2
	
	2	OF	11

	WIN
	G N
	O 3 &
	MO
	DULA
	R N
	O 1, S
	EE
	SHEE
	T A
	4-R

ts\01_G
	
MPR - MULTI PURPOSE ROOM, SEE SHEET A2-R

et

5'-0"±
18'-2"±
1'-7"±
29'-1"±
1'-11"±
11'-2"±
8'-4"±
28'-11"±
5'-1"±
3/4"/12"
3/9/2023 1:29 PM
7\108722001-Reroof of Cole Elementary\300 CAD\340 Sheet Sets\02_Roof Plan\A1-R LIBRARY.dwg -Stephen Grisez
LIBRARY
ARCHITECTURAL
615 W. STUART AVENUE
CLOVIS UNIFIED SCHOOL DISTRICT
COLE ELEMENTARY SCHOOL REROOF

21'-3"±

26'-3"±

19'-6"±

31'-10"±	16'-10"±

KEY NOTES - LIBRARY	

1.     REMOVE EXISTING BUILT-UP ROOFING SYSTEM AND ASSOCIATED FLASHINGS DOWN TO THE STRUCTURAL PLYWOOD DECK. CONTRACTOR TO INSPECT EXISTING     DECK     AND     COMMUNICATE     ANY      DAMAGE     TO      OWNER'S REPRESENTATIVE. CONTACTOR TO CONDUCT A FASTENER PULL OUT TEST PER MANUFACTURERS REQUIREMENTS. CONTRACTOR TO INSTALL NEW PVC ROOFING SYSTEM PER PROJECT SPECIFICATIONS AND MANUFACTURER REQUIREMENTS.
2. CONTRACTOR     TO     REMOVE     AND     DISPOSE     OF     EXISTING     FLASHINGS. CONTRACTOR     TO     CLEAN     EACH     PENETRATION     PER     MANUFACTURER REQUIREMENT AND CONTRACTOR TO INSTALL NEW PIPE PENETRATION FLASHING PER DETAIL 16/A501 TYP., AND MANUFACTURER REQUIREMENTS.
3.     CONTRACTOR TO REMOVE EXISTING COPING SYSTEM AND DISPOSE OF. CONTRACTOR TO INSTALL NEW (ES-1) ENGINEERED COPING SYSTEM SIMILAR TO DETAIL 14/A501. OWNER TO APPROVE COLOR.
4. CONTRACTOR TO REMOVE AND STORE EXISTING COUNTERFLASHING SYSTEMS     FOR     REINSTALLATION     WHERE     INDICATED     ON     DRAWINGS. CONTRACTOR TO PROVIDE NEW COUNTERFLASHING AT OWN EXPENSE IF DAMAGED DURING CONSTRUCTION. CONTRACTOR TO REINSTALL EXISTING FLASHIG SIMILAR TO DETAIL 3/A500.
5.     CONTRACTOR TO INSTALL NEW COUNTERFLASHING SYSTEMS AT CURBS SIMILAR TO DETAIL 5/A500. SEE SPECS FOR REQUIREMENTS.
6.     CONTRACTOR TO DISASSEMBLE AND CLEAN EXISTING ROOF DRAINS AND OVERFLOWS. CONTRACTOR TO INSTALL NEW ROOFING SYSTEM IN AND AROUND PER MANUFACTURER REQUIREMENTS AND PER DETAIL 6/A500 CONTRACTOR     TO     REPLACE     BOLTS     AND     WASHERS     PER     PROJECT SPECIFICATIONS. CONTRACTOR TO REPLACE DRAIN STRAINERS IF MISSING
22'-7"±	22'-2"±	OR DAMAGED.
7.     CONTRACTOR TO REMOVE EXISTING EXPANSION JOINT FLASHING AND INSTALL      NEW      SIMILAR      TO      DETAIL      13/A501      PER      MANUFACTURER REQUIREMENTS.
8. EXISTING PLYWOOD CRICKETS TO REMAIN.
9. ROOF AREA NOT A PART OF PROJECT.
NOTES	10. CONTRACTOR TO REMOVE EXISTING COPING, INSTALL NEW PER DETAIL
17/A501 THE DIMENSIONS ON THE DRAWING DO NOT
REFLECT ROOF SLOPE. CONTRACTOR RESPONSIBLE FOR MEASURING EACH ROOF AREA.

			

			

		
	DESIGN CONSULTANT: TROY BROOKS
	
	DRAFTED BY: SG
	CHECKED BY: TT
	
	DATE: 3/9/23
	
	JOB NO: 108722001
	
	PROJECT NO:
	
	PHASE:
	
	0	1"
ORIGINAL SCALE SHOWN IS ONE INCH. ADJUST SCALE FOR REDUCED OR ENLARGED PLANS.
	
	SHEETA1-R
	
	3	OF	11

23'-6"±	100'-5"±

60'-1"±
18'-1"±
RIDGE

40'-10"±
3-1/2"/12"
KEY NOTES - MPR AND PUMP HOUSE	

1. REMOVE     EXISTING     ASPHALT     SHINGLE     ROOFING     SYSTEM     AND ASSOCIATED FLASHINGS DOWN TO THE STRUCTURAL PLYWOOD DECK. CONTRACTOR TO INSPECT EXISTING DECK AND COMMUNICATE ANY DAMAGE TO OWNER'S REPRESENTATIVE. CONTRACTOR TO CONDUCT A FASTENER PULL OUT TEST PER MANUFACTURERS REQUIREMENTS. CONTRACTOR TO INSTALL REFLECTIVE LAMINATED ASPHALT SHINGLE ROOFING SYSTEM OVER NEW SYNTHETIC UNDERLAYMENT PER PROJECT SPECIFICATIONS AND MANUFACTURER REQUIREMENTS.

MPR - MULTI PURPOSE ROOM
615 W. STUART AVENUE
CLOVIS UNIFIED SCHOOL DISTRICT
COLE ELEMENTARY SCHOOL REROOF
2.REMOVE EXISTING BUILT-UP ROOFING SYSTEM AND ASSOCIATED FLASHINGS DOWN TO THE STRUCTURAL PLYWOOD DECK. CONTRACTOR TO INSPECT EXISTING DECK AND COMMUNICATE ANY DAMAGE TO OWNER'S REPRESENTATIVE. CONTRACTOR TO CONDUCT A FASTENER PULL OUT TEST PER MANUFACTURERS REQUIREMENTS. CONTRACTOR TO INSTALL NEW PVC ROOFING SYSTEM PER PROJECT SPECIFICATIONS AND MANUFACTURER REQUIREMENTS.

3/9/2023 1:29 PM G:\Clovis USD-1087\108722001-Reroof of Cole Elementary\300 CAD\340 Sheet Sets\02_Roof Plan\A2-R MPR - MULTI PURPOSE ROOM.dwg -Stephen Grisez
ARCHITECTURAL
3. CONTRACTOR TO INSTALL NEW CONTRACTOR TO REMOVE EXISTING FLASHING TO INSTALL NEW STEP- FLASHING, SIMILAR TO DETAIL 8/A500 CONTRACTOR TO REINSTALL COVER FLASHING OVER STEP- FLASHING.

19'-2"±
4.EXISTING PIPE PENETRATIONS. CONTRACTOR TO REMOVE AND DISPOSE EXISTING FLASHING SYSTEMS. CONTRACTOR TO CLEAN PENETRATION PER MANUFACTURER REQUIREMENTS. CONTRACTOR TO INSTALL NEW PIPE PENETRATION FLASHING PER DETAIL 7/A500 TYP.

5. CONTRACTOR TO REMOVE EXISTING EDGE METAL FLASHING AND INSTALL NEW PER DETAIL 11/A500. TYP.

6. CONTRACTOR TO REMOVE EXISTING EDGE METAL FLASHING AND GUTTER AND INSTALL NEW PER DETAIL 18/A501 TYP.

24'-1"±
7. CONTRACTOR TO REMOVE EXISTING FLASHINGS AND REINSTALL, PER DETAIL 5/A500.

8. CONTRACTOR TO REMOVE EXISTING FLASHING SYSTEM, AND INSTALL NEW COUNTER-FLASHING. CONTRACTOR TO CLEAN SCREEN SUPPORTS AND INSTALL NEW LIQUID FLASHING SIMILAR TO DETAIL 15/A501.

9. CONTRACTOR TO REMOVE EXISTING LOW SLOPE EXPANSION JOINT AND INSTALL NEW PER DETAIL 19/A501.

10. CONTRACTOR     TO     REMOVE     AND     DISPOSE     OF     EXISTING     PIPE PENETRATION, PATCH HOLE IN DECK WITH 20 GA. SHEET METAL.

11. CONTRACTOR TO INSTALL NEW TRANSITION FLASHING PER DETAIL 1/A500

50'-7"±	NOTES

THE DIMENSIONS ON THE DRAWING DO NOT REFLECT ROOF SLOPE. CONTRACTOR RESPONSIBLE FOR MEASURING EACH ROOF AREA.

DESIGN CONSULTANT:

TROY BROOKS

31'-11"±
DRAFTED BY:     CHECKED BY: RIDGE	SG	TT

20'-3"±
DATE: 3/9/23

JOB NO: 108722001 PUMP HOUSE	PROJECT NO:

PHASE:

0	1"

ORIGINAL SCALE SHOWN IS ONE

INCH. ADJUST SCALE FOR 25'-2"±	REDUCED OR ENLARGED PLANS.

SHEETA2-R

4	OF	11

50'-2"±
6'-8"±
WING NO 1
2-1/2"/12"
3/9/2023 1:30 PM G:\Clovis USD-1087\108722001-Reroof of C
F

L REROO

TRICT E

O 2

						

RIDGE

ELEMENTARY SCHOOL

OVIS UNIFIED SCHOOL DIST 615 W. STUART AVENUE
ARCHITECTURAL

WING NO 1 & WING NO WING NO 2.dwg -Stephe Grisez

									
2-1/2"/12"

COLE E

CLO

W ole Elementary\300 CAD\340 Sheet Sets\02_Roof Plan\A3-R WING NO 1 & W

RIDGE

	

50'-2"±

WING NO 2
171'-8"±

29'-1"±

KEY NOTES - WING 1 AND WING 2
1. REMOVE EXISTING ASPHALT SHINGLE ROOFING SYSTEM AND ASSOCIATED FLASHINGS DOWN TO THE STRUCTURAL PLYWOOD DECK. CONTRACTOR TO INSPECT EXISTING DECK AND      COMMUNICATE      ANY      DAMAGE      TO      OWNER'S REPRESENTATIVE. CONTACTOR TO CONDUCT A FASTENER PULL OUT TEST PER MANUFACTURERS REQUIREMENTS. CONTRACTOR      TO      INSTALL      REFLECTIVE      LAMINATED ASPHALT SHINGLE ROOFING SYSTEM OVER NEW SYNTHETIC UNDERLAYMENT     PER     PROJECT     SPECIFICATIONS     AND MANUFACTURER REQUIREMENTS.
2.EXISTING PIPE PENETRATIONS. CONTRACTOR TO REMOVE AND DISPOSE EXISTING FLASHINGS. CONTRACTOR TO CLEAN PENETRATION PER MANUFACTURER REQUIREMENTS. CONTRACTOR     TO     INSTALL     NEW     PIPE     PENETRATION FLASHINGS PER DETAIL 7/A500 TYP AND MANUFACTURER REQUIREMENTS.
3. CONTRACTOR TO REMOVE EXISTING EXHAUST VENTS AND REINSTALL PER MANUFACTURER REQUIREMENTS.
4.CONTRACTOR TO REMOVE EXISTING LOW PROFILE EXHAUST VENTS AND REPLACE WITH NEW TO MATCH. CONTRACTOR TO INSTALL PER MANUFACTURER REQUIREMENTS.
5. CONTRACTOR TO REMOVE EXISTING EDGE METAL FLASHING AND INSTALL NEW PER DETAIL 11/A500 AND MANUFACTURER REQUIREMENTS.
6. CONTRACTOR TO REMOVE AND DISPOSE OF EXISTING ANTENNA ANCHOR POINTS. REPAIR OPENINGS IN DECK WITH 20 GAUGE METAL PLATE SECURED INTO FRAMING.
7. CONTRACTOR TO REMOVE EXISTING FLASHINGS AND REINSTALL PER DETAIL 4/A500.
8. CONTRACTOR TO REMOVE EXISTING VALLEY METAL AND
INSTALL     NEW     26     GAUGE     DOUBLE-RIB     VALLEY     PER 171'-8"±	MANUFACTURER REQUIREMENTS.

NOTES

THE DIMENSIONS ON THE DRAWING DO NOT REFLECT ROOF SLOPE. CONTRACTOR RESPONSIBLE FOR MEASURING EACH ROOF AREA.

			

			

		
	DESIGN CONSULTANT: TROY BROOKS
	
	DRAFTED BY: SG
	CHECKED BY: TT
	
	DATE: 3/9/23
	
	JOB NO: 108722001
	
	PROJECT NO:
	
	PHASE:
	
	0	1"
ORIGINAL SCALE SHOWN IS ONE INCH. ADJUST SCALE FOR REDUCED OR ENLARGED PLANS.
	
	SHEETA3-R
	
	5	OF	11

2-1/2"/12"
3/9/2023 1:30 PM G:\Clovis USD-1087\108722001-Reroof of Cole Elementary\300 CAD\340 Sheet Sets\02_Roof Plan\A4-R WING NO 3 & MODULAR NO 1.dwg -Stephen Grisez
WING NO 3 & MODULAR NO 1
ARCHITECTURAL
615 W. STUART AVENUE
CLOVIS UNIFIED SCHOOL DISTRICT
COLE ELEMENTARY SCHOOL REROOF

KEY NOTES - WING 3 AND MODULAR 1 NOTES
1. REMOVE EXISTING ASPHALT SHINGLE ROOFING SYSTEM AND ASSOCIATED FLASHINGS DOWN TO THE STRUCTURAL
THE DIMENSIONS ON THE DRAWING DO NOT	PLYWOOD DECK. CONTRACTOR TO INSPECT EXISTING DECK AND COMMUNICATE ANY DAMAGE TO OWNER'S REFLECT ROOF SLOPE. CONTRACTOR	REPRESENTATIVE. CONTRACTOR TO CONDUCT A FASTENER PULL OUT TEST PER MANUFACTURERS RESPONSIBLE FOR MEASURING EACH ROOF AREA.	REQUIREMENTS. CONTRACTOR TO INSTALL REFLECTIVE LAMINATED ASPHALT SHINGLE ROOFING SYSTEM OVER
NEW SYNTHETIC UNDERLAYMENT PER PROJECT SPECIFICATIONS AND MANUFACTURER REQUIREMENTS.
2. EXISTING PIPE PENETRATIONS. CONTRACTOR TO REMOVE AND DISPOSE EXISTING FLASHINGS. CONTRACTOR TO CLEAN PENETRATION PER MANUFACTURER REQUIREMENTS. CONTRACTOR TO INSTALL NEW PIPE PENETRATION FLASHING PER DETAIL 7/A500 TYP., AND MANUFACTURER REQUIREMENTS.
3. CONTRACTOR TO REMOVE EXISTING EXHAUST VENTS AND REINSTALL PER MANUFACTURER REQUIREMENTS.
4. CONTRACTOR TO REMOVE EXISTING LOW PROFILE EXHAUST VENTS AND REPLACE WITH NEW VENTS TO MATCH. CONTRACTOR TO INSTALL PER MANUFACTURER REQUIREMENTS.
5. CONTRACTOR TO REMOVE EXISTING EDGE METAL FLASHING AND INSTALL NEW PER DETAIL 11/A500 AND MANUFACTURER REQUIREMENTS.
6. CONTRACTOR TO REMOVE AND REINSTALL EXISTING HEAT STACK FLASHINGS PER MANUFACTURER REQUIREMENTS.
7. CONTRACTOR TO REMOVE EXISTING FLASHINGS AND INSTALL NEW STEP-FLASHING SIMILAR TO DETAIL 8/A500. CONTRACTOR TO REINSTALL COVER FLASHING OVER STEP-FLASHING.
8. CONTRACTOR TO REMOVE AND REINSTALL EXISTING ANTENNA, CONTRACTOR TO SAFELY STORE DURING PROJECT FOR REINSTALLATION.
9. CONTRACTOR TO REMOVE AND DISPOSE OF EXISTING EXPANSION JOINT SYSTEM AND INSTALL NEW PER DETAIL 2/A500.
10. CONTRACTOR TO THOROUGHLY CLEAN AND PREP METAL SURFACE FOR INSTALLATION OF SPECIFIED TAPE AND COATING SYSTEM. SEE SPECS FOR REQUIREMENTS.
11. CONTRACTOR TO REMOVE EXISTING GUTTER SYSTEM AND INSTALL NEW TO MATCH EXISTING PROFILE. OWNER TO PICK COLOR.
12. CONTRACTOR TO INSTALL NEW FLASHING AT PIPE PENETRATIONS, PER DETAIL 15/A501. TYP.

MODULAR NO 1

RIDGE

WING NO 3

			

			

		
	DESIGN CONSULTANT: TROY BROOKS
	
	DRAFTED BY: SG
	CHECKED BY: TT
	
	DATE: 3/9/23
	
	JOB NO: 108722001
	
	PROJECT NO:
	
	PHASE:
	
	0	1"
ORIGINAL SCALE SHOWN IS ONE INCH. ADJUST SCALE FOR REDUCED OR ENLARGED PLANS.
	
	SHEETA4-R
	
	6	OF	11

3/9/2023 1:30
-1087\108722001-Reroof of Cole Elementary\300 CAD\340 Sheet Sets\02_Roof Plan\A5-R WING NO 4.dwg -Stephen Grisez
WING
ARCHIT
615 W. STU
CLOVIS UNIFIED
COLE ELEMENTAR
2-1/2"/12"
AND INSTALL NEW PER DETA L 11/A500.
REFLECT ROOF SLOPE. CONTRACTOR

RIDGE

		

45'-4"±

SCHOOL REROOF

HOOL DISTRICT AVENUE
TURAL

O 4

Y S

SCH ART
ECT

NO

171'-10"±

WING NO 4

KEY NOTES - WING 4

1. REMOVE EXISTING ASPHALT SHINGLE ROOFING SYSTEM AND ASSOCIATED FLASHINGS DOWN TO THE STRUCTURAL PLYWOOD DECK.     CONTRACTOR     TO     INSPECT     EXISTING     DECK     AND COMMUNICATE ANY DAMAGE TO OWNER'S REPRESENTATIVE. CONTRACTOR TO CONDUCT A FASTENER PULL OUT TEST PER MANUFACTURERS REQUIREMENTS. CONTRACTOR TO INSTALL REFLECTIVE LAMINATED ASPHALT SHINGLE ROOFING SYSTEM OVER     NEW     SYNTHETIC     UNDERLAYMENT     PER     PROJECT SPECIFICATIONS AND MANUFACTURER REQUIREMENTS.
2.EXISTING PIPE PENETRATIONS. CONTRACTOR TO REMOVE AND DISPOSE EXISTING FLASHING SYSTEMS, CONTRACTOR TO CLEAN PENETRATION PER MANUFACTURER REQUIREMENTS. CONTRACTOR TO INSTALL NEW PIPE PENETRATION FLASHING PER DETAIL 7/A500 TYP.
NOTES	3. CONTRACTOR TO REMOVE EXISTING EXHAUST VENTS AND THE DIMENSIONS ON THE DRAWING DO NOT                                   REINSTALL PER MANUFACTURER REQUIREMENTS.
RESPONSIBLE FOR MEASURING EACH ROOF AREA.	4.CONTRACTOR TO REMOVE IEXISTING EDGE METAL FLASHING

			

			

		
	DESIGN CONSULTANT: TROY BROOKS
	
	DRAFTED BY: SG
	CHECKED BY: TT
	
	DATE: 3/9/23
	
	JOB NO: 108722001
	
	PROJECT NO:
	
	PHASE:
	
	0	1"
ORIGINAL SCALE SHOWN IS ONE INCH. ADJUST SCALE FOR REDUCED OR ENLARGED PLANS.
	
	SHEETA5-R
	
	7	OF	11

37'-4"±
5'-11"±
3'-0"±
25'-10"±
20'-7"±
2-1/2"/12"
3/9/2023 1:30 PM G:\Clovis USD-1087\108722001-Reroof of Cole Elementary\300 CAD\340 Sheet Sets\02_Roof Plan\A6-R ADMIN.dwg -Stephen Grisez
ADMIN
ARCHITECTURAL
615 W. STUART AVENUE
CLOVIS UNIFIED SCHOOL DISTRICT
COLE ELEMENTARY SCHOOL REROOF
CONTRACTOR TO INSPECT EXISTING DECK AND COMMUNICATE ANY
OWNER'S REPRESENTATIVE. CONTRACTOR TO CONDUCT A FASTENER
AND AROUND PER MANUFACTURER REQUIREMENTS AND PER DETAIL
MISSING OR DAMAGED.
REPLACE NEW, CONTRACTOR TO INSTALL PER MANUFACTURER
REQUIREMENTS.
INSTALL NEW PER DETAIL 11/A500, TYP.
REFLECT ROOF SLOPE. CONTRACTOR

106'-9"±

RIDGE

RIDGE

RIDGE

4'-0"±

18'-4"±

30'-7"±

KEY NOTES - ADMINISTRATION                                                                                                       6. CONTRACTOR TO DISASSEMBLE AND CLEAN EXISTING ROOF DRAINS 1. REMOVE     EXISTING     ASPHALT     SHINGLE     ROOFING     SYSTEM     AND                     AND OVERFLOWS. CONTRACTOR TO INSTALL NEW ROOFING SYSTEM IN ASSOCIATED FLASHINGS DOWN TO THE STRUCTURAL PLYWOOD DECK.                     6/A500 CONTRACTOR TO REPLACE BOLTS AND WASHERS PER PROJECT DAMAGE TO OWNER'S REPRESENTATIVE. CONTRACTOR TO CONDUCT A                     SPECIFICATIONS. CONTRACTOR TO REPLACE DRAIN STRAINERS IF
53'-7"±	FASTENER PULL OUT TEST PER MANUFACTURERS REQUIREMENTS.
CONTRACTOR TO INSTALL REFLECTIVE LAMINATED ASPHALT SHINGLE	7.EXISTING PIPE PENETRATIONS. CONTRACTOR TO REMOVE AND DISPOSE
ROOFING SYSTEM OVER NEW SYNTHETIC UNDERLAYMENT PER PROJECT                     EXISTING FLASHING SYSTEMS, CONTRACTOR TO CLEAN PENETRATION SPECIFICATIONS AND MANUFACTURER REQUIREMENTS.                                                    PER MANUFACTURER REQUIREMENTS. CONTRACTOR TO INSTALL NEW
2.REMOVE EXISTING BUILT-UP ROOFING SYSTEM AND ASSOCIATED	PIPE PENETRATION FLASHING PER DETAIL 7/A500 TYP.
FLASHINGS DOWN TO THE STRUCTURAL PLYWOOD DECK. CONTRACTOR	8. CONTRACTOR TO REMOVE EXISTING VALLEY METAL AND INSTALL NEW TO INSPECT EXISTING DECK AND COMMUNICATE ANY DAMAGE TO                     26 GAUGE DOUBLE-RIB VALLEY PER MANUFACTURER REQUIREMENTS.
PULL OUT TEST PER MANUFACTURERS REQUIREMENTS. CONTRACTOR	9. CONTRACTOR TO REMOVE EXISTING LOW PROFILE EXHAUST VENTS AND TO INSTALL NEW PVC ROOFING SYSTEM PER PROJECT SPECIFICATIONS
AND MANUFACTURER REQUIREMENTS.
3. CONTRACTOR TO REMOVE EXISTING COPING SYSTEM AND DISPOSE OF.	10. CONTRACTOR TO REMOVE EXISTING EDGE METAL FLASHING AND
CONTRACTOR TO INSTALL NEW ENGINEERED (ES-1) COPING SYSTEM
SIMILAR TO DETAIL 14/A501. OWNER TO APPROVE COLOR.	11. CONTRACTOR TO REMOVE EXISTING FLASHINGS AND REINSTALL, PER 4.CONTRACTOR TO REMOVE AND STORE EXISTING COUNTER-FLASHING                     DETAIL 8/A500.
SYSTEMS FOR REINSTALLATION, CONTRACTOR TO PROVIDE NEW	12. ROOF AREA NOTE APART OF PROJECT.
NOTES	 COUNTER-FLASHING AT OWN EXPENSE IF DAMAGED. CONTRACTOR TO REINSTALL SIMILAR TO DETAIL 3/A500.
THE DIMENSIONS ON THE DRAWING DO NOT	5. CONTRACTOR TO INSTALL NEW CONTRACTOR TO REMOVE EXISTING
RESPONSIBLE FOR MEASURING EACH ROOF AREA.	FLASHING TO INSTALL NEW STEP- FLASHING, SIMILAR TO DETAIL 6/A500 CONTRACTOR TO REINSTALL COVER FLASHING OVER STEP-FLASHING.

			

			

		
	DESIGN CONSULTANT: TROY BROOKS
	
	DRAFTED BY: SG
	CHECKED BY: TT
	
	DATE: 3/9/23
	
	JOB NO: 108722001
	
	PROJECT NO:
	
	PHASE:
	
	0	1"
ORIGINAL SCALE SHOWN IS ONE INCH. ADJUST SCALE FOR REDUCED OR ENLARGED PLANS.
	
	SHEETA6-R
	
	8	OF	11

32'-8"±
10'-11"±
9'-10"±
3/9/2023 1:30 PM G:\Clovis USD-1087\108722001-Reroof of Cole Elementary\300 CAD\340 Sheet Sets\02_Roof Plan\A7-R CORRIDOR.dwg -Stephen Grisez
CORRIDOR
ARCHITECTURAL
615 W. STUART AVENUE
CLOVIS UNIFIED SCHOOL DISTRICT
COLE ELEMENTARY SCHOOL REROOF
WING 4
OWNER TO PICK OLOR.
REFLECT ROOF SLOPE. CONTRACTOR

		34'-2"±

							

						

SOUTH

			

WING 1 APPROXIMATE LOCATION

						
						
				81'-1"±

WING 2 APPROXIMATE LOCATION

WING 2                                                                                                                                                                                                            WING 3 APPROXIMATE LOCATION                                                                                                                                                                                                                                                                                                              64'-9"±                                                                           APPROXIMATE LOCATION

8'-5"±

APPROXIMATE LOCATION	KEY NOTES - CORRIDOR
1. REMOVE EXISTING BUILT-UP ROOFING SYSTEM AND ASSOCIATED FLASHINGS DOWN TO THE STRUCTURAL PLYWOOD DECK. CONTRACTOR TO INSPECT EXISTING DECK AND COMMUNICATE ANY DAMAGE TO OWNER'S REPRESENTATIVE. CONTRACTOR TO CONDUCT A FASTENER PULL OUT TEST PER MANUFACTURERS REQUIREMENTS. CONTRACTOR TO INSTALL NEW PVC ROOFING SYSTEM PER PROJECT SPECIFICATIONS AND MANUFACTURER REQUIREMENTS.
2.EXISTING PIPE PENETRATIONS. CONTRACTOR TO HIRE LICENSED ELECTRICIAN AS REQUIRED TO RAISE EXISTING ELECTRICAL CONDUIT. CONTRACTOR TO INSTALL NEW PIPE PENETRATION FLASHING PER DETAIL 16/A500 TYP.
3. CONTRACTOR TO REMOVE AND STORE EXISTING COUNTER-FLASHING SYSTEMS FOR REINSTALLATION, CONTRACTOR TO PROVIDE NEW COUNTER-FLASHING     AT     OWN     EXPENSE     IF     DAMAGED     DURING CONSTRUCTION. CONTRACTOR TO REINSTALL SIMILAR TO DETAIL 5/A500.
4.CONTRACTOR TO REMOVE AND DISPOSE OF EXISTING SUPPORTS. CONTRACTOR TO INSTALL NEW MIRO SUPPORTS PER PROJECT SPECIFICATIONS.
NOTES	5. CONTRACTOR TO REUSE EXISTING LOW-PROFILE RUBBER SUPPORTS.
6. CONTRACTOR TO REMOVE AND DISPOSE OF EXISTING EDGE METAL. THE DIMENSIONS ON THE DRAWING DO NOT	CONTRACTOR TO INSTALL NEW EDGE METAL PER MANUFACTURER'S
NORTH	9'-10"±	RESPONSIBLE FOR MEASURING EACH ROOF AREA.	REQUIREMENTS. CCONTRACTOR TO MATCH EXISTING EDGE PROFILE,

			

			

		
	DESIGN CONSULTANT: TROY BROOKS
	
	DRAFTED BY: SG
	CHECKED BY: TT
	
	DATE: 3/9/23
	
	JOB NO: 108722001
	
	PROJECT NO:
	
	PHASE:
	
	0	1"
ORIGINAL SCALE SHOWN IS ONE INCH. ADJUST SCALE FOR REDUCED OR ENLARGED PLANS.
	
	SHEETA7-R
	
	9	OF	11

MANUFACTURED REQUIREMENTS
NEW
SECURE CLEAT AT 8" O.C.
NEW STEP FLASHING TO BE
A500
3/9/2023 1:31 PM G:\Clovis USD-1087\108722001-Reroof of Cole Elementary\300 CAD\340 Sheet Sets\03_Details\A500 CONSTRUCTION DETAILS.dwg -Stephen Grisez
CONSTRUCTION DETAILS
ARCHITECTURAL
615 W. STUART AVENUE
CLOVIS UNIFIED SCHOOL DISTRICT
COLE ELEMENTARY SCHOOL REROOF

NEW 24 G.A. SHEET METAL FLASHING TO BE SECURED 12" O.C. WITH APPROVED RING SHANK NAILS, CONTRACTOR TO INSTALL A SELF ADHERING STRIP ACROSS TOP OF FLASHING
NEW SOLAR REFLECTIVE LAMINATED ASPHALT SHINGLES. SEE PROJECT SPECIFICATIONS AND MANUFACTURER, FOR SECUREMENT AND EXPOSURE REQUIREMENTS.

NEW SINGLE-PLY ROOFING SYSTEM OVER COVERBOARD. REFER TO PROJECT AND MANUFACTURERS SPECIFICATIONS

SECURE MEMBRANE FLASHING STRIP WITH TURN- BAR, SECURE PER MANUFACTURERS REQUIREMENTS, CONTRACTOR TO INSTALL A WATER-BLOCK OF BUTYL BEHIND MEMBRANE AT LOCATION OF TURN-BAR

NOT TO SCALE
1	TRANSITION BETWEEN LOW-SLOPE TO STEEP SLOPE

NEW 24 GAUGE STANDING SEAM CLEAT. VARIES	SEAM ON ONE SIDE WITH GROMMETED
FASTENERS 12" O.C. CONTRACTOR SHALL SECURE OTHER SIDE WITH CLEAT TO
INCORPORATED INTO	ALLOW FOR EXPANSION/CONTRACTION SHINGLE ROOF SYSTEM
SELF-ADHERING BASE SHINGLE & FELT	SHEET 12" ON DECK MIN ROOF SYSTEM                                                                            PRESSURE
TREATED 2X4 NAILERS

SIMPSON CLIPS
1'-0"	AT 3" O.C.	1'-0"

EXTERIOR DECKING

INCHES

3" = 1'-0"
2
A500	EXPANSION JOINT
	
EXISTING PLASTER.

EXISTING COUNTER FLASHING.

SECURE TO WALLS WITH APPROVED FASTENERS. SEAL TOP EDGE WITH SELF-ADHERING MEMBRANE.

EXISTING COUNTER FLASHING, CONTRACTOR TO REMOVE AND STORE FOR REINSTALLATION FOLLOWING THE INSTALLATION OF THE NEW ROOFING SYSTEM.

EXISTING 1X FURRING.

NEW SINGLE-PLY ROOFING SYSTEM OVER COVERBOARD, REFER TO PROJECT AND MANUFACTURERS SPECIFICATIONS.

INCHES

3" = 1'-0" 3
A500	FLASHING DETAIL

ROOF VENTILATOR

G.I. FLASHING, TO BE REMOVED AND REINSTALLED IN WATER-TIGHT CONDITION CAULK AS REQD.

8d NAILS 12" OC	G.I. FLASHING, TO
MASTIC	BE REMOVED AND REINSTALLED
EXISTING 2" x BLOCKING

INCHES

1-1/2" = 1'-0"
4
A500	RIDGE VENT DETAIL
	
NOTES
NEW WALL FLASHING ADHERED PER	1.	HOT AIR WELD LAPS MIN. OF 1 1/2". 2.	CONTRACTOR TO THOROUGHLY
CLEAN SUBSTRATE BEFORE NEW 24 GA. GI. SHEET METAL	INSTALLING FLASHING. FLASHING WITH 1/2" HEM,
SECURE GROMMETED FASTENERS EVERY 12" OC.

SECURE TO CURB WITH TURN BAR. ATTACH EVERY 12" O.C. W/ GALV. SCREWS

NEW PVC 60 MIL. MEMBRANE ROOF. SEE SPECS.

1/4" HIGH DENSITY BOARD. REFER TO PROJECT AND MANUFACTURERS SPEC

NOT TO SCALE
5
A500	MECH. EQUIPMENT OR SIMILAR
	NOTE	

1.        CONTRACTOR TO INSTALL NEW CAST IRON STRAINERS IF DAMAGED OR MISSING.

(E) CAST IRON ROOF DRAIN. INSTALL NEW	NEW SINGLE-PLY ROOFING SYSTEM OVER STAINLESS STEEL BOLTS AND WASHERS,	COVERBOARD, REFER TO PROJECT AND CONTRACTOR TO INSTALL WATER-BLOCK	MANUFACTURERS SPECIFICATIONS. SEALANT PER MANUFACTURER
REQUIREMENTS	FILL TOP w/ APPROVED SEALANT NEW STAINLESS STEEL DRAWBAND

INSTALL ALUMINUM TAPE AROUND PIPE
IF PIPE HAS EXISTING 2" MIN	ROOF MATERIAL

FEET

0		1 1" = 1'-0"
6
A500	ROOF DRAIN AND OVERFLOW
	CONTRACTOR TO APPLY NOTE	                                           APPROVED SEALANT
CONTRACTOR TO CLEAN ANY FOREIGN MATERIAL	ROOFING UNDERLAYMENT FROM THE EXISTING PIPE, PRIOR TO THE INSULATION	OVER PLYWOOD
OF THE NEW PIPE FLASHING.	SUBSTRATE TO BE LAID SO AS TO SPILL OVER TOP OF ANTI-CAPILLARY HEM.
STACK/VENT PIPE WITH VENTING CAP	FLASHING TO BE FIXED UNDER CARRIED THROUGH SHINGLES AND                                                                                        THE ASPHALT SHINGLES. FOLD SUBSTRATE. FIELD VERIFY SIZING.                                                                                         TOP EDGE TO FORM
ANTI-CAPILLARY HEM .

FLASHING AROUND PIPE PENETRATION.

FLASHING TO BE LAID SO
AS TO DISCHARGE WATER	CONTINUOUS BEAD OVER LOWER SHINGLES.	ROOF CEMENT ON
FLASHING AND
CONCEALED HALF DRESS LOWER EDGE OF FLASHING OVER	OF SHINGLE. SHINGLES AND SECURE WITH ROOF CEMENT'
AS PER MANUFACTURERS SPECS.	FOLD EDGES OF THE BOOT FLASHING BACK ONTO ITSELF TO CREATE A
SECONDARY WATER BARRIER. APPLY SEALANT, BEHIND
FLASHINGS, SECURE WITH
STAINLESS STEEL DRAWBAND.	INTEGRATED FLASHING BOOT.

NOT TO SCALE
7
A500	PIPE PENETRATION FLASHING - STEEP SLOPE

						

STEP FLASHING OR UPSTAND FLASHINGS INSTALLED AS PER MANUFACTURERS SPECS WITH SHINGLES LAID
EQUIPMENT CURB OR	OVER. SPECIFIC PENETRATING
ROOF.
PROVIDE 8" UPSTAND TO APRON FLASHING 6"MIN	FIX FLASHINGS.
UP TO CURB AND
DRESSED OUT OVER	PROVIDE MIN 6" OVERLAP. SHINGLES.
NEW SOLAR REFLECTIVE APRON	LAMINATED ASPHALT FLASHING TO                                                                                                                                    SHINGLES. SEE PROJECT DISCHARGE                                                                                                                                      SPECIFICATIONS AND
TO ROOF.	MANUFACTURER, FOR SECUREMENT AND EXPOSURE REQUIREMENTS.

NOTE	

CONTRACTOR TO INSTALL CRICKETED APRON AT TOP OF ANY CURB LARGER THAN 36" WIDE

NOT TO SCALE
8
A500	CURB DETAIL

CONTRACTOR TO INSTALL NEW HEAT STACK PER MANUFACTURERS REQUIREMENTS

FEET

0		1 1" = 1'-0"
9
A500	HEAT STACK

NEW 24 GA. GI SCUPPER. CAULK TO PROVIDE WATERTIGHT CONDITION.

NEW SINGLE-PLY ROOFING SYSTEM OVER COVERBOARD, REFER TO PROJECT AND MANUFACTURERS SPECIFICATIONS.

NEW 24 GA. CLAD METAL FLASHING (E) CONDUCTOR
AND DOWNSPOUT.

INCHES

1-1/2" = 1'-0"
10
A500	ROOF SCUPPER AND CONDUCTOR HEAD

NEW SOLAR REFLECTIVE LAMINATED ASPHALT SHINGLES. SEE PROJECT SPECIFICATIONS AND MANUFACTURER, FOR SECUREMENT AND EXPOSURE REQUIREMENTS.

NEW ROOFING UNDERLAYMENT OVER SUBSTRATE TO BE LAID SO AS TO EXTEND OVER DRIP EDGE. SECURE PER PROJECT SPECIFICATIONS.

NEW DRIP EDGE TO MATCH EXISTING PROFILE, SECURE WITH ROOFING NAILS 4" OC STAGGERED, CONTRACTOR TO SUBMIT COLOR FROM APPROVAL.

SHINGLES TO HAVE MIN 1/4" OVERHANG.

EXISTING FASCIA BOARD.

NOT TO SCALE
11
A500	EDGE METAL FLASHING

						

						
					
				DESIGN CONSULTANT: TROY BROOKS
	
				DRAFTED BY: SG
	CHECKED BY: TT
	
				DATE: 3/9/23
	
				JOB NO: 108722001
	
				PROJECT NO:
	
				PHASE:
	
				0	1"
ORIGINAL SCALE SHOWN IS ONE INCH. ADJUST SCALE FOR REDUCED OR ENLARGED PLANS.
	
				SHEETA500
	
				10	OF	11

8" MIN
EXISTING STRUCTURAL
FRAMING
MANUFACTURERS
SUBSTRATE. SECURE
6"
8"
SEE SPEC
8" MIN
ETAILS.dwg -Stephen Grisez
NSTRUCTION DETAILS
ARCHITECTURAL
615 W. STUART AVENUE
VIS UNIFIED SCHOOL DISTRICT
EMENTARY SCHOOL REROOF

							

BATT INSULATION
		
WOOD NAILER (SEE NOTE)

STEP FLASHINGS NEW ROOFING	INSTALLED AS PER
UNDERLAYMENT OVER	SPECS WITH SHINGLES PER PROJECT	LAID OVER EACH STEP. SPECIFICATIONS.	STEP FLASHINGS MUST
OVERLAP TO PROVIDE COMPLETE COVERAGE.

NEW SOLAR REFLECTIVE LAMINATED ASPHALT SHINGLES. SEE PROJECT SPECIFICATIONS AND MANUFACTURER, FOR SECUREMENT AND EXPOSURE REQUIREMENTS.

NOT TO SCALE
12
A501	STEP FLASHING - STEEP SLOPE
	
NEW FACTORY-MADE EXPANSION JOINT COVER. SEE SPECS.

INCHES

3" = 1'-0"
13
A501	SEISMIC JOINT AT PARAPET WALLS
	
NEW ES-1 OR MANUFACTURER'S REMOVE (E) STUCCO AS	PREFERRED STANDING SEAM REQ'D TO REMOVE (E)	COPING SYSTEM PER MTR. COPING RETURN.	REQUIREMENTS. SEE SPEC REPAIR STUCCO FINISH
TO MATCH EXISTING AND PAINT TO MATCH. INSTALL NEW
REMOVABLE	2"	3.5" SURFACE-MOUNTED
COUNTER FLASHING PAINT TO MATCH
NEW SINGLE-PLY FLASHING STRIP. REFER TO PROJECT AND MANUFACTURER'S SPECIFICATIONS

NEW SINGLE-PLY ROOFING SYSTEM OVER COVERBOARD. REFER TO PROJECT AND
1/4" COVER BOARD,	MANUFACTURER'S OR APPROVED EQUAL	SPECIFICATIONS

INCHES	 EXISTING BATT.	EXISTING 1/2" STRUCTURAL INSULATION	PLYWOOD DECK

3" = 1'-0"
14
A501	COPING

INSTALL MIN. OF 3 LAYERS OF LIQUID FLASHING. CONTRACTOR TO EXTEND MIN. OF 2" BEYOND FABRIC.

NEW FABRIC TO EXTEND MIN. 6" UP THE PIPE LAP MIN. 3" ON BASE FABRIC.

NEW FABRIC TO BE INSTALLED MIN. 3" AT BASE OF PIPE AND ON CAP SHEET.

CORRUGATED DECK

NOT TO SCALE
15
A501	PIPE PENETRATION FLASHING

NOTES

1.	HOT AIR WELD LAPS MIN. OF 1 1/2"

2.	CONTRACTOR TO THOROUGHLY CLEAN SUBSTRATE BEFORE INSTALLING FLASHING.

NEW STAINLESS STEEL
DRAW BAND	NEW SEALANT PER MANUFACTURERS
REQUIREMENTS

NEW FLASHING BOOT

NEW PVC 60 MIL. NEW FASTENERS AROUND	MEMBRANE ROOF. PENETRATIONS PER
MANUFACTURER REQUIREMENTS

NOT TO SCALE
16
A501	PIPE PENETRATION - SINGLE PLY FLASHING

CONTRACTOR TO REMOVE AND INSTALL NEW COPING. CONTRACTOR TO MATCH EXISTING.

INCHES

1-1/2" = 1'-0"
17
A501	SHEET METAL CAP

NEW PREFINISHED 24 GA. G.I SHT MTL. GUTTER SYSTEM, CONTRACTOR TO REFER TO SMACMA AND PROJECT SPECIFICATION TO ATTACHMENT. OWNER TO APPROVE COLOR.

6"

20" GA DOWNSPOUT THROAT W/ 1/4" FLANGES. CONT. SOLDER

NOT TO SCALE
18
A501	EDGE METAL WITH GUTTER FLASHING

BOTTOM FLAP OF JOINT	ROOF EXPANSION HOT AIR WELDED AND	JOINT, SEE PROJECT MECHANICALLY FASTENED	SPECIFICATIONS FOR
APPROVED MATERIALS TOP FLAP OF JOINT HOT AIR
WELDED TO MEMBRANE	TERM BAR & FASTENER
(N) 1/4" COVERBOARD	(E) 1/2" STRUCTURAL OVER PLYWOOD	PLYWOOD DECK

NOT TO SCALE
19
A501	EXPANSION JOINT - LOW SINGLE-PLY

						

COLE EL

CLO

CO 3/9/2023 1:52 PM G:\Clovis USD-1087\108722001-Reroof of Cole Elementary\300 CAD\340 Sheet Sets\03_Details\A501 CONSTRUCTION D

						

						
					
				DESIGN CONSULTANT: TROY BROOKS
	
				DRAFTED BY: SG
	CHECKED BY: TT
	
				DATE: 3/9/23
	
				JOB NO: 108722001
	
				PROJECT NO:
	
				PHASE:
	
				0	1"
ORIGINAL SCALE SHOWN IS ONE INCH. ADJUST SCALE FOR REDUCED OR ENLARGED PLANS.
	
				SHEETA501
	
				11	OF	11