Addendum No. 02 May 12, 2023

Campus Security Improvement Phase 1

OWNER:

PREPARED BY:

PBK PROJECT NO.: DSA FILE NO.:
DSA APPLICATION NO.:

Clovis Unified School District

1450 Herndon Ave. Clovis, CA. 93611

PBK Architects, Inc. 7790 N. Palm Avenue Fresno, California 93711

S2100500AR N/A
N/A

NOTICE TO BIDDERS

A. Receipt of this Addendum shall be acknowledged on the Proposal Form.
B. This Addendum forms part of the Contract Documents for the above referenced project and shall be incorporated integrally therewith.
C. Each proposer shall make necessary adjustments and submit their proposal with full knowledge of all modifications, clarifications, and supplemental data included therein. Where provisions of the following supplemental data differ from those of the original Contract Documents, this Addendum shall govern.

DRAWINGS:

CLOVIS HIGH SCHOOL:

2-01	 Sheet A1.0 – SITE PLAN, revise as follows: Add Sheet A1.0. See attached.

2-02	Sheet A4.0 – CLASSROM WING (BUILDING C), revise as follows: Revise Keynote 3 to Keynote 4. See attached.

2-03	 Sheet A5.0 – CLASSROOM WING (BUILDING D), revise as follows: AC symbol add note. ”AC IN ATTIC SPACE”. See attached.

2-04	 Sheet A5.1 – REFLECTED CEILING PLAN (BUILDING D), revise as follows: AC symbol add note. “AC IN ATTIC SPACE”. See attached.

2-05	 Sheet A10.0 – LIBRARY WING (BUILDING B), revise as follows: AC symbol add note. “AC IN ATTIC SPACE”. See attached.

2-06	 Sheet A10.1 – REFLECTED CEILING PLAN (BUILDING B), revise as follows: AC symbol add note. “AC IN ATTIC SPACE”. See attached.

1

Addendum No. 02 May 12, 2023

Campus Security Improvement Phase 1

2-07	Sheet D1.1 – REVISED DETAIL 12, revise as follows: Revised note see attached.

BUD RANK ELEMENTARY:

2-08	Sheet D1.1 – REVISED DETAIL 12, revise as follows: Revised note see attached.

FT. WASHINGTON ELEMENTARY:

2-09	Sheet A5.2 – REFLECTED CEILING PLAN (BUILDING D), revise as follows: Revise sheet number from A5.2 to A5.1.

2-10	Sheet D1.1 – REVISED DETAIL 12, revise as follows: Revised note see attached.

SPECIFICATION SECTIONS:

2-11	Specification Sections - Remove specifications from Book, revise as follows:

Remove sections from book. 03 30 00 Cast-in-place Concrete, 05 50 00 Metal Fabrications, 09 24 00 Cement Plastering, 09 29 00 Gypsum Board, 09 51 13 Acoustical Panel Ceiling, 08 41 13 Aluminum-Framed Entrance and Storefront.

2-12	 Remove Specification Section 01 10 00 Summary, revise as follows: Add specification 01 10 00 Summary. See attached.

END OF ADDENDUM NO. 2

John Hamilton Smith

__________________________________ NAME OF ARCHITECT, Architect

2

RM J
DATE
CHECKED BY
DRAWN BY
03.01.2023
PROJECT ARCHITECT
JOHN SMITH
PROJECT NUMBER
S2100500AR
.	.
.
.

			
BOYS

LOCKER

		

	
 G

		IRLS OCKER

	L

			

		
	
DIN
	
2BUIL

				

 

					
					
UILDIN
	G E1	

LEGEND

P.A. SPEAKER ALGO 8186 HORN
CONNECT WIRE TO TERMINAL CABINET SPEAKER

NORTH GYM BUILDING N

SOUTH GYM BUILDING S
B

BUILDING C	E	G 5

PORTABLES

LMC BUILDING B

BOILER	PORTABLES ADMIN	SNCK
BUILDING A	BAR

BUILDING H2

MPR BUILDING D	BUILDING F

BUILDING H3
		
CLOVIS HIGH SCHOOL
	
		REVISIONS

No.	DATE	DESCRIPTION
	2	.	ADDENDUM 02
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.

														

		
L

																		

																																																							
																																																						
																															BUILDING 1
				BUILDING 3	BUILDING 2

																																																						

																																																									

																																																												

																																																								

																																																								

																																																							

																																																							

																																																			

																																																									

																																																							

																																																					

																																																				

																																																				

																																																			

																																							

																																																																																	

																																																																															

																																																																																												

																																																																																																		

																																																																																																																

																																																																																																									

																													BUILDING K

BUILDING H1
	BUILDING H1

																																																																																																						

																																																																																																												

																																																																																													

																																																																																													

																																																																																																			

																																																																																													

																																																																																																										

																																																																																																							

																																																																																																				

																																																																																																

																																																																																															

																																																																																							

																																																																																							

																																																																																													

																																																																																													

																																																																																										

																																																																																														

																																																																																											

																																																																																											

																																																																																												

																																																																																											

																																																																																				

																																																																															

																																																																																

																																																																																																																	

C 15885
9-30-23 RENEWAL DATE
	
SITE PLAN

																																																																																																																		

																																																																																																																										

																																																																																																																												

																																																																																																																									

																																																																																																																		

																																																																																																																						

																																																																																																																												

																																																																																																																												

																																																																																																																							

																																																																																																																												
																																																																																																																												
																																																																																																	BUILDING T

																																																																																																																					

		SITE PLAN	.	N CLOVIS HIGH SCHOOL                                                                                                                    SCALE: 1/8"=1'-0"

2-01

A1.0	2

.	.

N
1

L

C 15885
9-30-23 RENEWAL DATE
	
CLASSROOM WING (BUILDING C)

	
A4.0

L
	OC
	K

4	AC
EXTERIOR DOOR # C1, C2, C3, C4, C5
2	AT DOOR FRAME
REX C3 DC CR DC

3	3

INTERIOR DOOR # C1, C2, C3, C4, C5

REX                                              REX                                                                                                              REX                                             REX C4                                                C5                                                                                                                C1                                                C2
DC DC	DC DC	DC DC	DC DC
AT DOOR FRAME CR	CR AT DOOR FRAME	CR AT DOOR FRAME	CR AT DOOR FRAME

1	1	1	1

SECOND FLOOR PLAN	FIRST FLOOR PLAN

CLASSROOM WING (BUILDING C)	. CLOVIS HIGH SCHOOL                                                                                                             SCALE: 1/8"=1'-0"
	
CLOVIS HIGH SCHOOL
	
	REVISIONS

No.	DATE	DESCRIPTION
	2	.	ADDENDUM 02
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.

BUILDING C : CLASSROOM	ABBREVIATIONS	KEYNOTES

DOOR	FRAME	WALL	CEILING
FF      FACTORY FINISH

FT      FACTORY

HM     HOLLOW METAL

PT      PAINT

GYP     GYP. BOARD FINISH

PH      PANIC HARDWARE

WC      WOOD CONSTRUCTION	CC      CONC. CONSTRUCTION

SI	SINGLE DOOR

DL      DOUBLE DOOR

FRP     FIBER RESISTANT PANEL

STU     STUCCO FINISH
TB.     T-BAR CEILING SYSTEM

1.      UNMANNED DOOR, PROVIDE CARD READER

2.     CAMPUS LOCKDOWN BUTTON. REFER TO SPECIFICATIONS FOR DETAILS 3.     EXISTING RATED WALL
4.     EXISTING ELECTRICAL PANEL LOCATION. CONTRACTOR TO INSTALL (2) NEW 120V, 20A CIRCUITS FROM PANEL TO NEW ACCESS CONTROL PANEL AND NEW DOOR HARDWARE POWER SUPPLY ENCLOSURE. INSTALL NEW 20A, CIRCUIT BREAKER IN EXISTING PANEL.

03.01.2023
PROJECT NUMBER
S2100500AR
DOOR No.
DOOR TYPE
DOOR SIZE
EXISTING CONST.
EXISTING CONST.
EXISTING FINISH
EXISTING FINISH
GENERAL NOTES
HARDWARE
(SEE SPECS)
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING WALL CONST.
DETAIL SHEET D1.1
W. x H.	SF      STOREFRONT	TK      TACKBOARD FINISH

SGP     SEMI-GLOSS PAINT	WIN     WINDOW SYSTEM DOOR SCHEDULE X

DATE
GENERAL NOTES

C1      DL	3'-0" x 7'-0"

C2	SI	3'-0" x 7'-0"

C3	SI	3'-0" x 7'-0"

C4	SI	3'-0" x 7'-0"

C5	SI	3'-0" x 7'-0"

HM	PT	HM	PT

HM	PT	HM	PT

HM	PT	HM	PT

HM	PT	HM	PT

HM	PT	HM	PT

CC	CC	STU	CC	TB	10	2	6

CC	CC	STU	CC	TB	10	2	6

CC	CC	STU	CC	TB	10	2	6

CC	CC	STU	CC	TB	10	2	6

CC	CC	STU	CC	TB	10	2	6

LEGEND

AC
NEW ACCESS CONTROL PANEL / DOOR CONTROLLER PANEL TO BE INSTALLED AT THIS LOCATION FOR THIS BUILDING. INSTALL NEW DEDICATED POWER RECEPTACLE INSIDE PANEL. ALL CARD READERS AND DOOR ACCESSORIES TO BE ROUTED BACK TO THIS PANEL FOR TERMINATION.

CAMPUS LOCKDOWN BUTTON WALL MOUNTED

DC
DOOR CONTACT FOR EACH DOOR LEAF. DOUBLE DOORS WILL NEED A "REX" LOCATED INSIDE THE BUILDING ABOVE THE DOORS.

CR CARD READER / ACCESS DEVICE

P.A. SPEAKER ALGO 8186 HORN

NEW 24"x24" ACCESS PANEL DETAIL 15/D1.1

INSTALL NEW CAT6A DATA CABLE IN NEW ACCESS CONTROL PANEL FOR NETWORK CONNECTIVITY. TERMINATE OUTLET ON BISCUIT JACK INSIDE PANEL AND CONNECT WIRING BACK TO NEAREST MDF/IDF RACK AND TERMINATE ON EXISTING PATCH PANEL IN RACK.

REX REQUEST TO EXIT MODULE INSTALLED ABOVE DOOR AND CONNECTED BACK TO DOOR CONTROLLER

EXISTING RATED WALL

EXISTING CMU / CONCRETE WALLS

EXISTING WOOD / METAL WALLS

1. DEMO FINISHES TO ACCESS WORK. REPAIR ALL FINISHES BACK TO ORIGINAL FINISH/CONDITION.

2. SEE SPECIFICATIONS FOR MORE INFORMATION.

3. EXISTING EXTERIOR WALL CONDITION IS CONCRETE / CMU SYSTEM U.O.N.. 4. SEE DTL. 12/D1.1 FOR ACCESS CONTROL SYSTEM DETAILS.
5. ALL INTERIOR WIREMOLD FROM CEILING TO DOOR WILL BE SURFACE MOUNTED U.N.O..

6. CONNECT DOOR CONTROLLER TO NEAREST OUTLET PREFERRED OR HARDWIRE THE NEXT OPTION. 7. USE WIREMOLD 2000 SERIES AND ACCESSORIES OR EQUAL.
8. ONE LINE DOOR LEAF ON A PAIR OF DOORS SHALL HAVE ELECTRIFIED HARDWARE. REMAINING "DEAD" WILL REMAIN EXIT ONLY AND EXTERIOR HARDWARE PULL WILL BE REMOVED FROM "DEAD" DOOR AND HOLES REPAIRED.

9. DOUBLE DOORS SHALL RECIEVE A REQUEST TO EXIT (REX) DEVICE MOUNTED AT CEILING OR WALL ABOVE DOORS. SINGLE DOORS WILL HAVE REX INSIDE DOOR PANIC HARDWARE.

CHECKED BY
DRAWN BY
PROJECT ARCHITECT
JOHN SMITH
.
.
2-02

03.01.2023
PROJECT NUMBER
S2100500AR
.	.
DOOR No.
DOOR TYPE
DOOR SIZE
EXISTING CONST.
EXISTING CONST.
EXISTING FINISH
EXISTING FINISH
GENERAL NOTES
HARDWARE
(SEE SPECS)
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING EXT. FINISH
EXISTING INT. FINISH
EXISTING WALL CONST.
DETAIL SHEET D1.1
NEW 24"x24" ACCESS PANEL
TERMINATION.
DOUBLE DOORS WILL NEED A "REX"
DC

N
1
CR
DC

L

C 15885
9-30-23 RENEWAL DATE
	
CLASSROOM WING (BUILDING D)

	
A5.0

L
	OC
	K

1	1	1	1

CR AT DOOR FRAME	CR AT DOOR FRAME	CR AT DOOR FRAME	CR AT DOOR FRAME	EXTERIOR DOOR # D1, D2, D3 D4, D5 DC DC                                         DC DC                                                                                                        DC DC                                         DC DC
D5                                                D4                                                                                                              D2                                                D1 REX                                              REX                                                                                                            REX                                              REX

2
AC       AC IN ATTIC SPACE 3	3

INTERIOR DOOR # D1, D2, D3 D4, D5
REX D3 DC
AT DOOR FRAME

4

SECOND FLOOR PLAN	FIRST FLOOR PLAN

CLASSROOM WING (BUILDING D)	. CLOVIS HIGH SCHOOL                                                                                                             SCALE: 1/8"=1'-0"
	
CLOVIS HIGH SCHOOL
	
	REVISIONS

No.	DATE	DESCRIPTION
	2	.	ADDENDUM 02
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.

BUILDING D : CLASSROOM	ABBREVIATIONS	KEYNOTES

DOOR	FRAME	WALL	CEILING
FF      FACTORY FINISH

FT      FACTORY

HM     HOLLOW METAL

PT      PAINT

GYP     GYP. BOARD FINISH

PH      PANIC HARDWARE

WC      WOOD CONSTRUCTION	CC      CONC. CONSTRUCTION

SI	SINGLE DOOR

DL      DOUBLE DOOR

FRP     FIBER RESISTANT PANEL

STU     STUCCO FINISH
TB.     T-BAR CEILING SYSTEM

1.      UNMANNED DOOR, PROVIDE CARD READER

2.     CAMPUS LOCKDOWN BUTTON. REFER TO SPECIFICATIONS FOR DETAILS 3.     EXISTING RATED WALL. TYP.

4.     EXISTING ELECTRICAL PANEL LOCATION. CONTRACTOR TO INSTALL (2) NEW 120V, 20A CIRCUITS FROM PANEL TO NEW ACCESS CONTROL PANEL AND NEW DOOR HARDWARE POWER SUPPLY ENCLOSURE. INSTALL NEW 20A, CIRCUIT BREAKER IN EXISTING PANEL.

W. x H.

DOOR SCHEDULE X

D1	SI	3'-0" x 7'-0"	HM	PT	HM	PT

D2	SI	3'-0" x 7'-0"	HM	PT	HM	PT

D3      SI	3'-0" x 7'-0"	HM	PT	HM	PT

D4	SI	3'-0" x 7'-0"	HM	PT	HM	PT

D5      SI	3'-0" x 7'-0"	HM	PT	HM	PT

CC	CC	STU	CC	TB	10	2	8

CC	CC	STU	CC	TB	10	2	8

CC	CC	STU	CC	TB	10	2	8

CC	CC	STU	CC	TB	10	2	8

CC	CC	STU	CC	TB	10	2	8

SF      STOREFRONT                                                  TK      TACKBOARD FINISH SGP     SEMI-GLOSS PAINT                                      WIN     WINDOW SYSTEM

LEGEND

AC
NEW ACCESS CONTROL PANEL / DOOR	CR CARD READER / ACCESS DEVICE CONTROLLER PANEL TO BE INSTALLED AT

P.A. SPEAKER ALGO 8186 HORN
THIS LOCATION FOR THIS BUILDING. INSTALL NEW DEDICATED POWER RECEPTACLE INSIDE PANEL. ALL CARD READERS AND DOOR ACCESSORIES TO
BE ROUTED BACK TO THIS PANEL FOR	DETAIL 15/D1.1

CAMPUS LOCKDOWN
BUTTON WALL MOUNTED
DOOR CONTACT FOR EACH DOOR LEAF.
INSTALL NEW CAT6A DATA CABLE IN NEW ACCESS CONTROL PANEL FOR NETWORK CONNECTIVITY. TERMINATE OUTLET ON BISCUIT JACK INSIDE PANEL AND CONNECT WIRING BACK TO NEAREST MDF/IDF RACK
RACK.
LOCATED INSIDE THE BUILDING ABOVE	AND TERMINATE ON EXISTING PATCH PANEL IN THE DOORS.

REX REQUEST TO EXIT MODULE INSTALLED ABOVE DOOR AND CONNECTED BACK TO DOOR CONTROLLER

EXISTING RATED WALL

EXISTING CMU / CONCRETE WALLS

EXISTING WOOD / METAL WALLS

GENERAL NOTES

1. DEMO FINISHES TO ACCESS WORK. REPAIR ALL FINISHES BACK TO ORIGINAL FINISH/CONDITION.

2. SEE SPECIFICATIONS FOR MORE INFORMATION.

3. EXISTING EXTERIOR WALL CONDITION IS CONCRETE / CMU SYSTEM U.O.N..

4. SEE DTL. 12/D1.1 FOR ACCESS CONTROL SYSTEM DETAILS.

5. ALL INTERIOR WIREMOLD FROM CEILING TO DOOR WILL BE SURFACE MOUNTED U.N.O..

6. CONNECT DOOR CONTROLLER TO NEAREST OUTLET PREFERRED OR HARDWIRE THE NEXT OPTION. 7. USE WIREMOLD 2000 SERIES AND ACCESSORIES OR EQUAL.
8. ONE LINE DOOR LEAF ON A PAIR OF DOORS SHALL HAVE ELECTRIFIED HARDWARE. REMAINING "DEAD" WILL REMAIN EXIT ONLY AND EXTERIOR HARDWARE PULL WILL BE REMOVED FROM "DEAD" DOOR AND HOLES REPAIRED.

9. DOUBLE DOORS SHALL RECIEVE A REQUEST TO EXIT (REX) DEVICE MOUNTED AT CEILING OR WALL ABOVE DOORS. SINGLE DOORS WILL HAVE REX INSIDE DOOR PANIC HARDWARE.

DATE
CHECKED BY
DRAWN BY
PROJECT ARCHITECT
JOHN SMITH
.
.
2-03

3
3
2

CLASSROOM WING (BUILDING D) CLOVIS HIGH SCHOOL

N .

SCALE: 1/8"=1'-0"

DATE
CHECKED BY
DRAWN BY
03.01.2023
PROJECT ARCHITECT
JOHN SMITH
PROJECT NUMBER
S2100500AR
.	.
.
.
EXISTING RATED WALL
AC
CR
P.A. SPEAKER ALGO 8186 HORN

L

C 15885
9-30-23 RENEWAL DATE
	
REFLECTED CEILING PLAN (BUILDING D)

	
A5.1

CR

KEYNOTES
	
LEGEND

1.      DOOR TO RECEIVE NEW HARDWARE AND CONNECT TO NEW CARD READER.
2.     INSTALL NEW BUILDING ACCESS CONTROL SYSTEM INTEGRATED WITH AUTOMATIC CAMPUS LOCKDOWN INTERFACE
3.     EXISTING RATED WALL
		
NEW ACCESS CONTROL PANEL / DOOR	EXISTING RATED WALL CONTROLLER PANEL TO BE INSTALLED AT
THIS LOCATION FOR THIS BUILDING. INSTALL NEW DEDICATED POWER RECEPTACLE INSIDE PANEL. ALL CARD
READERS AND DOOR ACCESSORIES TO	CARD READER / ACCESS DEVICE BE ROUTED BACK TO THIS PANEL FOR
TERMINATION.	DNA DOES NOT APPLY
LOW VOLTAGE PATHWAY	 INSTALL NEW CAT6A DATA CABLE IN NEW ACCESS CONTROL PANEL FOR
NEW 24"x24" ACCESS PANEL                                                           NETWORK CONNECTIVITY. TERMINATE DETAIL 15/D1.1                                                                                    OUTLET ON BISCUIT JACK INSIDE PANEL
AND CONNECT WIRING BACK TO NEAREST MDF/IDF RACK AND TERMINATE ON EXISTING PATCH PANEL IN RACK.

NOTES
			
1.      PATHWAY IS DIAGRAMATIC IN NATURE BUT SHOWN IN AREAS THAT APPEAR TO BE BEST AVVESSED ABOVE T-BAR SYSTEM. CONTRACTOR MAY PROPOSE A DIFFERENT PATHWAY BUT MUST BE APPROVED BY DISTRICT BEFORE WORK STARTS.
2.     SEE DTL. 12/D1.1 FOR ACCESS CONTROL SYSTEM DETAILS.
3.     ALL INTERIOR WIREMOLD FROM CEILING TO DOOR WILL BE SURFACE MOUNTED U.N.O..

1
1	1	1

CR AT DOOR FRAME	AT DOOR FRAME	CR AT DOOR FRAME	CR AT DOOR FRAME

D5	D4	D2	D1

11
D1.1 TYP.

TYP.	AC AC IN ATTIC SPACE

2

1 D3
CR
AT DOOR FRAME
11                                                                                                                                                                                                                                                                                                                                                                                                                 11 D1.1                                                                                                                                                                                                                                                                                                                                                                                                               D1.1

DOWN TO CLOSET BELOW

CONNECT WIRE TO TERMINAL CABINET SPEAKER

SECOND FLOOR PLAN	FIRST FLOOR PLAN
	
CLOVIS HIGH SCHOOL
	
	REVISIONS

No.	DATE	DESCRIPTION
	2	.	ADDENDUM 02
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.

2-04

DATE
CHECKED BY
DRAWN BY
03.01.2023
PROJECT ARCHITECT
JOHN SMITH
PROJECT NUMBER
S2100500AR
.	.
.
.
DOOR SIZE
.
CR
AC
EXISTING RATED WALL
AC
P.A. SPEAKER ALGO 8186 HORN
NEW 24"x24" ACCESS PANEL
MDF/IDF RACK AND TERMINATE ON
TERMINATION.
BUTTON WALL MOUNTED
DOOR CONTACT FOR EACH DOOR LEAF.
DOUBLE DOORS WILL NEED A "REX"
DC
REX
CONTROLLER
DC

L

C 15885
9-30-23 RENEWAL DATE
	
LIBRARY WING (BUILDING B)

	
A10.0

L
	OC
	K

EXTERIOR DOOR # B1

3

AT DOOR FRAME CR
1	DC B1 REX 1
AT DOOR FRAME
INTERIOR DOOR # B1	DC DC	2 B6                                           AC IN ATTIC SPACE
REX

EXTERIOR DOOR # B6

INTERIOR DOOR # B6
	BUILDING B : LIBRARY
	
CLOVIS HIGH SCHOOL
	
	DOOR No.
	DOOR TYPE

W. x H.
	DOOR
	FRAME
	WALL
	CEILING
					
				EXISTING CONST.
	
EXISTING FINISH
	
EXISTING CONST.
	
EXISTING FINISH
	
EXISTING WALL CONST.
	
EXISTING EXT. FINISH
	
EXISTING INT. FINISH
	
EXISTING EXT. FINISH
	
EXISTING INT. FINISH
	HARDWARE (SEE SPECS)
	GENERAL NOTES
	
DETAIL SHEET D1.1
		
	DOOR SCHEDULE X

B1
	
DL
	
(E) 3'-0" x 7'-0"
	
HM
	
PT
	
HM
	
PT
	
WIN
	
WIN
	
WIN
	
STU
	
GYP
	
9
	
2
	
8
		
	-
	-
	-
	-
	-
	-
	-
	-
	-
-
	-
-
	-
	-
	-
	-
	-

-
	
-
	
-
	
-
	
-
	
-
	
-
	
-
	-
-
	-
-
	
-
	
-
	
-
	-
	-
		
	-
	-
	
-
	-
	-
	-
	-
	-
	-
-
	-
-
	
-
	
-
	
-
	
-
	
-

-
	
-
	
-
	-
	-
	-
	-
	
-
	-
-
	-
-
	
-
	
-
	
-
	
-
	
-

B6
	
DL
	
(E) 3'-0" x 7'-0"
	
HM
	
PT
	
HM
	
PT
	
CC
	CC
WIN
	CC
WIN
	
STU
	
TB
	
9
	
2
	
8
		
	ABBREVIATIONS

FF      FACTORY FINISH	WC      WOOD CONSTRUCTION FT      FACTORY                                                        SI	SINGLE DOOR
HM     HOLLOW METAL	DL      DOUBLE DOOR
PT      PAINT	FRP     FIBER RESISTANT PANEL GYP     GYP. BOARD FINISH	STU     STUCCO FINISH
PH      PANIC HARDWARE	TB      T-BAR CEILING SYSTEM
SF      STOREFRONT                                                  TK      TACKBOARD FINISH SGP     SEMI-GLOSS PAINT                                      WIN     WINDOW SYSTEM
		
	LEGEND
		
	NEW ACCESS CONTROL PANEL / DOOR	CR CARD READER / ACCESS DEVICE CONTROLLER PANEL TO BE INSTALLED AT
THIS LOCATION FOR THIS BUILDING. INSTALL NEW DEDICATED POWER RECEPTACLE INSIDE PANEL. ALL CARD READERS AND DOOR ACCESSORIES TO
BE ROUTED BACK TO THIS PANEL FOR	DETAIL 15/D1.1

CAMPUS LOCKDOWN	 INSTALL NEW CAT6A DATA CABLE IN NEW ACCESS CONTROL PANEL FOR NETWORK CONNECTIVITY. TERMINATE OUTLET ON BISCUIT JACK INSIDE PANEL
LOCATED INSIDE THE BUILDING ABOVE	AND CONNECT WIRING BACK TO NEAREST THE DOORS.	EXISTING PATCH PANEL IN RACK. REQUEST TO EXIT MODULE
INSTALLED ABOVE DOOR AND
CONNECTED BACK TO DOOR	EXISTING CMU / CONCRETE WALLS
EXISTING WOOD / METAL WALLS
		
		REVISIONS

No.	DATE	DESCRIPTION
	2	.	ADDENDUM 02
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	
	KEYNOTES

	1.      UNMANNED DOOR, PROVIDE CARD READER
2.     CAMPUS LOCKDOWN BUTTON. REFER TO SPECIFICATIONS FOR DETAILS
3.     EXISTING ELECTRICAL PANEL LOCATION. CONTRACTOR TO INSTALL (2) NEW 120V, 20A CIRCUITS FROM PANEL TO NEW ACCESS CONTROL PANEL AND NEW DOOR HARDWARE POWER SUPPLY ENCLOSURE. INSTALL NEW 20A, CIRCUIT BREAKER IN EXISTING PANEL.
		
	GENERAL NOTES
		
	1. DEMO FINISHES TO ACCESS WORK. REPAIR ALL FINISHES BACK TO ORIGINAL FINISH/CONDITION.
2. SEE SPECIFICATIONS FOR MORE INFORMATION.
3. EXISTING EXTERIOR WALL CONDITION IS CONCRETE / CMU SYSTEM U.O.N..
4. SEE DTL. 12/D1.1 FOR ACCESS CONTROL SYSTEM DETAILS.
5. ALL INTERIOR WIREMOLD FROM CEILING TO DOOR WILL BE SURFACE MOUNTED U.N.O..
6. CONNECT DOOR CONTROLLER TO NEAREST OUTLET PREFERRED OR HARDWIRE THE NEXT OPTION. 7. USE WIREMOLD 2000 SERIES AND ACCESSORIES OR EQUAL.
		
	8. ONE LINE DOOR LEAF ON A PAIR OF DOORS SHALL HAVE ELECTRIFIED HARDWARE. REMAINING "DEAD" WILL REMAIN EXIT ONLY AND EXTERIOR HARDWARE PULL WILL BE REMOVED FROM "DEAD" DOOR AND HOLES REPAIRED.
9. DOUBLE DOORS SHALL RECIEVE A REQUEST TO EXIT (REX) DEVICE MOUNTED AT CEILING OR WALL ABOVE DOORS. SINGLE DOORS WILL HAVE REX INSIDE DOOR PANIC HARDWARE.

LIBRARY WING (BUILDING B) CLOVIS HIGH SCHOOL

N
. SCALE: 1/8"=1'-0"

2-05

DATE
CHECKED BY
DRAWN BY
03.01.2023
PROJECT ARCHITECT
JOHN SMITH
PROJECT NUMBER
S2100500AR
.	.
.
.
12
CR
P.A. SPEAKER ALGO 8186 HORN

L

C 15885
9-30-23 RENEWAL DATE
	
REFLECTED CEILING PLAN (BUILDING B)

	
A10.1

KEYNOTES
	
LEGEND

1.      DOOR TO RECEIVE NEW HARDWARE AND CONNECT TO NEW CARD READER.
2.     INSTALL NEW BUILDING ACCESS CONTROL SYSTEM INTEGRATED WITH AUTOMATIC CAMPUS LOCKDOWN INTERFACE
3.     EXISTING RATED WALL
		
AC
	
NEW ACCESS CONTROL PANEL / DOOR	EXISTING RATED WALL CONTROLLER PANEL TO BE INSTALLED AT
THIS LOCATION FOR THIS BUILDING. INSTALL NEW DEDICATED POWER RECEPTACLE INSIDE PANEL. ALL CARD
READERS AND DOOR ACCESSORIES TO	CARD READER / ACCESS DEVICE BE ROUTED BACK TO THIS PANEL FOR
TERMINATION.	DNA DOES NOT APPLY
LOW VOLTAGE PATHWAY	 INSTALL NEW CAT6A DATA CABLE IN NEW ACCESS CONTROL PANEL FOR
NEW 24"x24" ACCESS PANEL                                                           NETWORK CONNECTIVITY. TERMINATE DETAIL 15/D1.1                                                                                    OUTLET ON BISCUIT JACK INSIDE PANEL
AND CONNECT WIRING BACK TO NEAREST MDF/IDF RACK AND TERMINATE ON EXISTING PATCH PANEL IN RACK.

NOTES

1.      PATHWAY IS DIAGRAMATIC IN NATURE BUT SHOWN IN AREAS THAT APPEAR TO BE BEST AVVESSED ABOVE T-BAR SYSTEM. CONTRACTOR MAY PROPOSE A DIFFERENT PATHWAY BUT MUST BE APPROVED BY DISTRICT BEFORE WORK STARTS.
2.     SEE DTL. 12/D1.1 FOR ACCESS CONTROL SYSTEM DETAILS.
3.     ALL INTERIOR WIREMOLD FROM CEILING TO DOOR WILL BE SURFACE MOUNTED U.N.O..

	
	AC

		

DNA

DNA

DNA

AT DOOR FRAME CR

1	B1

1
AT DOOR FRAME CR	D1.1	2
B6	 AC IN ATTIC SPACE

DNA

2

DNA

DNA

DNA

DNA DNA

DNA

DNA

		
CLOVIS HIGH SCHOOL
	
		REVISIONS

No.	DATE	DESCRIPTION
	2	.	ADDENDUM 02
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.

DNA	DNA

LIBRARY WING (BUILDING B) CLOVIS HIGH SCHOOL

N .

SCALE: 1/8"=1'-0"

2-06

DATE
CHECKED BY
DRAWN BY
03.01.2023
PROJECT ARCHITECT
JOHN SMITH
PROJECT NUMBER
S2100500AR
.
.
8

PLASTER
WHERE OCCURS
(E) CEMENT
(E) ALUM. ANGLE
(E) DOOR
1
2
3
HT. VARIES
2
D1.1
CEILING FIN.
6
HM DOOR JAMB
(E) DOOR,
(E) H.M. FRAME
OPTION 1
9
10
11
10
D1.1
L
CORE HOLE
AS REQUIRED
1/2"
PENETRATION
14
E:\08- 47 c entral hi gh school \_updat e to new c ode\det ails\c eil ing\A ccess Panel.dwg 02/19/ 19 07 :13
CORNER
BEAD
SEE PLAN FOR SIZE
HINGE
o/ GYP. BD.
#12 W.S. EA.
#12 SMS EA. SIDE
AT CORNER (8
TOTAL)
15
1	3	9
4
3	1	9
2

						

					

(E) H.M.

				

	

NEW ALUM. CHANNEL FULL HT. FRAME
BOTH SIDES. TO MATCH FINISH. OPTION 2

	
L

C 15885
9-30-23 RENEWAL DATE
	
DETAILS

	
D1.1

(E) PLYWOOD SHEATHING
(E) CONCRETE WALL	(E) VINYL TACKBD, WHERE OCCURS                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             (E) WOOD HEADER
NON-SHRINK OR	SCHEDULE 40 BLACK	EXISTING CMU
EPOXY GROUT	STEEL PIPE SLEEVE.		HT. VARIES	(E) CEMENT NEW WIRE MOLD
NEW WIREMOLD	(E) GYP. BOARD
C	D1.1      OR      D1.1      OR      D1.1	(E) SF DOOR FRAME	(E) J-MOLD
GALVANIZED
STEEL CONDUIT	SEALANT TYP.
PACK WITH OAKUM	(E) ALUM. FLASHING	NEW WIREMOLD

(E) STOREFRONT,
(E) DOOR

(E) DOOR,	(E) H.M. FRAME	ALUM. ANGLE

G:\ ACAD T emp lates\ _Full_De tail.dwg 10/02/12 14 :21
@ CONCRETE / CMU WALL	SCALE: 3" = 1'-0"	HM DOOR HEADER		DOOR HEAD G: \A CAD Te mp lates\_Full_Detail.dwg 10/ 02/1 2 1 4: 21
CONCRETE CONDITION	SCALE: 3" = 1'-0"	D1.1	(E) SF DOOR	@ STORE FRONT	SCALE: 3" = 1'-0" MTL. FRAM'G.	ROUGH OPENING                                                                                                                                                                                                                                                                                                                                                                                                                    OR
DOOR SIZE PLUS 1/4"
CAM LATCH	 (E) PLYWOOD SHEATHING
ACOUSTICAL TILE	OR
EXISTING CMU	(E) 2x FRAMING
(E) VINYL TACKBD, WHERE OCCURS
G: \ACA D Templates\ _Ful l_Detai l.dwg 1 0/02/12 14: 21
ACCESS DOOR w/
ACOUSTICAL TILE INFILL,	CORNER (8 TOTAL)	PLASTER	(E) GYP. BOARD
AT ACOUSTICAL TILE

WD. FRAM'G.	ROUGH OPENING
DOOR SIZE PLUS 1/4"	CAM LATCH	NEW WIREMOLD	(E) FLASHING
HINGE	GYP. BD.	WIRE PASS THROUGH	WIRE PASS THROUGH	NEW WIREMOLD OPTION 1

ACCESS DOOR w/	(E) STOREFRONT, GYP. BD. INFILL,
SEE PLAN FOR SIZE
AT GYP. BD. FIN.
ACCESS PANEL	 RATED WALL PENETRATION	                                                             SEE DETAIL 9/DT1.1 FOR MORE INFORMATION AND ABOVE CEILING CONDITIONS
E:\08-47 central high school\_update to new code\details\ceiling\Access Panel.dwg 02/19/19 07:13	.	SCALE: 1-1/2" = 1'-0"	SCALE: N.T.S.	CONCRETE CONDITION	SCALE: 3" = 1'-0"	STOREFRONT ELEVATION		DOOR JAMB G: \A CAD Te mp lates\_Full_Detail.dwg 10/ 02/1 2 1 4: 21
SCALE: 1" = 1'-0"	@ STOREFRONT	SCALE: 3" = 1'-0" .

(E) STUCCO FINISH	(E) PLY WD.

(E) HEADER BEAM

CEILING FIN.	(E) TACKBOARD, NEW WIRE MOLD	WHERE OCCURS
J-MOLD	NEW WIREMOLD
D1.1      OR      D1.1      OR      D1.1	(E) HM DOOR FRAME
(E) WD. TRIM OR FILLER
(E) ALUM. FLASHING

(E) SCREW, 5/8" DIA.

(E) DOOR,	(E) H.M. FRAME

G:\AC A D Templa tes\_Fu ll_Detail.d wg 1 0/02/1 2 14:21
HM DOOR HEADER
D1.1	(E) HM DOOR	SCALE: 3" = 1'-0"
OR
	
CLOVIS HIGH SCHOOL
	
	REVISIONS

No.	DATE	DESCRIPTION
	2	.	ADDENDUM 02
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.

2

G:\AC AD Te mpl ate s\_Ful l_De tai l. dwg 10/0 2/12 14:21

12

ACCESS CONTROL SYSTEM	4 SCALE: N.T.S.                           D1.1

OR

10

EXISTING STOREFRONT	D1.1 DOOR SYSTEM

RIVETS

NEW ALUM. CHANNEL FULL HT. FRAME
BOTH SIDES. PAINT TO MATCH. OPTION 2

(E) STUCCO FINISH

J-MOLD

(E) PLY WD.

(E) HEADER BEAM

(E) TACKBOARD, WHERE OCCURS

18 GA. MILL FINISH ALUMINUM.

.	.
HARDWARE AS REQUIRED PER DOOR SCHEDULE

EXISTING GLAZING TO REMAIN

(E) ALUM. FLASHING

WIRE PASS THROUGH OPTION 1

(E) WD. TRIM OR FILLER

NEW WIREMOLD

(E) SCREW, 5/8" DIA.

6
13 EXTERIOR SPEAKERS SCALE: N.T.S.	1E : \08-47 central hi gh schoo l\_upd ate to n ew cod e\d etai ls\cei li ng\Access Pa nel .dwg 02/19/19 07:13

DOOR HARDWARE PLATE
.	SCALE: 1-1/2" = 1'-0"

SEE DETAIL 9/DT1.1 FOR MORE INFORMATION AND ABOVE CEILING CONDITIONS G:\AC A D Templa tes\_Fu ll_Detail.d wg 1 0/02/1 2 14:21

HM DOOR ELEVATION

SCALE: 1" = 1'-0"

.

(E) DOOR,	FRAME

4 HM DOOR JAMB

2-07

SCALE: 3" = 1'-0"

DATE
CHECKED BY
DRAWN BY
08.15.2022
PROJECT ARCHITECT
JOHN SMITH
PROJECT NUMBER
S2100500AR
.
.
8

PLASTER
WHERE OCCURS
(E) CEMENT
(E) ALUM. ANGLE
(E) DOOR
1
2
3
HT. VARIES
2
D1.1
CEILING FIN.
6
HM DOOR JAMB
(E) DOOR,
(E) H.M. FRAME
OPTION 1
9
10
11
10
D1.1
L
CORE HOLE
AS REQUIRED
1/2"
PENETRATION
14
E:\08- 47 c entral hi gh school \_updat e to new c ode\det ails\c eil ing\A ccess Panel.dwg 02/19/ 19 07 :13
CORNER
BEAD
SEE PLAN FOR SIZE
HINGE
o/ GYP. BD.
#12 W.S. EA.
#12 SMS EA. SIDE
AT CORNER (8
TOTAL)
15
1	3	9
4
3	1	9
2

						

					

(E) H.M.

				

	

NEW ALUM. CHANNEL FULL HT. FRAME
BOTH SIDES. TO MATCH FINISH. OPTION 2

	
L

C 15885
9-30-23 RENEWAL DATE
	
DETAILS

	
D1.1

(E) PLYWOOD SHEATHING
(E) CONCRETE WALL	(E) VINYL TACKBD, WHERE OCCURS                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             (E) WOOD HEADER
NON-SHRINK OR	SCHEDULE 40 BLACK	EXISTING CMU
EPOXY GROUT	STEEL PIPE SLEEVE.		HT. VARIES	(E) CEMENT NEW WIRE MOLD
NEW WIREMOLD	(E) GYP. BOARD
C	D1.1      OR      D1.1      OR      D1.1	(E) SF DOOR FRAME	(E) J-MOLD
GALVANIZED
STEEL CONDUIT	SEALANT TYP.
PACK WITH OAKUM	(E) ALUM. FLASHING	NEW WIREMOLD

(E) STOREFRONT,
(E) DOOR

(E) DOOR,	(E) H.M. FRAME	ALUM. ANGLE

G:\ ACAD T emp lates\ _Full_De tail.dwg 10/02/12 14 :21
@ CONCRETE / CMU WALL	SCALE: 3" = 1'-0"	HM DOOR HEADER		DOOR HEAD G: \A CAD Te mp lates\_Full_Detail.dwg 10/ 02/1 2 1 4: 21
CONCRETE CONDITION	SCALE: 3" = 1'-0"	D1.1	(E) SF DOOR	@ STORE FRONT	SCALE: 3" = 1'-0" MTL. FRAM'G.	ROUGH OPENING                                                                                                                                                                                                                                                                                                                                                                                                                    OR
DOOR SIZE PLUS 1/4"
CAM LATCH	 (E) PLYWOOD SHEATHING
ACOUSTICAL TILE	OR
EXISTING CMU	(E) 2x FRAMING
(E) VINYL TACKBD, WHERE OCCURS
G: \ACA D Templates\ _Ful l_Detai l.dwg 1 0/02/12 14: 21
ACCESS DOOR w/
ACOUSTICAL TILE INFILL,	CORNER (8 TOTAL)	PLASTER	(E) GYP. BOARD
AT ACOUSTICAL TILE

WD. FRAM'G.	ROUGH OPENING
DOOR SIZE PLUS 1/4"	CAM LATCH	NEW WIREMOLD	(E) FLASHING
HINGE	GYP. BD.	WIRE PASS THROUGH	WIRE PASS THROUGH	NEW WIREMOLD OPTION 1

ACCESS DOOR w/	(E) STOREFRONT, GYP. BD. INFILL,
SEE PLAN FOR SIZE
AT GYP. BD. FIN.
ACCESS PANEL	 RATED WALL PENETRATION	                                                             SEE DETAIL 9/DT1.1 FOR MORE INFORMATION AND ABOVE CEILING CONDITIONS
E:\08-47 central high school\_update to new code\details\ceiling\Access Panel.dwg 02/19/19 07:13	.	SCALE: 1-1/2" = 1'-0"	SCALE: N.T.S.	CONCRETE CONDITION	SCALE: 3" = 1'-0"	STOREFRONT ELEVATION		DOOR JAMB G: \A CAD Te mp lates\_Full_Detail.dwg 10/ 02/1 2 1 4: 21
SCALE: 1" = 1'-0"	@ STOREFRONT	SCALE: 3" = 1'-0" .

(E) STUCCO FINISH	(E) PLY WD.

(E) HEADER BEAM

CEILING FIN.	(E) TACKBOARD, NEW WIRE MOLD	WHERE OCCURS
J-MOLD	NEW WIREMOLD
D1.1      OR      D1.1      OR      D1.1	(E) HM DOOR FRAME
(E) WD. TRIM OR FILLER
(E) ALUM. FLASHING

(E) SCREW, 5/8" DIA.

(E) DOOR,	(E) H.M. FRAME

G:\AC A D Templa tes\_Fu ll_Detail.d wg 1 0/02/1 2 14:21
HM DOOR HEADER
D1.1	(E) HM DOOR	SCALE: 3" = 1'-0"
OR
	
BUD RANK ELEMENTARY
	
	REVISIONS

No.	DATE	DESCRIPTION
	2	.	ADDENDUM 02
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.

2

G:\AC AD Te mpl ate s\_Ful l_De tai l. dwg 10/0 2/12 14:21

12

ACCESS CONTROL SYSTEM	4 SCALE: N.T.S.                           D1.1

OR

10

EXISTING STOREFRONT	D1.1 DOOR SYSTEM

RIVETS

NEW ALUM. CHANNEL FULL HT. FRAME
BOTH SIDES. PAINT TO MATCH. OPTION 2

(E) STUCCO FINISH

J-MOLD

(E) PLY WD.

(E) HEADER BEAM

(E) TACKBOARD, WHERE OCCURS

18 GA. MILL FINISH ALUMINUM.

.	.
HARDWARE AS REQUIRED PER DOOR SCHEDULE

EXISTING GLAZING TO REMAIN

(E) ALUM. FLASHING

WIRE PASS THROUGH OPTION 1

(E) WD. TRIM OR FILLER

NEW WIREMOLD

(E) SCREW, 5/8" DIA.

6
13 EXTERIOR SPEAKERS SCALE: N.T.S.	1E : \08-47 central hi gh schoo l\_upd ate to n ew cod e\d etai ls\cei li ng\Access Pa nel .dwg 02/19/19 07:13

DOOR HARDWARE PLATE
.	SCALE: 1-1/2" = 1'-0"

SEE DETAIL 9/DT1.1 FOR MORE INFORMATION AND ABOVE CEILING CONDITIONS G:\AC A D Templa tes\_Fu ll_Detail.d wg 1 0/02/1 2 14:21

HM DOOR ELEVATION

SCALE: 1" = 1'-0"

.

(E) DOOR,	FRAME

4 HM DOOR JAMB

2-08

SCALE: 3" = 1'-0"

DATE
CHECKED BY
DRAWN BY
03.01.2023
PROJECT ARCHITECT
JOHN SMITH
PROJECT NUMBER
S2100500AR
8

PLASTER
WHERE OCCURS
(E) CEMENT
(E) ALUM. ANGLE
(E) DOOR
1
2
3
HT. VARIES
2
D1.1
CEILING FIN.
6
HM DOOR JAMB
(E) DOOR,
(E) H.M. FRAME
OPTION 1
9
10
11
10
D1.1
L
CORE HOLE
AS REQUIRED
1/2"
PENETRATION
14
E:\08- 47 c entral hi gh school \_updat e to new c ode\det ails\c eil ing\A ccess Panel.dwg 02/19/ 19 07 :13
CORNER
BEAD
SEE PLAN FOR SIZE
HINGE
o/ GYP. BD.
#12 W.S. EA.
#12 SMS EA. SIDE
AT CORNER (8
TOTAL)
15
1	3	9
4
3	1	9
2

						

					

(E) H.M.

				

	

NEW ALUM. CHANNEL FULL HT. FRAME
BOTH SIDES. TO MATCH FINISH. OPTION 2

	
L

C 15885
9-30-23 RENEWAL DATE
	
DETAILS

	
D1.1

(E) PLYWOOD SHEATHING
(E) CONCRETE WALL	(E) VINYL TACKBD, WHERE OCCURS                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                                             (E) WOOD HEADER
NON-SHRINK OR	SCHEDULE 40 BLACK	EXISTING CMU
EPOXY GROUT	STEEL PIPE SLEEVE.		HT. VARIES	(E) CEMENT NEW WIRE MOLD
NEW WIREMOLD	(E) GYP. BOARD
C	D1.1      OR      D1.1      OR      D1.1	(E) SF DOOR FRAME	(E) J-MOLD
GALVANIZED
STEEL CONDUIT	SEALANT TYP.
PACK WITH OAKUM	(E) ALUM. FLASHING	NEW WIREMOLD

(E) STOREFRONT,
(E) DOOR

(E) DOOR,	(E) H.M. FRAME	ALUM. ANGLE

G:\ ACAD T emp lates\ _Full_De tail.dwg 10/02/12 14 :21
@ CONCRETE / CMU WALL	SCALE: 3" = 1'-0"	HM DOOR HEADER		DOOR HEAD G: \A CAD Te mp lates\_Full_Detail.dwg 10/ 02/1 2 1 4: 21
CONCRETE CONDITION	SCALE: 3" = 1'-0"	D1.1	(E) SF DOOR	@ STORE FRONT	SCALE: 3" = 1'-0" MTL. FRAM'G.	ROUGH OPENING                                                                                                                                                                                                                                                                                                                                                                                                                    OR
DOOR SIZE PLUS 1/4"
CAM LATCH	 (E) PLYWOOD SHEATHING
ACOUSTICAL TILE	OR
EXISTING CMU	(E) 2x FRAMING
(E) VINYL TACKBD, WHERE OCCURS
G: \ACA D Templates\ _Ful l_Detai l.dwg 1 0/02/12 14: 21
ACCESS DOOR w/
ACOUSTICAL TILE INFILL,	CORNER (8 TOTAL)	PLASTER	(E) GYP. BOARD
AT ACOUSTICAL TILE

WD. FRAM'G.	ROUGH OPENING
DOOR SIZE PLUS 1/4"	CAM LATCH	NEW WIREMOLD	(E) FLASHING
HINGE	GYP. BD.	WIRE PASS THROUGH	WIRE PASS THROUGH	NEW WIREMOLD OPTION 1

ACCESS DOOR w/	(E) STOREFRONT, GYP. BD. INFILL,
SEE PLAN FOR SIZE
AT GYP. BD. FIN.
ACCESS PANEL	 RATED WALL PENETRATION	                                                             SEE DETAIL 9/DT1.1 FOR MORE INFORMATION AND ABOVE CEILING CONDITIONS
E:\08-47 central high school\_update to new code\details\ceiling\Access Panel.dwg 02/19/19 07:13	.	SCALE: 1-1/2" = 1'-0"	SCALE: N.T.S.	CONCRETE CONDITION	SCALE: 3" = 1'-0"	STOREFRONT ELEVATION		DOOR JAMB G: \A CAD Te mp lates\_Full_Detail.dwg 10/ 02/1 2 1 4: 21
SCALE: 1" = 1'-0"	@ STOREFRONT	SCALE: 3" = 1'-0" .

(E) STUCCO FINISH	(E) PLY WD.

(E) HEADER BEAM

CEILING FIN.	(E) TACKBOARD, NEW WIRE MOLD	WHERE OCCURS
J-MOLD	NEW WIREMOLD
D1.1      OR      D1.1      OR      D1.1	(E) HM DOOR FRAME
(E) WD. TRIM OR FILLER
(E) ALUM. FLASHING

(E) SCREW, 5/8" DIA.

(E) DOOR,	(E) H.M. FRAME

G:\AC A D Templa tes\_Fu ll_Detail.d wg 1 0/02/1 2 14:21
HM DOOR HEADER
D1.1	(E) HM DOOR	SCALE: 3" = 1'-0"
OR
	
FORT WASHINGTON ELEMENTARY
	
	REVISIONS

No.	DATE	DESCRIPTION
	2	.	ADDENDUM 02
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.
	.	.	.

2

G:\AC AD Te mpl ate s\_Ful l_De tai l. dwg 10/0 2/12 14:21

12

ACCESS CONTROL SYSTEM	4 SCALE: N.T.S.                           D1.1

OR

10

EXISTING STOREFRONT	D1.1 DOOR SYSTEM

RIVETS

NEW ALUM. CHANNEL FULL HT. FRAME
BOTH SIDES. PAINT TO MATCH. OPTION 2

(E) STUCCO FINISH

J-MOLD

(E) PLY WD.

(E) HEADER BEAM

(E) TACKBOARD, WHERE OCCURS

18 GA. MILL FINISH ALUMINUM.

.	.
HARDWARE AS REQUIRED PER DOOR SCHEDULE

EXISTING GLAZING TO REMAIN

(E) ALUM. FLASHING

WIRE PASS THROUGH OPTION 1

(E) DOOR,

(E) WD. TRIM OR FILLER

NEW WIREMOLD

(E) SCREW, 5/8" DIA.

.
.
FRAME

6
13 EXTERIOR SPEAKERS SCALE: N.T.S.	1E : \08-47 central hi gh schoo l\_upd ate to n ew cod e\d etai ls\cei li ng\Access Pa nel .dwg 02/19/19 07:13

DOOR HARDWARE PLATE
.	SCALE: 1-1/2" = 1'-0"

SEE DETAIL 9/DT1.1 FOR MORE INFORMATION AND ABOVE CEILING CONDITIONS G:\AC A D Templa tes\_Fu ll_Detail.d wg 1 0/02/1 2 14:21

HM DOOR ELEVATION

SCALE: 1" = 1'-0"

.

4 HM DOOR JAMB

2-10 SCALE: 3" = 1'-0"

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

SECTION 01 10 00

SUMMARY

PART 1 - GENERAL

2-12

1.01	SUMMARY

A.	General: Construction of BASE BID and Alternate portions of the work for Clovis Unified School District – Campus Security Improvement Project Fresno/Clovis, California. BASE BID and Alternate portions of the work is defined as all material, labor, equipment and services necessary to do all work shown on the drawings and called for in the Specifications.

GENERAL SUMMARY OF THE PROJECT

Thefollowinginformationappliesto all Bidpackagesandshallbe reviewedcarefullyfor inclusion ineachbid. Following are critical logistics related to the Project:

1.	Construction of new door lockdown system and improved PA system including all necessary new door hardware, cardreaders, cabling, power supplies, new speakers, integrationintodistrictsystem, demo and patch of any disturbed finishes.

2.	All work for the project will be performed during the hours of 7:00 a.m to 3:30 p.m. Work will be performed on an active campus with students and teachers present.

3.	Submittals and material procurement shallbegin immediately upon award or letter of intent from the District.

4.	Material procurement is critical and shall be diligently pursued to meet the contract schedule.

5.	Bid packages shall review the project completely prior to bidding the work.

6.	Any substitution of details or materials must be pre-approved by the Architect, engineers and DSA. Allsubstitution requestsmust besubmitted per Notice To Contractors.Bid Packagesareresponsible for all costs and time delays required for substitution approval.

In addition to the summary of work for each Bid Package, the following will apply and become a part of the contract with each respective Bid package.

STORM WATER POLLUTION PREVENTION PLAN AND DUST CONTROL

1.	Not Applicable.

ALTERNATES

1.	None.

SUBMITTALS AND MATERIAL PROCUREMENT

1.	Submittals and material procurement shallbegin immediately upon award or letter of intent from the District.

2.	Material procurement is critical and shall be diligently pursued to meet the contract schedule.

SUMMARY 01 10 00 - 1

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

SCHEDULE

1.	Bid packages shall review the project and schedule completely prior to bidding the work.

2.	Thebidpackagewillbe requiredtoprovidea schedule and crewsizing showinghow thework willbe accomplished within the given time frame.

CREW SIZES

1.	All bid packages shall review the schedule and confirm that they can crew the project accordingly prior to submitting a bid. Include with each bid minimum and maximum crew sizes projected for the project.

STATE AGENCY REQUIREMENTS

1.	All work shall comply with OSHA requirements.

COORDINATION OF WORK

1.	Coordination of work during the preconstruction period is equally as critical to resolving all issues priorto thestart of work. Bidpackageshallreview theproject, coordinate andquestionanyissuesto allow resolution prior to the start of work.

2.	Review and verify all existing conditions.

3.	Provide all necessary temporary utilities for own work.

4.	All bid packages shall attend coordination meetings and provide coordination drawings for work related to other trades. Note conflicts and provide potential solutions to the architect for review. Coordination and drawingapprovalmustoccur prior to start ofwork. Bid packagesshallattendapre-installation meeting prior to the start of their work onsite. All bid packages shall be available for pre-installation meetings of other bid packages for coordination of related work.

5.	Provide written request for information through the CM for layout information from related trades.

6.	Request and review all associated shop drawings for coordination and layout purposes prior to installation of related materials.

7.	Review all as-builts prior to starting work.

SITE LOGISTICS:

1.	Only company vehicles are allowed onsite. No tool drop-off or parking by personal vehicles will be allowed. Bid package to make provisions for transport or tool distribution needs.

2.	Lunch and breaks shall be at designated areas only. No other areas will be allowed.

3.	Storageareaswillbeconfinedto the areas designated bytheCM. Stagingareasaroundthebuilding shall be coordinated with the CM. Storage onsite will be controlled due to limited space available.

4.	Daily cleanup and off-haul is required for each trade for their own work debris.

SUMMARY 01 10 00 - 2

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

GENERAL ITEMS TO BE PROVIDED BY EACH BID PACKAGE:

1.	Protect all work, new and existing, from damage until acceptance by owner.

2.	Provide water and shade for own crews.

3.	Furnish all access to roof for own work.

4.	Furnish and install own floor protection as needed (Tarps, plastic, plywood, etc needed to protect work for own scope

5.	Furnish and install all physical layout for own work.

6.	Each bid package will be responsible for removal from the site of all debris and spoils generated by each bid package.

7.	Secure all ladders and lifts each evening.

8.	Provide protection of all roofing when own work requires access on the roofing systems.

9.	Provide caution tape and/or barriers for open area work and traffic control.

10.	Provide safe condition for own installations so as not to expose any person to a safety hazard per OSHA regulations.

11.	Any substitution of details or materials must be pre-approved by the Architect, Engineers and DSA. All substitution requests must be submitted to MWC prior to bid. This bid package is responsible for all costs and time delays required for substitution approval.

12.	Review as-builts prior to starting work.

13.	Provide copy of daily reports to Construction Manager each day work is performed on site.

14.	Provide copy of weekly safety meeting sign-in sheet to Construction Manager each week work is performed on-site.

15.	This project will be constructed on an active campus during school hours. Work will be performed around studentsandteachers.Anyworkthatneedstobeperformedin/aboveclassroomswillneedto becompleted beforeor afterschool.Allemployeesworkingonsiteshallbewearing badgesand pass CUSD background check. Any communication with teachers/students will not be acceptable and employees will be removed from the job site immediately.

SUMMARY 01 10 00 - 3

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

BID PACKAGE

CDL-01 – DOOR HARDWARE

Furnishandinstallallworkspecificallyrequiredthroughout theprojectdocumentstocompletetheworkof this bid package that specifically includes, but is not limited to the following:

SPECIFICATION SECTIONS

DIVISION 00 DIVISION 01
08 11 13 08 71 00

HOLLOW METAL DOORS AND FRAMES DOOR HARDWARE

Referto additionalrelated specificationssectionsforworkspecificallyincluded in thisbidpackagenotedbelow.

GENERAL ITEMS

1.	Furnish and install all layout for own work.

2.	Provide all power for own work.

3.	See General Notes at beginning of summary of work specification section for other items.

COORDINATION WITH OTHER TRADES –

1.	Coordinate physical connection to door hardware with low voltage contractor.

2.	Coordinate student access to allow proper student flow.

FURNISH AND INSTALL ITEMS

1.	Furnish and install alldoor hardware.Referto FOB itemsbelow for items to be installed byelectrical package.Remove anyexistingdoor hardwarerequired for installation of newhardwareandturnover to District.

2.	Drill all necessary holes in doors and frames as required to allow for installation of own work.

3.	Furnish and install new doors where shown.

4.	Furnish and install any cover plates as shown on drawings to cover any existing holes in doors/frames.

FOB Items

1.	Furnish FOB jobsite door hardware power supplies/battery backups to be installed by the Electrical/Low Voltage Contractor.

INSTALLATION OF FOB ITEMS

1.	None

END OF BID PACKAGE

SUMMARY 01 10 00 - 4

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

BID PACKAGE

CDL-02 – ELECTRICAL & LOW VOLTAGE

Furnish andinstallallworkspecificallyrequiredthroughout theprojectdocumentstocompletetheworkof this bid package that specifically includes, but is not limited to the following:

SPECIFICATION SECTIONS

DIVISION 00 DIVISION 01
06 10 00 08 41 13 08 80 00 09 91 23 26 00 00 26 05 00 27 10 00 27 51 13 28 31 00

ROUGH CARPENTRY
ALUMINUM FRAMED ENTRANCES AND STOREFRONTS GLASS AND GLAZING
PAINTING
GENERAL ELECTRICAL
COMMON WORK RESULTS FOR ELECTRICAL STRUCTURED CABLING SYSTEM
PAGING SYSTEMS
ACCESS CONTROL SYSTEM

Referto additionalrelated specificationssectionsforworkspecificallyincluded in thisbid packagenotedbelow.

GENERAL ITEMS

1.	Furnish and install all layout for own work

2.	Provide all power for own work.

3.	See General Notes at beginning of summary of work specification section for other items

COORDINATION WITH OTHER TRADES

1.	Coordinate physical connection to door hardware with low voltage contractor.

2.	Coordinate student access to allow proper student flow.

3.	Provide useofelectricalequipmentanddevicesasrequiredbytheConstructionManagerfortesting ofequipment priorto finalacceptance,which willnotinitiatethe warrantyperioduntilfiling of noticeof completion.

FURNISH AND INSTALL ITEMS

1.	Furnish and install all required cabling for door lock and PA systems.

2.	Furnish and install all surface-mounted raceways for any cabling that can not be run inside walls/ceilings/frames. Wiring shall be routed through storefront/HM frames where possible. Grout filled framesshallreceive surface mount wiremold. Emergencypush button at front office desk shall be installed in wall adjacent to reception desk as shown on drawings. Wiring to be concealed inside wall if possible.

3.	Furnish and install surface mount EMT conduit in gymnasiums. Paint conduit to match adjacent surroundings.

SUMMARY 01 10 00 - 5

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

4.	Furnish and install ceiling wires and cable supports for cabling running above accessible ceiling. Brace every 4’.

5.	Remove and reinstall any glass in storefront/HM systems as required for access to own work.

6.	Remove and reinstall acoustical ceiling tiles as required for access to own work. Any damaged tiles shall be replaced at contractors expense.

7.	Furnish and installfirestoppingfor ownwork asrequired at anypenetrationsthrough firewalls.Refer to plans for firewall locations.

8.	Furnishandinstallallaccess doorsnecessaryto provide accesstoworkincludedin thisbidpackage. Anticipated access doors are shown on drawings. Provide required ceiling/soffit framing for installation of access doors.

9.	Furnish and install watertight closures at all penetrations through exterior walls.

10.	Furnish andinstallallnew speakersandcablingforPAsystem upgrade asshownondrawings.Make physical connection to existing system.

11.	Drill all necessary holes/sleeves in walls, doors, and frames as required to allow for installation of own work.

12.	Furnish andinstallallsecurity/accesscontrolpanelsand powersuppliesfor allbuildingsasrequired.

13.	Make final connection/termination where cabling connects to door hardware.

14.	Furnish and install power for door notifier/power supplies/battery backups. See detail 12/D1.1 for additional information. Provide power from existing electrical panel to equipment location as called out on plans.

15.	Furnish and install emergency push button located at front desk as indicated on drawings.

16.	Furnish and install lockable enclosure panel for all power supplies and battery backups to allow for clean installationandto eliminatepotentialvandalismto equipment exposed to publicview.Refer to drawings for exact locations and sizes.

17.	Furnish and install network cabling to access control equipment.

18.	Furnish and install card readers, security wiring, and headend equipment.

19.	Furnish and install interface relays, door position contacts, and request to exit devices.

FOB ITEMS

1.	None

INSTALLATION OF FOB ITEMS

1.	Install power supplies/battery backups furnished FOB by Door Hardware Contractor.

SUMMARY 01 10 00 - 6

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

2.	Any equipment/materialprovided FOB from the door hardware bid package and installed by this bid package, the installing contractor shall meet all certifications/licensing requirements necessary to install and warranty the product.

END OF BID PACKAGE

SEE ATTACHED SCHEDULE

END OF SECTION 01 10 00

SUMMARY 01 10 00 - 7

ID
	
1

	Task
Mode 
	Task Name
	
BUD RANK ELEM
	Duration
	
	Start
	
Thu 11/9/23
	Finish

	Nov	Dec	
	Qtr 1, 2024
	Jan	Feb	
	
				27 days
		Fri 12/15/23
				
2
			INSTALL NEW DOOR HARDWARE
	6 days
	Thu 11/9/23
	Thu 11/16/23
				
3
			PULL CABLING/RUN WIREMOLD
	9 days
	Tue 11/14/23
	Fri 11/24/23
				
4
			INSTALL CARD READERS/SPEAKERS
	5 days
	Mon 11/27/2
	Fri 12/1/23
				
5
			TERMINATE DEVICES
	3 days
	Mon 12/4/23
	Wed 12/6/23
				
6
			TEST SYSTEM
	2 days
	Thu 12/7/23
	Fri 12/8/23
				
7
			PUNCHLIST CORRECTIONS
	5 days
	Mon 12/11/2
	Fri 12/15/23
				
8
			FORT WASHINGTON
	23 days
	Fri 11/17/23
	Tue 12/19/23
				
9
			INSTALL NEW DOOR HARDWARE
	4 days
	Fri 11/17/23
	Wed 11/22/2
				
10
			PULL CABLING/RUN WIREMOLD
	6 days
	Wed 11/22/2
	Wed 11/29/2
				
11
			INSTALL CARD READERS/SPEAKERS
	4 days
	Thu 11/30/23
	Tue 12/5/23
				
12
			TERMINATE DEVICES
	3 days
	Wed 12/6/23
	Fri 12/8/23
				
13
			TEST SYSTEM
	2 days
	Mon 12/11/2
	Tue 12/12/23
				
14
			PUNCHLIST CORRECTIONS
	5 days
	Wed 12/13/2
	Tue 12/19/23
				
15
			CLOVIS HIGH
	59 days
	Thu 11/23/2
	3Tue 2/13/24

										
16
			INSTALL NEW DOOR HARDWARE
	18 days
	Thu 11/23/23
	Mon 12/18/2
				
17
			PULL CABLING/RUN WIREMOLD & CONDUIT
	26 days
	Thu 11/30/23
	Thu 1/4/24

										
18
			INSTALL CARD READERS/SPEAKERS
	12 days
	Fri 1/5/24
	Mon 1/22/24
				
19
			TERMINATE DEVICES
	8 days
	Tue 1/23/24
	Thu 2/1/24
				
20
			TEST SYSTEM
	3 days
	Fri 2/2/24
	Tue 2/6/24
				
21
			PUNCHLIST CORRECTIONS
	5 days
	Wed 2/7/24
	Tue 2/13/24

										

Project: CUSD Lockdown Contr Date: Wed 5/10/23
	Task	Project Summary	Manual Task	Start-only	Deadline
Split	Inactive Task	Duration-only	Finish-only	Progress
Milestone	Inactive Milestone	Manual Summary Rollup	External Tasks	Manual Progress
Summary	Inactive Summary	Manual Summary	External Milestone
	
Page 1