Addendum No. 03 May 19, 2023

Campus Security Improvement Phase 1

OWNER:

PREPARED BY:

PBK PROJECT NO.: DSA FILE NO.:
DSA APPLICATION NO.:

Clovis Unified School District

1450 Herndon Ave. Clovis, CA. 93611

PBK Architects, Inc. 7790 N. Palm Avenue Fresno, California 93711

S2100500AR N/A
N/A

NOTICE TO BIDDERS

A. Receipt of this Addendum shall be acknowledged on the Proposal Form.
B. This Addendum forms part of the Contract Documents for the above referenced project and shall be incorporated integrally therewith.
C. Each proposer shall make necessary adjustments and submit their proposal with full knowledge of all modifications, clarifications, and supplemental data included therein. Where provisions of the following supplemental data differ from those of the original Contract Documents, this Addendum shall govern.

GENERAL:

3-01	Bid Open Date, revise as follows:

Revise open bid date from 05-30-2023 at 1:00 pm to 05-31-2023 at 1:00 pm. See attached.

3-02	Bid Walk Sign-in Sheet, as follows:

Bid walk sign-in sheet 05-16-2023. See attached.

3-03	Bid Walk Sign-in Sheet, as follows:

Bid walk sign-in sheet 05-18-2023. See attached.

3-04	Hardware Package, revise as follows:

Changing the license requirement for the door hardware package from a “B” License to a “C28” License.

3-05	Campuses and Buildings, revise as follows: 1.	Applies to all campuses and buildings:
a.     At door power supply wall mounted enclosure, contractor shall hard wire the 20A circuit wiring at the door power supply enclosure in lieu of plug-in style power connec&on. Mark panel and circuit informa&on on junc&on box indica&ng power connec&on informa&on.

b. All new exterior speakers shall be Bogen SAH15 model.

1

Addendum No. 03 May 19, 2023

Campus Security Improvement Phase 1 CLOVIS HIGH SCHOOL:

3-06	Sheet A3.0 – MULTI-PURPOSE (BUILDING F), revise as follows:

Revise location of AC panel and Electrical panels. Add ceiling access panel. See attached.

3-07	Sheet A3.0 – MULTI-PURPOSE (BUILDING F), revise as follows:
a.     Updated loca&on of exis&ng electrical panel in kitchen back hallway to provide (2) circuits back to IDF room for power to card reader control panel and door power supplies.
b. Updated loca&on of exis&ng headend IDF cabinet in Kitchen Manager’s Oﬃce. Mount new access control panel and door power supplies high up on wall next to exis&ng IDF wall cabinet.

3-08	Sheet A3.1 – REFLECTED CEILING PLAN (BUILDING F), revise as follows: Revise location of AC panel. See attached.

3-09	Sheet A10.0 – LIBRARY (BUILDING B), revise as follows:

AC symbol revise note to read. ”AC IN WALL ATTIC SPACE”. See attached.

3-10	Sheet A4.0 – CLASSROOM (BUILDING C), revise as follows:
a.     Exis&ng electrical panel keyed note shall be iden&ﬁed as keyed note #4 on plan in lieu of keyed note #3.
b. Update keyed note #4 for exis&ng electrical panel at back electrical room. Provide (2) – Square D, 20A tandem single pole circuit breaker in exis&ng panelboard where available breaker space is limited. Contractor to replace exis&ng two 20A breakers with new tandem breakers. One breaker is for the new door power supplies and the other circuit will be for the new access control panel. Contractor to update label in panel indica&ng addi&onal load informa&on.

3-11	Sheet A5.0 – CLASSROOM (BUILDING D), revise as follows:
a.     Update keyed note #4 for exis&ng electrical panel at back electrical room. Provide (2) – Square D, 20A tandem single pole circuit breaker in exis&ng panelboard where available breaker space is limited. Contractor to replace exis&ng two 20A breakers with new tandem breakers. One breaker is for the new door power supplies and the other circuit will be for the new access control panel. Contractor to update label in panel indica&ng addi&onal load informa&on.

3-12	 Sheet A10.1 – REFLECTED CEILING PLAN (BUILDING B), revise as follows: AC symbol revise note to read. “AC IN WALL ATTIC SPACE”. See attached.

3-13	 Sheet A11.0 – NORTH GYM (BUILDING N), revise as follows: Revise location of AC panel and Electrical panels. See attached.

3-14	Sheet A11.0 – NORTH GYM (BUILDING N), revise as follows:
a.     Updated loca&on of exis&ng electrical panel ‘L400B’ in band storage room that will provide two circuits for the access control panel and door power supplies.

2

Addendum No. 03 May 19, 2023

Campus Security Improvement Phase 1

b. Updated loca&on of exis&ng wall mounted IDF in band prac&ce room.

3-15	Sheet A11.1 – REFLECTED CEILING PLAN (BUILDING N), revise as follows: Revise location of AC panel. See attached.

3-16	Sheet A12.0 – SOUTH GYM (BUILDING S), revise as follows: Revise location of Electrical panels. See attached.

3-17	Sheet A12.0 – SOUTH GYM (BUILDING S), revise as follows:

a. Update location of existing electrical panel ‘G3P’ near stairway that will provide two circuits for access control panel and door power supplies.

3-18	 Pictures – CLASSROOM WING (BUILDING D), revise as follows: Add picture at office IDF wall mounted. See attached.

3-19      Pictures – MPR (BUILDING F), revise as follows: Add pictures at MPR doors. See attached.

3-20	 Pictures – SOUTH GYM (BUILDING S), revise as follows: Add pictures at South Gym door. See attached.

BUD RANK ELEMENTARY:

3-21	 Sheet A2.0 – ADMINISTRATION (BUILDING A), revise as follows: Add ceiling access panel at Library. See attached.

3-22	Sheet A2.0 – ADMINISTRATION (BUILDING A), revise as follows:
Update keyed note #4 for exis&ng electrical panel at headend IDF room, Panel ‘L1A’. Provide (2)

– Square D, 20A tandem single pole circuit breaker in exis&ng panelboard where available breaker space is limited. Contractor to replace exis&ng two 20A breakers with new tandem breakers. One breaker is for the new door power supplies and the other circuit will be for the new access control panel. Contractor to update label in panel indica&ng addi&onal load informa&on.

3-23	 Sheet A2.1 – REFLECTED CEILING PLAN (BUILDING A), revise as follows: Add ceiling access panel at Library. See attached.

3-24	Sheet A6.0 – CLASSROOM WING (BUILDING E), revise as follows:
Update keyed note #4 for exis&ng electrical panel, Panel ‘L5A’. Provide (2) – Square D, 20A

tandem single pole circuit breaker in exis&ng panelboard where available breaker space is limited. Contractor to replace exis&ng two 20A breakers with new tandem breakers. One breaker is for the new door power supplies and the other circuit will be for the new access control panel. Contractor to update label in panel indica&ng addi&onal load informa&on.

3

Addendum No. 03 May 19, 2023

Campus Security Improvement Phase 1

3-25      Pictures – MPR (BUILDING F), revise as follows: Add pictures at MPR doors. See attached.

FT. WASHINGTON ELEMENTARY:

3-26	Sheet A4.0 – LIBRARY MEDIA (BUILDING G), revise as follows:

Update keyed note #3 for exis&ng electrical panel at headend IDF room, Panel ‘ALM’. Provide (2) – Square D, 20A tandem single pole circuit breaker in exis&ng panelboard where available breaker space is limited. Contractor to replace exis&ng two 20A breakers with new tandem breakers. One breaker is for the new door power supplies and the other circuit will be for the new access control panel. Contractor to update label in panel indica&ng addi&onal load informa&on.

3-27	 Sheet A5.0 – ADMINISTRATION/MPR (BUILDING D), revise as follows: Revise location of Electrical panels. See attach.

3-28	Sheet A5.0 – ADMINISTRATION/MPR (BUILDING D), revise as follows:
Update keyed note #5 for exis&ng electrical panel at headend IDF room. Exis&ng Panel ‘B’ in principal’s oﬃce. Provide (2) – Square D, 20A tandem single pole circuit breaker in exis&ng panelboard where available breaker space is limited. Contractor to replace exis&ng two 20A breakers with new tandem breakers. One breaker is for the new door power supplies and the other circuit will be for the new access control
panel. Contractor to update label in panel indica&ng addi&onal load informa&on.

3-29	Sheet D1.1 – DETAILS, revise as follows:

Detail 13 shall be modiﬁed so that all new exterior intercom paging speakers shall be Bogen SAH15 in lieu of Algo 8186 models. All new intercom paging speakers shown on plans shall be Bogen SAH15 models connected back to local building terminal cabinet for connec&on back to intercom backbone system.

SPECIFICATION SECTIONS:

3-30	 Section 01 25 00 – REQUEST FOR SUBSTITUTION, revise as follows: Add Request for Substitution form. See attach.

3-31	Section 28 13 00 – ACCESS CONTROL SYSTEM, revise as follows: a.     All mullion mounted readers shall be MTB11 in lieu of MT11. b. Any wall mounted readers shall be MT15 in lieu of MTK15.

3-32	 Section 01 10 00 Schedule of Work, revise as follows: Revise Schedule of Work. See attached.

4

Addendum No. 03 May 19, 2023

Campus Security Improvement Phase 1

END OF ADDENDUM NO. 3

John Hamilton Smith

__________________________________ NAME OF ARCHITECT, Architect

5

3-01 NOTICE TO CONTRACTORS

Notice is hereby given that CLOVIS UNIFIED SCHOOL DISTRICT, (hereinafter referred to as "Owner") will receive sealed bids prior to the date and time stated for the Bid Opening for construction of:

BID 2942– CAMPUS SECURITY IMPROVEMENTS PHASE 1

as per drawings and specifications which may be obtained from architect: MARK WILSON CONSTRUCTION
Attention: Cole Bendoski
5799 E Clinton Ave. Fresno, CA 93727 Email: estimating@markwilsonconstruction.com
Phone: 559-348-0421

Upon receipt of the contract documents provide the following information: 1.      Organization/Contact Person for each Prime Contractor
2.	Mailing address and P.O. Box Number for each Prime Contractor 3.	Phone Number for each Prime Contractor
4.	FAX Number for each Prime Contractor

The project will be bid as multiple prime contracts according to the list below:

Bid Form Bid

Package #
	Bid Package

Description
	Contractor License

Requirement (, = or)
	
CSI –01
	DOOR HARDWARE
	B
	
CSI –02
	ELECTRICAL & LOW VOLTAGE
	C-7 or C-10

Mandatory Pre-Bid Meeting
To be eligible to bid this project, ALL bid packages must attend at least one pre-bid meeting job walk. Contractor must visit all sites on either May 16, 2023 or May 18, 2023 as follows:

First Meeting Tuesday, May 16, 2023
1.Fort Washington Elementary School located at 960 E Teague Ave, Fresno CA 93720 at 9:00am. Meet at flagpole.
2.Bud Rank Elementary School located at 3650 Powers Ave. Clovis, CA 93619 at 10:00am. Meet at flagpole.
3.Clovis High School located at 1055 Fowler Ave. Clovis, CA 93611 at 11:00am. Meet at flagpole.

Second meeting, Thursday May 18, 2023:
1.Fort Washington Elementary School located at 960 E Teague Ave, Fresno CA 93720 at 9:00am. Meet at flagpole.
2.Bud Rank Elementary School located at 3650 Powers Ave. Clovis, CA 93619 at 10:00am. Meet at flagpole.
3.Clovis High School located at 1055 Fowler Ave. Clovis, CA 93611 at 11:00am. Meet at flagpole.

Time of completion for this project shall be 90 calendar days (per construction manager’s work schedule) from the start of the project as established within the Owner’s Notice to Proceed. All procurement, coordination, milestones, durations, activities, and sequences for the bid packages shall be performed as shown in the Construction Management Bid Schedule and Section 01320 of the specification and as modified by a monthly schedule update, if any.

Bids will be sealed and filed at the following address: Bids will NOT be accepted at the bid opening location.

Clovis Unified School District PURCHASING
1450 Herndon Avenue Clovis, California 93611

before 1:00 p.m. on May 31, 2023
Bids will be opened in public at the following address: Bids will NOT be accepted at the bid opening location.
Clovis Unified School District CONSTRUCTION SERVICES OFFICE 1470 Herndon Avenue Clovis, California 93611
The DVBE Declaration of Good Faith Efforts to use Disabled Veteran Business Enterprises must be signed, filed, and included in sealed bid package, before 1:00 p.m. on May 31, 2023, at which time the bids (including the DVBE Declaration of Good Faith Efforts to Use Disabled Veteran Business Enterprises) will be opened in public.

Bids must be accompanied by a bidder's bond, cashier's check, or certified check for at least ten per cent (10%) of the amount of the base bid and made payable to the Owner, issued by an Admitted Surety (an insurance organization authorized by the Insurance Commissioner to transact business of insurance in the State of California during this calendar year), which shall be given as a guarantee that the bidder will enter into a contract if awarded the work and will be declared forfeited, paid to, or retained by the Owner as liquidated damages if the bidder refuses or neglects to enter into the contract provided by the Owner after being requested to do so.

The Contractor shall be required to satisfy the conditions set forth in the contract and Education Code section 45125.2 regarding fingerprinting requirements and student safety prior to permitting any contact with students. Upon award of the contract and before beginning work, the Contractor shall be required to provide a verification of compliance with the student safety provisions of the contract and Education Code section 45125.2.

Upon award of the bid, require signature on the enclosed declaration to ensure compliance with the general Conditions and the Education Code.

The successful bidder will be required to furnish a Payment (Labor and Material) Bond in the amount of one hundred per cent (100%) of the contract price, and a Faithful Performance Bond in the amount of one hundred per cent (100%) of the contract price, said bonds to be secured from an Admitted Surety (an insurance organization authorized by the Insurance Commissioner to transact business of insurance in the State of California during this calendar year), and satisfactory to the Owner. The bidder will be required to give satisfactory proof to the Owner of the maintenance of Public Liability and Property Damage Insurance in an amount with a combined single limit of not less than $2,000,000 per occurrence.

The successful bidder will be allowed to substitute securities or establish an escrow in lieu of retainage, pursuant to Public Contract Code Section 22300, and as described in the General Conditions.

The Owner will not consider or accept any bids from contractors who are not licensed to do business in the State of California, in accordance with the California Public Contract Code, providing for the licensing of contractors. In accordance with Section 3300 of said Code, the Contractor shall have a license classification as described in the MULTIPLE PRIME CONTRACT SCHEDULE.

Pursuant to Labor Code sections 1725.5 and 1771.1, all contractors and subcontractors that wish to bid on, be listed in a bid proposal, or enter into a contract to perform public work must be registered with the Department of Industrial Relations. No bid will be accepted, nor any contract entered into without proof of the contractor’s and subcontractors’ current registration with the Department of Industrial Relations to perform public work. If awarded a Contract, the Bidder, and its subcontractors, of any tier, shall maintain active registration with the Department of Industrial Relations for the duration of the Project.

This Project is subject to compliance monitoring and enforcement by the Department of Industrial Relations. In bidding on this project, it shall be the Bidder’s sole responsibility to evaluate and include the cost of complying with all labor compliance requirements under this contract and applicable law in its bid.

The lowest bid shall be determined as follows: The lowest total of the prime bid on the base contract and the bids on all additive items and all deductive items. (Public Contract Code section 20103.8, subd. (b)). The District reserves the right to add or deduct any of the additive or deductive items from the project or contract after the lowest responsible and responsive bidder is determined.

The Director of the Department of Industrial Relations of the State of California, in the manner provided by law, has ascertained the general prevailing rate per diem wages and rate for legal holidays and overtime work as set forth in the Agreement. The Contractor must pay for any labor therein described or classified in an amount not less than rates specified. Copies of the required rates are on file at the Owner's business office and are available to any interested party on request.

The Owner reserves the right to waive any irregularity and to reject any or all bids.

Unless otherwise required by law, no bidder may withdraw its bid for a period of sixty (60) days after date set for the opening thereof.
Dated:	May 5, 2023	Clovis Unified School District

Advertise:	May 5, 2023 May 12, 2023

By: MICHAEL JOHNSTON
ASSISTANT SUPERINTENDENT OF BUSINESS SERVICES

3-02

3-03

3-18

Clovis H.S. BUILDING D IDF

3-19

Clovis H.S. MPR
F10

Clovis H.S. MPR
F10

Clovis H.S. MPR
F11

Clovis H.S. MPR
F11

Clovis H.S. MPR
F12

Clovis H.S. MPR
F12

3-20

Clovis H.S. South Gym S7

Clovis H.S. South Gym S7

3-25

Bud Rank MPR
F2, F3, F4

Bud Rank MPR
F2, F3, F4

CUSD District Wide Lockdown Project No. S2100500AR	Clovis Unified School District

3-30

CUSD District Wide Lockdown Clovis Unified School District

Project No. S2100500AR

CUSD District Wide Lockdown Project No. S2100500AR	Clovis Unified School District

PBK Architects
Project No. S2100500AR

SECTION 01 10 00

SUMMARY (ADM 3)

CUSD District Wide Lockdown Clovis Unified School District

3-32

PART 1 - GENERAL

1.01	SUMMARY

A.	General: Construction of BASE BID and Alternate portions of the work for Clovis Unified School District – Campus Security Improvement Project Fresno/Clovis, California. BASE BID and Alternate portionsof theworkis defined asallmaterial, labor, equipment, and servicesnecessary to do all work shown on the drawings and called for in the Specifications.

GENERAL SUMMARY OF THE PROJECT

Thefollowinginformationappliesto all Bidpackagesandshallbe reviewedcarefullyfor inclusion ineachbid. Following are critical logistics related to the Project:

1.	Construction of new door lockdown system and improved PA system including all necessary new door hardware, cardreaders, cabling, power supplies, new speakers, integrationintodistrictsystem, demo and patch of any disturbed finishes.

2.	All work for the project will be performed during the hours of 7:00a.m to 3:30 p.m. Work will be performed on an active campus with students and teachers present.

3.	Submittals and material procurement shallbegin immediately upon award or letter of intent from the District.

4.	Material procurement is critical and shall be diligently pursued to meet the contract schedule.

5.	Bid packages shall review the project completely prior to bidding the work.

6.	Any substitution of details or materials must be pre-approved by the Architect, engineers, and DSA. Allsubstitution requestsmust besubmitted per NoticeToContractors. BidPackagesareresponsible for all costs and time delays required for substitution approval.

In addition to the summary of work for each Bid Package, the following will apply and become a part of the contract with each respective Bid package.

STORM WATER POLLUTION PREVENTION PLAN AND DUST CONTROL

1.	Not Applicable.

ALTERNATES

1.	None.

SUBMITTALS AND MATERIAL PROCUREMENT

1.	Submittals and material procurement shallbegin immediately upon award or letter of intent from the District.

2.	Material procurement is critical and shall be diligently pursued to meet the contract schedule.

SUMMARY 01 10 00 - 1

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

SCHEDULE

1.	Bid packages shall review the project and schedule completely prior to bidding the work.

2.	Thebidpackagewillbe requiredtoprovidea schedule and crewsizing showinghow thework willbe accomplished within the given time frame.

CREW SIZES

1.	All bid packages shall review the schedule and confirm that they can crew the project accordingly prior to submitting a bid. Include with each bid minimum and maximum crew sizes projected for the project.

STATE AGENCY REQUIREMENTS

1.	All work shall comply with OSHA requirements.

COORDINATION OF WORK

1.	Coordination of work during the preconstruction period is equally as critical to resolving all issues priorto thestart of work. Bidpackageshallreview theproject, coordinate andquestionanyissuesto allow resolution prior to the start of work.

2.	Review and verify all existing conditions.

3.	Provide all necessary temporary utilities for own work.

4.	All bid packages shall attend coordination meetings and provide coordination drawings for work related to other trades. Note conflicts and provide potential solutions to the architect for review. Coordination and drawingapprovalmustoccur prior to start ofwork. Bid packagesshallattendapre-installation meeting prior to the start of their work onsite. All bid packages shall be available for pre-installation meetings of other bid packages for coordination of related work.

5.	Provide written request for information through the CM for layout information from related trades.

6.	Request and review all associated shop drawings for coordination and layout purposes prior to installation of related materials.

7.	Review all as-builts prior to starting work.

SITE LOGISTICS

1.	Only company vehicles are allowed onsite. No tool drop-off or parking by personal vehicles will be allowed. Bid package to make provisions for transport or tool distribution needs.

2.	Lunch and breaks shall be at designated areas only. No other areas will be allowed.

3.          Storageareaswillbeconfinedto the areas designated bytheCM. Stagingareasaround the building shall be coordinated with the CM. Storage onsite will be controlled due to limited space available.

4.	Daily cleanup and off haul is required for each trade for their own work debris.

SUMMARY 01 10 00 - 2

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

GENERAL ITEMS TO BE PROVIDED BY EACH BID PACKAGE

1.	Protect all work, new and existing, from damage until acceptance by owner.

2.	Provide water and shade for own crews.

3.	Furnish all access to roof for own work.

4.	Furnish and install own floor protection as needed(Tarps, plastic, plywood, etc needed to protect work for own scope

5.	Furnish and install all physical layout for own work.

6.	Each bid package will be responsible for removal from the site of all debris and spoils generated by each bid package.

7.	Secure all ladders and lifts each evening.

8.	Provide protection of all roofing when own work requires access on the roofing systems.

9.	Provide caution tape and/or barriers for open area work and traffic control.

10.	Provide safe condition for own installations so as not to expose any person to a safety hazard per OSHA regulations.

11.	Any substitution of details or materials must be pre approved by the Architect, Engineers and DSA. Allsubstitutionrequestsmust be submitted to MWC prior to bid. This bid package isresponsible for all costs and time delays required for substitution approval.

12.	Review as-builts prior to starting work.

13.	Provide copy of daily reports to Construction Manager each day work is performed on site.

14.	Provide copy of weekly safety meeting sign in sheet to Construction Manager each week work is performed on site.

15.	This project will be constructed on an active campus during school hours. Work will be performed around students and teachers. Anywork that needs to be performed in/above classroomswillneed to be completed before or after school. All employees working on site shall be wearing badges and pass CUSD background check. Any communication with teachers/students will not be acceptable and employees will be removed from the jobsite immediately.

SUMMARY 01 10 00 - 3

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

CDL-01 – DOOR HARDWARE

Furnishandinstallallworkspecificallyrequiredthroughout theprojectdocumentstocompletetheworkof this bid package that specifically includes, but is not limited to the following:

SPECIFICATION SECTIONS

DIVISION 00 DIVISION 01
08 11 13 08 71 00 09 91 23

HOLLOW METAL DOORS AND FRAMES DOOR HARDWARE
PAINTING (ADM 3)

Referto additionalrelated specificationssectionsforworkspecificallyincluded in thisbidpackagenotedbelow.

GENERAL ITEMS

1.	Furnish and install all layout for own work.

2.	Provide all power for own work.

3.	See General Notes at beginning of summary of work specification section for other items.

COORDINATION WITH OTHER TRADES –

1.	Coordinate physical connection to door hardware with low voltage contractor.

2.	Coordinate student access to allow proper student flow.

FURNISH AND INSTALL ITEMS

1.	Furnishandinstallalldoorhardware.RefertoFOBitemsbelowforitemstobeinstalledbyelectricalpackage. RemoveanyexistingdoorhardwarerequiredforinstallationofnewhardwareandturnovertoDistrict.

2.	Drill all necessary holes in doors and frames as required to allow for installation of own work.

3.	Furnish and install new doors/frames where shown. (ADM 3)

4.	Furnish and install any cover plates as shown on drawings to cover any existing holes in doors/frames.

5.	Furnish andinstallany necessary patchworkto adjacentfinishesasa resultofinstallationof new door frames. (ADM 3).

6.	Furnish and install paint at new doors/frames. (ADM 3)

FOB ITEMS

1.	Furnish FOB jobsite door hardware power supplies/battery backups to be installed by the Electrical/Low Voltage Contractor.

INSTALLATION OF FOB ITEMS

1.	None

END OF BID PACKAGE

SUMMARY 01 10 00 - 4

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

CDL-02 – ELECTRICAL & LOW VOLTAGE

Furnish andinstallallworkspecificallyrequiredthroughout theprojectdocumentstocompletetheworkof this bid package that specifically includes, but is not limited to the following:

SPECIFICATION SECTIONS

DIVISION 00 DIVISION 01
06 10 00 08 41 13 08 80 00 09 91 23 26 00 00 26 05 00 27 10 00 27 51 13 28 31 00

ROUGH CARPENTRY
ALUMINUM FRAMED ENTRANCES AND STOREFRONTS GLASS AND GLAZING
PAINTING
GENERAL ELECTRICAL
COMMON WORK RESULTS FOR ELECTRICAL STRUCTURED CABLING SYSTEM
PAGING SYSTEMS
ACCESS CONTROL SYSTEM

Refertoadditionalrelatedspecificationssectionsforworkspecificallyincludedinthisbidpackagenotedbelow

GENERAL ITEMS

1.	Furnish and install all layout for own work

2.	Provide all power for own work.

3.	See General Notes at beginning of summary of work specification section for other items

COORDINATION WITH OTHER TRADES

1.	Coordinate physical connection to door hardware with low voltage contractor.

2.	Coordinate student access to allow proper student flow.

3.	Provide useofelectricalequipmentanddevicesasrequiredbytheConstructionManagerfortesting ofequipment priorto finalacceptance,which willnotinitiatethe warrantyperioduntilfiling of noticeof completion.

FURNISH AND INSTALL ITEMS

1.	Furnish and install all required cabling for door lock and PA systems.

2.	Furnish and install all surface mounted raceways for any cabling that can not be run inside walls/ceilings/frames. Wiring shall be routed through storefront/HM frames where possible. Grout filled framesshallreceivesurfacemountwiremold. Emergencypushbuttonatfrontofficedeskshallbeinstalled inwall adjacenttoreceptiondesk asshownon drawings. Wiringto beconcealedinsidewall ifpossible.

3.	Furnish and install surface mount EMT conduit in gymnasiums. Paint conduit to match adjacent surroundings.

4.	Furnish and install ceiling wires and cable supports for cabling running above accessible ceiling. Brace every 4’.

5.	Remove and reinstall any glass in storefront/HM systems as required for access to own work.

SUMMARY 01 10 00 - 5

PBK Architects
Project No. S2100500AR

CUSD District Wide Lockdown Clovis Unified School District

6.	Remove and reinstall acoustical ceiling tiles asrequired for accessto own work. Anydamaged tiles shall be replaced at contractor’s expense.

7.	Furnish andinstallfire stoppingfor own workasrequiredat anypenetrationsthroughfirewalls. Refer to plans for firewall locations.

8.	Furnishandinstallallaccess doorsnecessaryto provide accesstoworkincludedin thisbidpackage. Anticipated access doors are shown on drawings. Provide required ceiling/soffit framing for installation of access doors.

9.	Furnish and install watertight closures at all penetrations through exterior walls.

10.	Furnish and install all new speakers and cabling for PA system upgrade as shown on drawings. Make physical connection to existing system.

11.	Drill all necessary holes/sleeves in walls, doors, and frames as required to allow for installation of own work.

12.	Furnish andinstallallsecurity/accesscontrolpanelsand powersuppliesfor allbuildingsasrequired.

13.	Make final connection/termination where cabling connects to door hardware.

14.	Furnish and install power for door notifier/power supplies/battery backups. See detail 12/D1.1 for additional information. Provide power from existing electrical panel to equipment location as called out on plans.

15.	Furnish and install emergency push button located at front desk as indicated on drawings.

16.	Furnish and install lockable enclosure panel for all power supplies and battery backups to allow for cleaninstallationandto eliminatepotentialvandalismto equipmentexposedtopublicview. Referto drawings for exact locations and sizes.

17.	Furnish and install network cabling to access control equipment.

18.	Furnish and install card readers, security wiring, and headend equipment.

19.	Furnish and install interface relays, door position contacts, and request to exit devices.

FOB Items

1.	None

INSTALLATION OF FOB ITEMS

1.	Install power supplies/battery backups furnished FOB by Door Hardware Contractor.

2.	Any equipment/materialprovided FOB from the door hardware bid package and installed by this bid package, the installing contractor shall meet all certifications/licensing requirements necessary to install and warranty the product.

END OF BID PACKAGE

SEE ATTACHED SCHEDULE

END OF SECTION 01 10 00

SUMMARY 01 10 00 - 6

ID
	
1

	Task
Mode 
	Task Name
	
BUD RANK ELEM
	Duration
	
	Start
	
Thu 11/9/23
	Finish

	Nov	Dec	
	Qtr 1, 2024
	Jan	Feb	
	
				27 days
		Fri 12/15/23
				
2
			INSTALL NEW DOOR HARDWARE
	6 days
	Thu 11/9/23
	Thu 11/16/23
				
3
			PULL CABLING/RUN WIREMOLD
	9 days
	Tue 11/14/23
	Fri 11/24/23
				
4
			INSTALL CARD READERS/SPEAKERS
	5 days
	Mon 11/27/2
	Fri 12/1/23
				
5
			TERMINATE DEVICES
	3 days
	Mon 12/4/23
	Wed 12/6/23
				
6
			TEST SYSTEM
	2 days
	Thu 12/7/23
	Fri 12/8/23
				
7
			PUNCHLIST CORRECTIONS
	5 days
	Mon 12/11/2
	Fri 12/15/23
				
8
			FORT WASHINGTON
	23 days
	Fri 11/17/23
	Tue 12/19/23
				
9
			INSTALL NEW DOOR HARDWARE
	4 days
	Fri 11/17/23
	Wed 11/22/2
				
10
			PULL CABLING/RUN WIREMOLD
	6 days
	Wed 11/22/2
	Wed 11/29/2
				
11
			INSTALL CARD READERS/SPEAKERS
	4 days
	Thu 11/30/23
	Tue 12/5/23
				
12
			TERMINATE DEVICES
	3 days
	Wed 12/6/23
	Fri 12/8/23
				
13
			TEST SYSTEM
	2 days
	Mon 12/11/2
	Tue 12/12/23
				
14
			PUNCHLIST CORRECTIONS
	5 days
	Wed 12/13/2
	Tue 12/19/23
				
15
			CLOVIS HIGH
	59 days
	Thu 11/23/2
	3Tue 2/13/24

										
16
			INSTALL NEW DOOR HARDWARE
	18 days
	Thu 11/23/23
	Mon 12/18/2
				
17
			PULL CABLING/RUN WIREMOLD & CONDUIT
	26 days
	Thu 11/30/23
	Thu 1/4/24

										
18
			INSTALL CARD READERS/SPEAKERS
	12 days
	Fri 1/5/24
	Mon 1/22/24
				
19
			TERMINATE DEVICES
	8 days
	Tue 1/23/24
	Thu 2/1/24
				
20
			TEST SYSTEM
	3 days
	Fri 2/2/24
	Tue 2/6/24
				
21
			PUNCHLIST CORRECTIONS
	5 days
	Wed 2/7/24
	Tue 2/13/24

										

Project: CUSD Lockdown Contr Date: Wed 5/10/23
	Task	Project Summary	Manual Task	Start-only	Deadline
Split	Inactive Task	Duration-only	Finish-only	Progress
Milestone	Inactive Milestone	Manual Summary Rollup	External Tasks	Manual Progress
Summary	Inactive Summary	Manual Summary	External Milestone
	
Page 1